(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "RS485_BSV")
		(rev "2")
		(company "ООО \"Экросхим\"")
		(comment 1 "Антон Мухин")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(aux_axis_origin 30 63)
		(grid_origin 30 63)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin yes)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue no)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerbers/")
		)
	)
	(net 0 "")
	(net 1 "Net-(D4-PD0)")
	(net 2 "Net-(D4-PD1)")
	(net 3 "+3V3")
	(net 4 "GND")
	(net 5 "+12V")
	(net 6 "+5V")
	(net 7 "UA_RDY")
	(net 8 "XRAY_ON")
	(net 9 "NO_LINK")
	(net 10 "OVERLOAD")
	(net 11 "OVERHEAT")
	(net 12 "+12VA")
	(net 13 "+3.3VA")
	(net 14 "Net-(D5A-+)")
	(net 15 "Net-(D5B-+)")
	(net 16 "Net-(D6A-+)")
	(net 17 "Net-(D6B-+)")
	(net 18 "HV_24V")
	(net 19 "HV_15V")
	(net 20 "Net-(D2-B)")
	(net 21 "U1_RX")
	(net 22 "TXEN")
	(net 23 "Net-(D2-A)")
	(net 24 "U1_TX")
	(net 25 "SWO")
	(net 26 "unconnected-(D4-PC15-Pad4)")
	(net 27 "unconnected-(D4-PB4-Pad56)")
	(net 28 "unconnected-(D4-PB2-Pad28)")
	(net 29 "Ia_CTRL")
	(net 30 "SWCLK")
	(net 31 "unconnected-(D4-PC6-Pad37)")
	(net 32 "unconnected-(D4-PB9-Pad62)")
	(net 33 "unconnected-(D4-PC3-Pad11)")
	(net 34 "unconnected-(D4-PB10-Pad29)")
	(net 35 "unconnected-(D4-PC14-Pad3)")
	(net 36 "Net-(D4-PC10)")
	(net 37 "unconnected-(D4-PC0-Pad8)")
	(net 38 "RESET")
	(net 39 "unconnected-(D4-PB8-Pad61)")
	(net 40 "SWDIO")
	(net 41 "Net-(D4-PB14)")
	(net 42 "unconnected-(D4-PD2-Pad54)")
	(net 43 "Ua_MON")
	(net 44 "unconnected-(D4-PA1-Pad15)")
	(net 45 "unconnected-(D4-PA12-Pad45)")
	(net 46 "Net-(D4-PC11)")
	(net 47 "HV_ENABLE")
	(net 48 "unconnected-(D4-PB1-Pad27)")
	(net 49 "unconnected-(D4-PB0-Pad26)")
	(net 50 "unconnected-(D4-PC12-Pad53)")
	(net 51 "Ua_CTRL")
	(net 52 "unconnected-(D4-PC2-Pad10)")
	(net 53 "Net-(D4-PB12)")
	(net 54 "CONN")
	(net 55 "Ia_MON")
	(net 56 "Net-(D4-PA3)")
	(net 57 "unconnected-(D4-PC13-Pad2)")
	(net 58 "unconnected-(D4-PB11-Pad30)")
	(net 59 "LED_ACT")
	(net 60 "Net-(D4-PB15)")
	(net 61 "unconnected-(D4-PA15-Pad50)")
	(net 62 "Net-(D4-PA2)")
	(net 63 "Net-(D4-PB13)")
	(net 64 "unconnected-(D4-PA0-Pad14)")
	(net 65 "Net-(D5A--)")
	(net 66 "Net-(D5B--)")
	(net 67 "Net-(D6B--)")
	(net 68 "Net-(D6A--)")
	(net 69 "unconnected-(D7-NC-Pad1)")
	(net 70 "X_HV_ENABLE")
	(net 71 "Net-(X2-Pin_1)")
	(net 72 "Net-(HL1-K)")
	(net 73 "Net-(HL2-K)")
	(net 74 "X_HV_24V")
	(net 75 "Net-(HL3-K)")
	(net 76 "Net-(HL4-K)")
	(net 77 "/X_UA_RDY")
	(net 78 "/X_XRAY_ON")
	(net 79 "/X_NO_LINK")
	(net 80 "/X_OVERLOAD")
	(net 81 "/X_OVERHEAT")
	(net 82 "X_Ua_MON")
	(net 83 "X_Ia_MON")
	(net 84 "X_Ua_CTRL")
	(net 85 "X_Ia_CTRL")
	(net 86 "X_HV_15V")
	(net 87 "Net-(VD10-K)")
	(net 88 "Net-(VD9-K)")
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(uuid "00f5daba-7b38-4bc1-b23c-d270b495d104")
		(at 57.9 50.862499 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 1.5 -0.6 90)
			(layer "F.SilkS")
			(uuid "4383f2fa-a29c-452a-bf36-e66156dcbc9c")
			(effects
				(font
					(size 0.9 0.7)
					(thickness 0.15)
				)
				(justify right)
			)
		)
		(property "Value" "100p"
			(at 0 1.679999 90)
			(layer "F.Fab")
			(uuid "c6e60aa7-79f8-4143-84e0-b83028ef526c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "18bfed9b-a8d4-4fd9-b625-c87511c61154")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f4a96919-c871-4b49-9ec9-5fcaa0ac11ad")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bde9a7f9-33f9-4db9-903d-10d826d8ccfe")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "07781090-f00e-4b67-8f01-fdf2e81050cd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/83c0046a-37de-470b-99d1-727d652be716")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d5850440-68a4-459e-a490-924d38d9d2f5")
		)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c809edd9-7445-4648-aa38-d51c0ec15fcb")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "98733dee-4c44-412d-aa7b-c990b102ae1a")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "82dfb61e-b385-48b9-a043-e1f192f7e1cd")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "98ad9fd1-20ce-4b45-bc29-f93a4d5a403d")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ab020248-e8b2-4e41-8003-cff2ea5f6b56")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a82e863b-1a6e-4b8f-987e-21b93d00bd5b")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "590cb5c4-966e-4ddc-b6b6-831881464a03")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fc25dac6-15b0-461b-b7a8-33ca99df18af")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0a10fd9a-e8fb-45e4-abbf-a21dfd92119e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "7d4ff762-e511-4afd-9b1f-85b8370e7cd3")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "OVERHEAT")
			(pintype "passive")
			(uuid "240eb033-cb2f-4c65-ba19-f0e50f4e802a")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "35917133-bd0c-4c54-8bb2-7f506a21944b")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(uuid "017768cc-b409-40de-b363-d39e9f8bdb87")
		(at 89.5 40.5 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C27"
			(at 0 -1.679999 90)
			(layer "F.SilkS")
			(uuid "d14cc85a-fb6b-4c57-8263-a84fa5a03265")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100p"
			(at 0 1.679999 90)
			(layer "F.Fab")
			(uuid "0c48157e-7885-436d-9f3e-20a88a09350a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b6ea193c-98ed-4847-8c51-3ca8ed1f9b87")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4376d635-9762-4ae5-ba48-2d54838cdf60")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fe55923a-36f0-4155-bb1b-812e2543da8a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5aa6eec0-caae-4f1f-a728-4d5749e7cfd1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/bb520daa-2298-4434-9b9b-abbdb144a412")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6fed2cdc-3ab3-49e2-8627-4ab8aaf2e2aa")
		)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4e171369-5841-4945-b477-2dc6d649bdda")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0c9faf25-9fdd-4ca3-80ed-e4f379e843d3")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2d94fb72-a424-4360-ba4e-20a137d13fdf")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "040fa545-c3ca-4001-a3ab-c23a104ac1dc")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f55f4ccb-909c-4ef8-8e40-ccbd9b2bb17c")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7acb857c-1920-47d1-803c-57f98ef54cdf")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a3817729-4490-4db2-9d9c-dac8a852dc63")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c0c21300-b74a-4c01-8a81-63e28e2280db")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3e89d74a-87f9-4faa-bbe2-afdb158a2722")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "5fdd79b1-1f3a-4bdc-8c6a-3cd7e9db6644")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "HV_24V")
			(pintype "passive")
			(uuid "a95340a2-4b3f-4313-93eb-c0d226b5d975")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "475f4e59-930b-4b85-a3d4-0ca3defb03aa")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "024f544d-204c-4917-93ae-940b37f2940f")
		(at 46.6 44.5 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R22"
			(at 0 0 90)
			(layer "F.SilkS")
			(uuid "e0eaec3c-8763-456c-b267-2461565e8e92")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "97b4ded2-4204-488a-bbcc-8ac9f43b02a3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8b067d45-fb55-4461-bce1-040028e385dc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e12014c6-d2f5-4395-9895-fe7b1e4d747d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "19078385-7c18-4404-9fd7-47f307bfaed7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/6f15ce7b-bcf1-4b6e-ab4b-bfb90d1d61c5")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fd1f20cd-01ce-422b-a523-7002bf99b8ef")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0d52d722-84f3-41e7-8bf0-f60a380fa197")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5c2459e1-f702-47d0-94b8-9ca2a7316d42")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2d1f0ec9-902e-4ed2-8b24-a2f9dd22c385")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "40653554-05e5-49d1-a76e-01ecca3b5e39")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "91f30c7e-a01c-4dc5-9603-5bb43e95f7e5")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "877556fa-9f85-47b9-aae4-62983b389413")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "33a23747-4d71-415b-990b-1d2e958d102f")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "755fdf5f-1d95-4b3e-ba72-0179514efbdd")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d6aae446-d453-4e67-83c7-e4b047ef4ca4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "9c362d18-8eaa-43d5-b009-a1e0e68ad854")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 88 "Net-(VD9-K)")
			(pintype "passive")
			(uuid "545f45b8-f308-4a32-996a-7b6b8d75a560")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 68 "Net-(D6A--)")
			(pintype "passive")
			(uuid "2dbd1103-bc42-46d6-9358-dc270626c789")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "02791824-f012-428c-85f5-ef7ff5f0c69e")
		(at 36.1 38.6)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R33"
			(at 0 1.700001 0)
			(layer "F.SilkS")
			(uuid "e7f9014d-31d3-4fbb-b658-5969610b95fd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "68345e49-5c27-4e06-a353-71a7d541ff30")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "42caf7e4-9de0-4fd7-a4f1-80ca2b5846f2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c936fca0-01d6-44e3-984a-4d3a0ca077d6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "759198f9-ebbe-49d4-a42c-d0e988441de5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/54df956a-163d-4a54-9372-72fb8265bbaa")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f22fcb48-f99c-4a82-9d88-ee3c4b7052c2")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0bacdcdc-b116-4c31-92dc-204f1b47bc5b")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "682f8f66-1850-46b9-ba25-11bbd91c03c0")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "646adab6-9ac2-40c7-93c3-fb25a3c372d8")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "854d8002-15c6-4a23-ad07-2c7ef5835660")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "530bbe1a-31b7-4e96-94d5-0b5b89372478")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e39bde95-3d6b-405a-8490-4757db57d8eb")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "36bcd269-2d71-4617-af44-a0a194d519ae")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "41442e4c-0e40-4e22-9644-ca8f3933b787")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4bbc73c1-297c-45d6-b81b-c6778031664d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d521d90a-5b77-4605-a7a4-68263bedd723")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 51 "Ua_CTRL")
			(pintype "passive")
			(uuid "159b8cee-4efd-467d-b486-c8d93f4fe921")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 4 "GND")
			(pintype "passive")
			(uuid "ae7fd5e3-a154-4b41-abe8-524cd50c77b2")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm"
		(layer "F.Cu")
		(uuid "05d938e0-be4e-42e4-aae1-98836cbbfe79")
		(at 50.2 41.550001 180)
		(descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
		(tags "test point THT pad")
		(property "Reference" "TP12"
			(at 0 -1.448001 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "205face0-3542-4394-88a7-92afa47a1e2c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 1.550001 0)
			(layer "F.Fab")
			(uuid "4b7b0001-fa30-49ff-88bc-1ad0586bd140")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "68a8308d-da23-4c86-90d8-84f727a450b1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fa163767-cc93-4174-ac5e-1ba605016304")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "44cc7c62-d215-4a3b-a247-321efd1a46c6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/eac184a4-8e5d-4c6b-be80-a57985287497")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 0 0.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "dcd1e750-d031-4a7a-b7d9-143d44656163")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "31c9fbad-a12a-4cc3-aba7-8d316786b295")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
			(uuid "3cdce5bd-554a-4f47-b8c6-e515a96b6825")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1 1)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Ia_CTRL")
			(pinfunction "1")
			(pintype "passive")
			(uuid "16f96f9b-6e33-42f5-b7e0-6836969d2749")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Horizontal"
		(layer "F.Cu")
		(uuid "0626d90f-0897-4266-adea-1cfba5f06f11")
		(at 126.35 55.975)
		(descr "Through hole angled pin header, 2x03, 2.54mm pitch, 6mm pin length, double rows")
		(tags "Through hole angled pin header THT 2x03 2.54mm double row")
		(property "Reference" "X3"
			(at -2.1 -0.575 90)
			(layer "F.SilkS")
			(uuid "458d1442-8ea2-4ec2-8d17-f16b53a6a4b2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PLD-6R"
			(at 5.655 7.35 0)
			(layer "F.Fab")
			(uuid "6b4826f2-94a9-4be8-a73b-5ebdb20b7b0e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8f80376d-051c-40eb-b523-f104e75ace74")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7a264e6b-98e9-4f23-a3d7-70fd40a6ef58")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "510d0578-c690-4041-88f1-8602382c53d2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Label" "SWD"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7f4a070e-638c-4f56-b827-26759dcd5444")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(path "/b07c61fb-0925-4f82-abbe-95eb1aa3958d")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.27 -1.27)
			(end 0 -1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bfd0e660-0a0c-4153-8ba2-8f65d36fe7d6")
		)
		(fp_line
			(start -1.27 0)
			(end -1.27 -1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cfda63bc-3318-4ea4-a5ed-f1d4006a5bd5")
		)
		(fp_line
			(start 1.042929 2.16)
			(end 1.497071 2.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e6f78ea9-a3c2-4b11-b0ec-d8622c882013")
		)
		(fp_line
			(start 1.042929 2.92)
			(end 1.497071 2.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fb4f8775-4234-4c4c-a18d-3c5d9d4331ce")
		)
		(fp_line
			(start 1.042929 4.7)
			(end 1.497071 4.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a2e3be7e-aa38-4165-a6d0-84bf8c03ca6b")
		)
		(fp_line
			(start 1.042929 5.46)
			(end 1.497071 5.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "24360c9d-ea3b-407c-95f3-f5bf812614b8")
		)
		(fp_line
			(start 1.11 -0.38)
			(end 1.497071 -0.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3ddf14e8-8167-4fbc-a127-8b360c681394")
		)
		(fp_line
			(start 1.11 0.38)
			(end 1.497071 0.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c87e76ac-c749-41d0-aaa1-8bea6f52a24e")
		)
		(fp_line
			(start 3.582929 -0.38)
			(end 3.98 -0.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9388b238-2c67-4e81-9f4e-f574d4a2cdb9")
		)
		(fp_line
			(start 3.582929 0.38)
			(end 3.98 0.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5f1e61c3-3114-4a51-bf96-f758ed19f723")
		)
		(fp_line
			(start 3.582929 2.16)
			(end 3.98 2.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "91efc73e-37d1-4540-9586-a16cba977ea2")
		)
		(fp_line
			(start 3.582929 2.92)
			(end 3.98 2.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "90896e72-33c8-4865-8899-780f79721aa5")
		)
		(fp_line
			(start 3.582929 4.7)
			(end 3.98 4.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4da92c72-6aba-46fd-ad49-01d02b5fdfc0")
		)
		(fp_line
			(start 3.582929 5.46)
			(end 3.98 5.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "008b6adb-d7c6-46f1-9c3e-919291c0762e")
		)
		(fp_line
			(start 3.98 -1.33)
			(end 3.98 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "32833285-74ee-41c7-91eb-803510cdb8be")
		)
		(fp_line
			(start 3.98 1.27)
			(end 6.64 1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5ed939a9-93c1-4a46-a58d-a497ef0528dd")
		)
		(fp_line
			(start 3.98 3.81)
			(end 6.64 3.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3d56ce31-6119-4939-8a70-d15920a2b1b2")
		)
		(fp_line
			(start 3.98 6.41)
			(end 6.64 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6eaa3270-d106-4b2d-a019-6022a9c4b7d7")
		)
		(fp_line
			(start 6.64 -1.33)
			(end 3.98 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "08082238-d6f0-4bf1-99cb-a74c89d007ef")
		)
		(fp_line
			(start 6.64 -0.38)
			(end 12.64 -0.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7a79ef03-20c3-4ff5-b179-9fe6f8ed6ebc")
		)
		(fp_line
			(start 6.64 -0.32)
			(end 12.64 -0.32)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "13426b66-38d0-4afc-8356-1df8e6eee9d7")
		)
		(fp_line
			(start 6.64 -0.2)
			(end 12.64 -0.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9e3b3003-f403-45fe-b56d-152d901fcda5")
		)
		(fp_line
			(start 6.64 -0.08)
			(end 12.64 -0.08)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e8a2da0a-f832-4876-94c7-5ea03e8c8597")
		)
		(fp_line
			(start 6.64 0.04)
			(end 12.64 0.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "89eb8575-e2bf-4ac1-ad13-8bcce546d895")
		)
		(fp_line
			(start 6.64 0.16)
			(end 12.64 0.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ed97ed2a-0d40-40bc-8943-439588d032b2")
		)
		(fp_line
			(start 6.64 0.28)
			(end 12.64 0.28)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "15d44394-7932-47b2-918f-78ea976a19d6")
		)
		(fp_line
			(start 6.64 2.16)
			(end 12.64 2.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "588ee8e8-7b2b-4916-814d-eb6ab145bb94")
		)
		(fp_line
			(start 6.64 4.7)
			(end 12.64 4.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f3ee9132-e720-474d-9f4b-8ad87075feb8")
		)
		(fp_line
			(start 6.64 6.41)
			(end 6.64 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "caf42e0a-4ac4-41dc-a126-d399cfee15ae")
		)
		(fp_line
			(start 12.64 -0.38)
			(end 12.64 0.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bfe4e671-e8fb-4ca4-8d18-252b5f60105c")
		)
		(fp_line
			(start 12.64 0.38)
			(end 6.64 0.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f1e63f81-6eab-4de8-b9ee-089060073e6e")
		)
		(fp_line
			(start 12.64 2.16)
			(end 12.64 2.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "98a21200-ce27-4611-97a6-4243686b99e2")
		)
		(fp_line
			(start 12.64 2.92)
			(end 6.64 2.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b6591748-18b1-4689-94a3-791ac39cfc62")
		)
		(fp_line
			(start 12.64 4.7)
			(end 12.64 5.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "04e2e41e-bc20-450a-8cd0-c44fc124af2f")
		)
		(fp_line
			(start 12.64 5.46)
			(end 6.64 5.46)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "57b111c5-6f9f-450b-8652-ed994fbcdc68")
		)
		(fp_line
			(start -1.8 -1.8)
			(end -1.8 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "510cbaae-55a1-48a6-84e2-12fdc9fe152b")
		)
		(fp_line
			(start -1.8 6.85)
			(end 13.1 6.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9845f756-1925-45bd-ab0c-594f102782e9")
		)
		(fp_line
			(start 13.1 -1.8)
			(end -1.8 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2288dfa5-8bc2-43d7-a9d3-8a08bca4c8f2")
		)
		(fp_line
			(start 13.1 6.85)
			(end 13.1 -1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b9ab925c-0e8a-4be8-b055-4a400be388ef")
		)
		(fp_line
			(start -0.32 -0.32)
			(end -0.32 0.32)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6dacf897-fc41-4a27-87ee-fd2ce9c209ee")
		)
		(fp_line
			(start -0.32 -0.32)
			(end 4.04 -0.32)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "15e1395a-174b-4525-8212-e95ad4b4bf46")
		)
		(fp_line
			(start -0.32 0.32)
			(end 4.04 0.32)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c3240b30-6a86-49ad-a0a1-87321a1e2e59")
		)
		(fp_line
			(start -0.32 2.22)
			(end -0.32 2.86)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "940eb14d-a9d8-468d-96b6-786fed54d2c3")
		)
		(fp_line
			(start -0.32 2.22)
			(end 4.04 2.22)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6860e3aa-5360-4f7d-8ffa-a30e87d0654e")
		)
		(fp_line
			(start -0.32 2.86)
			(end 4.04 2.86)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "13fb8911-6b25-4e7b-becd-1a23a0054d7c")
		)
		(fp_line
			(start -0.32 4.76)
			(end -0.32 5.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "91ae60d2-4501-4603-9dd5-88f06edf1531")
		)
		(fp_line
			(start -0.32 4.76)
			(end 4.04 4.76)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "41d51ceb-79ff-415e-908f-3331f95d32a8")
		)
		(fp_line
			(start -0.32 5.4)
			(end 4.04 5.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b43fbb88-feb4-4049-b1ba-56300d7fde26")
		)
		(fp_line
			(start 4.04 -0.635)
			(end 4.675 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e6ce0aa2-608f-4b7d-a788-c1e521b99f99")
		)
		(fp_line
			(start 4.04 6.35)
			(end 4.04 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a17491f3-f5fe-4e5b-9e63-54c66786bf27")
		)
		(fp_line
			(start 4.675 -1.27)
			(end 6.58 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a88b276d-d83b-4abd-94e2-da2f1bef6c6a")
		)
		(fp_line
			(start 6.58 -1.27)
			(end 6.58 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9808a934-76ec-4533-a2fa-050d3bbe1df0")
		)
		(fp_line
			(start 6.58 -0.32)
			(end 12.58 -0.32)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c9b6a04b-3018-46ad-9960-145103a8ade8")
		)
		(fp_line
			(start 6.58 0.32)
			(end 12.58 0.32)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "65466f7a-8a32-44fe-95db-023b93791681")
		)
		(fp_line
			(start 6.58 2.22)
			(end 12.58 2.22)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "20f3bc79-91b6-4c5a-8c02-3727560c1c78")
		)
		(fp_line
			(start 6.58 2.86)
			(end 12.58 2.86)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a345d469-205d-4266-bf09-18ce50a37246")
		)
		(fp_line
			(start 6.58 4.76)
			(end 12.58 4.76)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e0da4948-2f84-4bcf-a8f9-b0fdc31c4c58")
		)
		(fp_line
			(start 6.58 5.4)
			(end 12.58 5.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "885fe667-47d4-422b-9a87-8e3735d60e4e")
		)
		(fp_line
			(start 6.58 6.35)
			(end 4.04 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8a5a67f5-2da4-44ad-8499-0971655eecf1")
		)
		(fp_line
			(start 12.58 -0.32)
			(end 12.58 0.32)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a873e50b-0880-4f58-a78a-1ae5ff11ccfb")
		)
		(fp_line
			(start 12.58 2.22)
			(end 12.58 2.86)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b0d690f6-046b-4152-b618-fb233ee28a80")
		)
		(fp_line
			(start 12.58 4.76)
			(end 12.58 5.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "96a9f224-1766-43b2-a1f8-e8217712bfe7")
		)
		(fp_text user "${REFERENCE}"
			(at 5.31 2.54 90)
			(layer "F.Fab")
			(uuid "48f6818d-84cf-4822-a922-88cbf9ff8d07")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "SWDIO")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "1d430498-6bc2-4aaf-9dae-974c691609dc")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+3V3")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "e6a5e404-2946-476e-bb4c-d7fc7fd8a053")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "SWCLK")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "23d9fdaf-3458-4491-8750-e8e86d89d370")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "SWO")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "d2c0cb78-7e65-4aac-8269-6af8983601f1")
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "RESET")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "4252482a-ef6a-471b-a8eb-5fd5112f17bd")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
			(uuid "e856880f-35b8-4451-9df1-fe838757ce1f")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "090d888c-082f-401f-b100-d23e31fa9492")
		(at 85.5 40.5 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R30"
			(at -1.57735 -1.65 90)
			(layer "F.SilkS")
			(uuid "816e344f-e806-4d54-95e3-01dcba92389d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "0799e262-6191-4b21-8788-8376598bdb5a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ca312eb4-bd75-418a-8678-136ff4141105")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f089afd0-b308-4e59-917b-107e3deba079")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e87a9091-36c9-4ae8-9ace-580e1ba33bb7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/e250f50b-9397-4305-a8d2-a0dbdab48fdf")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c339eebc-f293-4a6e-87d4-4dab4af0f9fd")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "25d2cc46-c192-4479-82df-e55f4917f7a6")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d0e1f4a5-9bd5-48be-8746-025dc4ef21fa")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "72af0747-97cd-4dd6-b7f2-9c8158563ba4")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6407dd20-8eba-47e6-b0ad-23c6644eb364")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c1ea4c27-a4fa-41c8-b4bc-a6e9ee40dad3")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "efcf9595-bdc5-49a9-879b-b3a3e0357c5f")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37816f40-ae13-40f5-8543-cc1cc26796ad")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bc3e176e-5b77-4a60-acc5-0efb7b48bb21")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "77682df6-af1a-44ad-93f8-3108b4bff431")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "32493019-4680-4494-87a7-ca1beb7cf224")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 74 "X_HV_24V")
			(pintype "passive")
			(uuid "1f6ebb4e-ac32-4ca1-836e-027f1b568f16")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 18 "HV_24V")
			(pintype "passive")
			(uuid "2176ba40-31fa-4e61-9f5b-3d259c628062")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fiducial:Fiducial_1mm_Mask3mm"
		(layer "F.Cu")
		(uuid "13755bf7-0c2a-4da7-a453-8de8e07ea7a4")
		(at 80 60.5)
		(descr "Circular Fiducial, 1mm bare copper, 3mm soldermask opening (recommended)")
		(tags "fiducial")
		(property "Reference" "FID5"
			(at 0 -2.54 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "6f6d7861-30ab-4ee2-8ccf-970a661040e8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Fiducial"
			(at 0 2.286 0)
			(layer "F.Fab")
			(uuid "60062095-af64-4f7a-8072-4480359535f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Fiducial:Fiducial_1mm_Mask3mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1cbc6bc8-29fd-4880-acf8-6184790014b0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "38e5f283-41e0-4ec8-a97d-d43afa0f33f7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Fiducial Marker"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3913b8b9-29a4-4183-9310-c5e8c63ef04e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Fiducial*")
		(path "/cbdd9e77-66aa-4b84-81a8-24592b84b997")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1.75 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "c4856e9b-71ba-47ba-be4d-f06fdd3aaece")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "cd98a152-73dd-48f7-b55f-b5e5a5ce5ac1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5ac27ca2-3095-4421-b77f-cfd584855806")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 1)
			(clearance 1)
			(uuid "a82f7d58-9ddd-453a-9043-ee9047483907")
		)
	)
	(footprint "Ecohim:TestPoint_Pad_D0.8mm_no_circle"
		(layer "F.Cu")
		(uuid "17a4fcd6-1811-44df-b19e-fa054de9278e")
		(at 95.7 47.6 -90)
		(descr "SMD pad as test Point, diameter 0.8mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at 0 -1.448001 90)
			(layer "F.SilkS")
			(hide yes)
			(uuid "453c410f-10d1-4dbd-96a2-7ef2a5159ca2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 1.550001 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "fca5ba5b-4229-4e92-82be-0d25c36311fc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Ecohim:TestPoint_Pad_D0.8mm_no_circle"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "92a7156e-ca7a-4f3a-9726-39fd6375534b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "09de95e4-7d49-4313-919b-3d0e7d6689c7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "ec31bcae-c224-4329-bd70-715d6773fefb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/6228b101-2adf-43ee-b4e3-8102bee64622")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 0.381 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "57967c14-fc36-45e2-ad62-289260065b7f")
		)
		(pad "1" smd circle
			(at 0 0 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask")
			(net 62 "Net-(D4-PA2)")
			(pinfunction "1")
			(pintype "passive")
			(uuid "5172ee4a-e5c8-4a42-8694-632dfc0df8ff")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "1c95d89d-173a-4b48-a112-32141e7b2d70")
		(at 70.9 47.162499 -90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "VD1"
			(at -2.5 0 180)
			(layer "F.SilkS")
			(uuid "d7adffa3-65bd-4b82-b0e2-8cd53fed99bc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BAT54S"
			(at 0 2.4 90)
			(layer "F.Fab")
			(uuid "e200836d-fc64-4e62-8384-be95bfa608bd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b24b8bb6-8d58-4a8e-812a-1e9aea084e76")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds11005.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "600d0975-a63d-421a-9d0a-38be59ea6708")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "dual schottky barrier diode, in series"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "80885ec9-4b48-4ab3-b087-7a0f49f18a69")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Link" "https://www.chipdip.ru/product/bat54s-nxp"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cbf77d7f-f6e2-4cde-9634-30430ac86ea8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/87d22d79-20c8-4fb5-bc49-b3c4ace8252e")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 1.560001)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9184d4b8-ee91-4a04-8c78-f1138fa8eb84")
		)
		(fp_line
			(start 0 1.560001)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8a4954f7-6b64-4fec-8946-99168f24768a")
		)
		(fp_line
			(start 0 -1.560001)
			(end -0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c8e33c20-b39f-4a28-9f8d-a6fbd8e8d8ed")
		)
		(fp_line
			(start 0 -1.560001)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "35038f1b-d171-4fa4-8d90-e5d1d0fa7d2c")
		)
		(fp_poly
			(pts
				(xy -1.1625 -1.51) (xy -1.4025 -1.84) (xy -0.9225 -1.839999) (xy -1.1625 -1.51)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "26d62b44-5f50-4be5-a4ca-30ac6604b70a")
		)
		(fp_line
			(start -1.92 1.700001)
			(end 1.92 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5652983a-6710-43de-86fd-9b843ada6de7")
		)
		(fp_line
			(start 1.92 1.700001)
			(end 1.92 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e02ff3a1-142b-484c-b825-b101770e20ca")
		)
		(fp_line
			(start -1.92 -1.700001)
			(end -1.92 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ccc154f0-6bf4-4f7f-a9e5-b654141a24b6")
		)
		(fp_line
			(start 1.92 -1.700001)
			(end -1.92 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a92fe250-ce7c-4345-9132-2fa07480763b")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "81126f90-723e-4b43-a10f-9e2ea5e56c24")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c9024df5-6b2d-4710-856b-b256b3639c88")
		)
		(fp_line
			(start -0.65 -1.125001)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4ead4bc9-ee16-42b3-ae3a-e36f18628f75")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6b000433-930c-4a58-a0f3-f782237c3922")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9e0537a5-6284-4fa7-9cbf-54f1525e1288")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "581c181f-c5d8-4678-b71c-a0fe8aee8c5e")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "fd15db33-9a36-4ceb-8f9d-422e29fa0a88")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pintype "passive")
			(uuid "85291a3a-83bf-4b3f-8367-bddc923a04a5")
		)
		(pad "3" smd roundrect
			(at 0.937501 0 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "UA_RDY")
			(pintype "passive")
			(uuid "460deb39-59d0-4bed-b512-b36552af6b76")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "1f432f04-61b5-4f37-8ac5-52095f9c8b4c")
		(at 45.6 54.3 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R25"
			(at -0.9 1.7 90)
			(layer "F.SilkS")
			(uuid "df9d425e-4801-4939-a9b9-5c8085106088")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "48e6c06d-8b5c-4d33-9fdd-b400836348e9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "444ea0a2-e872-406a-9c64-beead54c30c2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a735f38c-3478-46ab-98e4-4d6d9be18cac")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "66e0d25d-9256-42d8-8933-f4151f7925c2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/aec1502e-3267-41c9-8896-5a3acac7d6b7")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b0f0ca31-1248-4c45-8085-ef8e4360ad86")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f57d3735-9a8c-4f4d-892b-d16748eaf4a4")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cd07dffc-9da6-4cb6-babe-bf8dc809cb0e")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a6858c3f-8cd0-468d-8399-dc4799cd7aef")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "444a5a08-c196-4a06-81ff-5aed227a1b88")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "438c1d4e-cd7d-401b-a913-f8b2afb8e1a1")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "403a46bc-1234-4c63-b849-50b658dbf048")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "485fe6a5-a76d-42c2-8efd-443ddb879ce7")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5270fd34-5e73-403a-a324-130e503d4725")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8dc60744-8bb5-4622-ae24-819d9ef21996")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "586b17e5-b027-404b-8f33-9008cd0f8c3b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 66 "Net-(D5B--)")
			(pintype "passive")
			(uuid "14e67d92-69c5-4e78-865e-f4e6d794e171")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 55 "Ia_MON")
			(pintype "passive")
			(uuid "625ba1c9-5e48-4e0b-b921-0b9554380c23")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Ecohim:TestPoint_Pad_D0.8mm_no_circle"
		(layer "F.Cu")
		(uuid "1fa43386-c25c-4211-82f6-a6b12f3b62d0")
		(at 82 47.8 -90)
		(descr "SMD pad as test Point, diameter 0.8mm")
		(tags "test point SMD pad")
		(property "Reference" "TP7"
			(at 0 -1.448001 90)
			(layer "F.SilkS")
			(hide yes)
			(uuid "6194ee09-bacf-494b-b817-fcb7eca26403")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 1.550001 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "80c7c0c9-2528-48b2-baa3-4f97bf49a114")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Ecohim:TestPoint_Pad_D0.8mm_no_circle"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "e5f05c14-1cae-4a06-a05d-14523f21b98b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "8b47d503-9120-4021-a472-2ab9f1bee2d7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "4b5342e3-8ba5-482f-bef7-faaea76c3bf3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/b2073d22-3ba1-4988-b021-fe5b1fbdfa94")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 0.381 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "5f381923-054b-45d1-ae9c-8f97f0ed77f8")
		)
		(pad "1" smd circle
			(at 0 0 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask")
			(net 63 "Net-(D4-PB13)")
			(pinfunction "1")
			(pintype "passive")
			(uuid "68e5199b-d616-4812-b87b-9b929ab008e0")
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm"
		(layer "F.Cu")
		(uuid "24caaeeb-1626-495e-9d33-a7345932bfe9")
		(at 38.3 51.2)
		(descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
		(tags "test point THT pad")
		(property "Reference" "TP16"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "11f3d574-8cd8-440a-bd4d-ccd04e2df20d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(uuid "db091f4a-cb0c-4456-b1ee-e1958cb55368")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3be752bc-9e81-40d3-95cc-64f5eaf1d374")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "afb9b33e-6092-4df2-aaf7-e5d23e9ceba2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8f9d3f6f-25dd-4610-b9a4-838f23e8d918")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/36263021-afda-4cbe-acf7-c1879c6252e8")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 0 0.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "f2ca6895-ef81-472e-887c-af35886958de")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "fa843b84-765a-470e-ba20-c609a7714789")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
			(uuid "cff599d9-dd0a-4673-8fd2-6db4e1610d4c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1 1)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Ua_MON")
			(pinfunction "1")
			(pintype "passive")
			(uuid "f45c4205-4454-4e8d-adf6-eed3de83a86a")
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "26e029f1-3479-45e8-bb3f-c4d170945084")
		(at 48.599999 44.5 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R26"
			(at 0 0 90)
			(layer "F.SilkS")
			(uuid "da1cec23-4438-4b76-add5-9b76209bd2c3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "150"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "71575630-4043-4256-841a-98ce15670e9c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a4974bfa-6cff-4670-91ec-711823c51f41")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "db7e42dd-437f-4681-9a40-4cdf88d2d0ec")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a2accb88-8018-4e99-8b46-5ffdd56e4d8a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/795a0451-c40e-4e6f-be1a-66696050f3b2")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "29b4a6e1-f770-4bed-b3a1-07a72027a845")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "88bd31d1-57b5-454b-b441-4b3016775c98")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5925f729-7227-4595-bb5f-24c107827208")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "21c6e9f7-0601-439f-b007-dd71645c1702")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "46f21f04-f776-4e57-92e0-835e8b53149c")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f3eb1808-f3f3-49f0-bd23-514f14a68645")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1a8f3255-7bed-4c3f-a5e0-6500316ed7b9")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c974d4f1-aee3-4773-9a83-c83521a4c5eb")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4140b98c-0bc6-405a-a1da-593857ac612b")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "127c7007-6417-4bbe-8e02-3c6d974fb12d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "368e1523-d461-4345-a3d2-72fcacf264b8")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 88 "Net-(VD9-K)")
			(pintype "passive")
			(uuid "5dea981b-0660-4b78-acd2-fb1e51e763bf")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 85 "X_Ia_CTRL")
			(pintype "passive")
			(uuid "8e5ab2d1-1180-4032-bf99-eb055a4fdce7")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "2b5e971b-74e0-4a18-85cc-f40220a7792d")
		(at 66.9 47.162499 -90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "VD2"
			(at -2.5 -0.3 180)
			(layer "F.SilkS")
			(uuid "ba6fd365-7f57-41a4-b29d-63099d7c21cd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BAT54S"
			(at 0 2.4 90)
			(layer "F.Fab")
			(uuid "0d1658b5-1e06-4bba-83c6-67eb59e727e3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "377ec0a9-629c-4ffa-adcf-85a9bc8aee8a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds11005.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "54228922-279b-4775-b2a2-b6ba25f27621")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "dual schottky barrier diode, in series"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "571b75f1-74e3-4985-8805-c3c410692c1e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Link" "https://www.chipdip.ru/product/bat54s-nxp"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "422dc6cb-e850-4d09-83db-24b91df31651")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/3d2dff2e-81e6-4473-8cdc-b67aaa7552b4")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 1.560001)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c8c4f505-1025-451a-b7a7-3bb1763c4268")
		)
		(fp_line
			(start 0 1.560001)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "254d5ad1-a775-496f-8faf-276c561c6f78")
		)
		(fp_line
			(start 0 -1.560001)
			(end -0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "37f2504a-c52d-4dc8-a14f-97201b7c6c47")
		)
		(fp_line
			(start 0 -1.560001)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "24f15eaa-539a-4209-9932-66d06c73b931")
		)
		(fp_poly
			(pts
				(xy -1.1625 -1.51) (xy -1.4025 -1.84) (xy -0.9225 -1.839999) (xy -1.1625 -1.51)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "7fc894b2-b1eb-4980-9f0e-cf4897031f0a")
		)
		(fp_line
			(start -1.92 1.700001)
			(end 1.92 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7e3e5912-9265-476e-814e-98d4e347ab8d")
		)
		(fp_line
			(start 1.92 1.700001)
			(end 1.92 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "830cca4f-80d2-4c4d-a5a8-20ee12da0915")
		)
		(fp_line
			(start -1.92 -1.700001)
			(end -1.92 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "21402224-16b1-44b0-9086-80a815d34b63")
		)
		(fp_line
			(start 1.92 -1.700001)
			(end -1.92 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1eae9e5c-b123-4e0d-9698-e9b09a021d29")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ffd3c85a-2761-42f6-a5d5-78da6ec8aa90")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "75b2baeb-735d-45f8-a795-1df27dc2dcaf")
		)
		(fp_line
			(start -0.65 -1.125001)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "afda133d-a753-4acb-9031-80c2789c535c")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3ee4a382-8bab-4009-90f4-4edab1ea19f1")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c8f20871-a611-49b4-9500-430ce790951c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "e94d2c8e-b17e-46fc-a6ac-34b8d8783b88")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "be890f0d-f885-42e6-bb21-0947b87b2cdd")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pintype "passive")
			(uuid "256846a9-3afe-45d3-bb7b-b7dd570e83f9")
		)
		(pad "3" smd roundrect
			(at 0.937501 0 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "XRAY_ON")
			(pintype "passive")
			(uuid "96152a06-ae43-4d07-9390-f8199f6bea96")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_QFP:LQFP-64_10x10mm_P0.5mm"
		(layer "F.Cu")
		(uuid "2f0a6015-8983-4a1d-b585-a1a1469462f3")
		(at 89.7 52.5 180)
		(descr "LQFP, 64 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ad7606_7606-6_7606-4.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "LQFP QFP")
		(property "Reference" "D4"
			(at 0 0 90)
			(layer "F.SilkS")
			(uuid "32f1e997-bdab-4ef1-83f6-7658afef187c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "STM32F103RCT6"
			(at 0 7.4 0)
			(layer "F.Fab")
			(uuid "ed18c8dd-29d7-4a83-bd5b-b51e777c04ba")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a5631ec9-8a17-4a0c-8a1e-315341b6e805")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103rc.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "92788582-5b69-474e-9924-a330adc3612b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 48KB RAM, 72 MHz, 2.0-3.6V, 51 GPIO, LQFP64"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c41e4743-9867-4206-bf34-fda05bc22438")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LQFP*10x10mm*P0.5mm*")
		(path "/52af5f9a-4bb4-4276-b5d9-69cbb19785e5")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 5.11 5.11)
			(end 5.11 4.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5131d62d-01c3-467a-b8d6-7f1706d80550")
		)
		(fp_line
			(start 5.11 -5.11)
			(end 5.11 -4.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "df9b7b0c-e2ec-45ad-ac0e-953f47c3ac7f")
		)
		(fp_line
			(start 4.16 5.11)
			(end 5.11 5.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0f8d9ba0-e605-4eea-b9e9-6426e50360b1")
		)
		(fp_line
			(start 4.16 -5.11)
			(end 5.11 -5.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c4938404-8f13-4cdd-b5cc-6bcd304d26bc")
		)
		(fp_line
			(start -4.16 5.11)
			(end -5.11 5.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3809d31a-c1ed-4d66-8776-0c1678da92ed")
		)
		(fp_line
			(start -4.16 -5.11)
			(end -5.11 -5.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9a46cfed-4d6f-42b2-9ea6-60b071d6eb37")
		)
		(fp_line
			(start -5.11 5.11)
			(end -5.11 4.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1f3c7e27-9267-49bd-8f88-8528adcc6b17")
		)
		(fp_line
			(start -5.11 -5.11)
			(end -5.11 -4.16)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c1cfc5a4-30eb-4a81-a21d-96233b2bb94d")
		)
		(fp_poly
			(pts
				(xy -5.725 -4.16) (xy -6.065 -4.63) (xy -5.385 -4.629999) (xy -5.725 -4.16)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "74334c4b-94f0-476d-a1be-ceaca4b6bce0")
		)
		(fp_line
			(start 6.7 4.150001)
			(end 6.699999 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d23869e6-d127-4620-a986-dc2fe1d2f9a2")
		)
		(fp_line
			(start 6.7 -4.150001)
			(end 6.699999 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "963f2755-0da9-4fb2-9a89-ffbe04502da0")
		)
		(fp_line
			(start 5.25 5.25)
			(end 5.25 4.150001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2b5b06bf-bffd-41b2-8873-1c59093dbd91")
		)
		(fp_line
			(start 5.25 4.150001)
			(end 6.7 4.150001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "09518003-8727-49ad-82f4-63a415a127b9")
		)
		(fp_line
			(start 5.25 -4.150001)
			(end 6.7 -4.150001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3adabec8-4b34-4ae0-82ae-bae9a5388926")
		)
		(fp_line
			(start 5.25 -5.25)
			(end 5.25 -4.150001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ad277095-cb13-4328-a703-854305d0f6ee")
		)
		(fp_line
			(start 4.150001 6.7)
			(end 4.150001 5.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9d7eb83b-45ff-43e7-af3a-79c26c740669")
		)
		(fp_line
			(start 4.150001 5.25)
			(end 5.25 5.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ab253504-61af-4210-9c81-5de21c438813")
		)
		(fp_line
			(start 4.150001 -5.25)
			(end 5.25 -5.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6a01511c-3c6e-4274-8cfd-210aed4633da")
		)
		(fp_line
			(start 4.150001 -6.7)
			(end 4.150001 -5.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0fb8c041-6722-41ed-aa23-05cd1218362b")
		)
		(fp_line
			(start 0 6.699999)
			(end 4.150001 6.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3a951b32-6514-49f8-86c5-e31642a0942d")
		)
		(fp_line
			(start 0 6.699999)
			(end -4.150001 6.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1bf7aa9a-4e0b-4e41-9be0-af8b72eb6dd1")
		)
		(fp_line
			(start 0 -6.699999)
			(end 4.150001 -6.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1fcbaa58-1e33-42fe-aaa0-13abc2b66ec4")
		)
		(fp_line
			(start 0 -6.699999)
			(end -4.150001 -6.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0f395a75-eca0-4bb0-aee0-a302dc374d4d")
		)
		(fp_line
			(start -4.150001 6.7)
			(end -4.150001 5.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "acb3caf9-6aca-4574-9529-2bce8bac5c08")
		)
		(fp_line
			(start -4.150001 5.25)
			(end -5.25 5.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9817a5e2-9958-469e-b79f-6dd672e64020")
		)
		(fp_line
			(start -4.150001 -5.25)
			(end -5.25 -5.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4ba7fd7c-a257-49b7-90d9-99067333d003")
		)
		(fp_line
			(start -4.150001 -6.7)
			(end -4.150001 -5.25)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "51272d7a-6e61-41dd-a698-40e2976107b8")
		)
		(fp_line
			(start -5.25 5.25)
			(end -5.25 4.150001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b3bb7321-6fee-442c-b4c4-ebf8fc0652bc")
		)
		(fp_line
			(start -5.25 4.150001)
			(end -6.7 4.150001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d6bc2448-873c-47df-b2d9-ef7df01832cd")
		)
		(fp_line
			(start -5.25 -4.150001)
			(end -6.7 -4.150001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aaff1729-60e9-41d3-b7b6-565a58e07f95")
		)
		(fp_line
			(start -5.25 -5.25)
			(end -5.25 -4.150001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "804b94b0-9581-4552-a002-6861523a0af5")
		)
		(fp_line
			(start -6.7 4.150001)
			(end -6.699999 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "db92abe3-ff55-4d40-9091-3ad81fc02d8f")
		)
		(fp_line
			(start -6.7 -4.150001)
			(end -6.699999 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "49f7a7cd-4098-43fd-bbf4-aa99b6b34b6e")
		)
		(fp_line
			(start 5 5)
			(end -5 5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f72125f0-3e2e-45a8-8210-d53798461d8e")
		)
		(fp_line
			(start 5 -5)
			(end 5 5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7495cc09-c38a-413a-8d00-7a0e450c3806")
		)
		(fp_line
			(start -4 -5)
			(end 5 -5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e9e4c3a8-e6bd-4733-af66-abd02448423e")
		)
		(fp_line
			(start -5 5)
			(end -5 -4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f550478a-6789-4363-8bb0-0820b126f6dd")
		)
		(fp_line
			(start -5 -4)
			(end -4 -5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ce917072-fa4b-4a76-9c8b-678bd649490b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "8901b7e5-6404-4d52-b6bb-fb8f8b48d951")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -5.675 -3.749999 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pinfunction "VBAT")
			(pintype "power_in")
			(uuid "e40e3666-bf5f-44bd-9c8c-5232efdcc89a")
		)
		(pad "2" smd roundrect
			(at -5.675 -3.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 57 "unconnected-(D4-PC13-Pad2)")
			(pinfunction "PC13")
			(pintype "bidirectional+no_connect")
			(uuid "23eb94c7-d8e8-4ab3-b2b1-91bf1f87da49")
		)
		(pad "3" smd roundrect
			(at -5.675 -2.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "unconnected-(D4-PC14-Pad3)")
			(pinfunction "PC14")
			(pintype "bidirectional+no_connect")
			(uuid "76002485-65f3-44d1-b0b2-c3dc190c3d81")
		)
		(pad "4" smd roundrect
			(at -5.675 -2.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "unconnected-(D4-PC15-Pad4)")
			(pinfunction "PC15")
			(pintype "bidirectional+no_connect")
			(uuid "d6b90c51-e0c1-4cb9-92e3-e94ecdd6553f")
		)
		(pad "5" smd roundrect
			(at -5.675 -1.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(D4-PD0)")
			(pinfunction "PD0")
			(pintype "bidirectional")
			(uuid "bb8a7692-3472-4bc0-b4ac-eeae4721a47e")
		)
		(pad "6" smd roundrect
			(at -5.675 -1.249999 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(D4-PD1)")
			(pinfunction "PD1")
			(pintype "bidirectional")
			(uuid "8994739a-cadb-411c-9a13-06eaa1c6a769")
		)
		(pad "7" smd roundrect
			(at -5.675 -0.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "RESET")
			(pinfunction "NRST")
			(pintype "input")
			(uuid "e573cbc5-ac1f-452b-9708-03b4447bc116")
		)
		(pad "8" smd roundrect
			(at -5.675 -0.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "unconnected-(D4-PC0-Pad8)")
			(pinfunction "PC0")
			(pintype "bidirectional+no_connect")
			(uuid "0e3f7be9-7eaf-4fb8-bd91-98e699d456d8")
		)
		(pad "9" smd roundrect
			(at -5.675 0.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "LED_ACT")
			(pinfunction "PC1")
			(pintype "bidirectional")
			(uuid "1350d44d-3033-48dc-b0c1-e05bf62246ce")
		)
		(pad "10" smd roundrect
			(at -5.675 0.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 52 "unconnected-(D4-PC2-Pad10)")
			(pinfunction "PC2")
			(pintype "bidirectional+no_connect")
			(uuid "4a2344c0-323c-4682-819f-eec5a26b3f9c")
		)
		(pad "11" smd roundrect
			(at -5.675 1.249999 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "unconnected-(D4-PC3-Pad11)")
			(pinfunction "PC3")
			(pintype "bidirectional+no_connect")
			(uuid "7925940a-6b4f-4c5d-bdb3-4366b0a1809e")
		)
		(pad "12" smd roundrect
			(at -5.675 1.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "VSSA")
			(pintype "power_in")
			(uuid "128b033a-2256-45c8-bcc7-663c9f830c11")
		)
		(pad "13" smd roundrect
			(at -5.675 2.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+3.3VA")
			(pinfunction "VDDA")
			(pintype "power_in")
			(uuid "721d6134-cd96-48c1-82d7-425d654c6b9d")
		)
		(pad "14" smd roundrect
			(at -5.675 2.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "unconnected-(D4-PA0-Pad14)")
			(pinfunction "PA0")
			(pintype "bidirectional+no_connect")
			(uuid "b567c76a-e33a-4ebb-b1a6-93833b699587")
		)
		(pad "15" smd roundrect
			(at -5.675 3.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "unconnected-(D4-PA1-Pad15)")
			(pinfunction "PA1")
			(pintype "bidirectional+no_connect")
			(uuid "2334192b-3beb-4ada-9a0c-8b2b4f4c3fc5")
		)
		(pad "16" smd roundrect
			(at -5.675 3.749999 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 62 "Net-(D4-PA2)")
			(pinfunction "PA2")
			(pintype "bidirectional")
			(uuid "1b711896-f723-435b-9d95-6772ab691b3b")
		)
		(pad "17" smd roundrect
			(at -3.749999 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "Net-(D4-PA3)")
			(pinfunction "PA3")
			(pintype "bidirectional")
			(uuid "fa784d07-e56a-403f-b66c-52496c8e89fb")
		)
		(pad "18" smd roundrect
			(at -3.25 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(uuid "d10f76da-a1f5-44d7-bc44-f232cb6da15c")
		)
		(pad "19" smd roundrect
			(at -2.75 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
			(uuid "b4ae6648-2a1b-49fc-9623-d6e051c712a8")
		)
		(pad "20" smd roundrect
			(at -2.25 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "Ua_CTRL")
			(pinfunction "PA4")
			(pintype "bidirectional")
			(uuid "3478dc31-24c6-4fc1-a156-9077795ba55d")
		)
		(pad "21" smd roundrect
			(at -1.75 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "Ia_CTRL")
			(pinfunction "PA5")
			(pintype "bidirectional")
			(uuid "5d5c8eff-8cdf-4815-b7c3-09a9cfa85610")
		)
		(pad "22" smd roundrect
			(at -1.249999 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "Ua_MON")
			(pinfunction "PA6")
			(pintype "bidirectional")
			(uuid "1384eb4c-5fa2-4ece-8f39-4928046a618f")
		)
		(pad "23" smd roundrect
			(at -0.75 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 55 "Ia_MON")
			(pinfunction "PA7")
			(pintype "bidirectional")
			(uuid "91988cf6-f7a5-40a9-9abd-47625080bef9")
		)
		(pad "24" smd roundrect
			(at -0.25 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "HV_15V")
			(pinfunction "PC4")
			(pintype "bidirectional")
			(uuid "c0d6a8c0-53f2-4bcd-83a3-e677e9fa79b7")
		)
		(pad "25" smd roundrect
			(at 0.25 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "HV_24V")
			(pinfunction "PC5")
			(pintype "bidirectional")
			(uuid "bb3c30e1-37de-415e-8a59-bff854d07a0b")
		)
		(pad "26" smd roundrect
			(at 0.75 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "unconnected-(D4-PB0-Pad26)")
			(pinfunction "PB0")
			(pintype "bidirectional+no_connect")
			(uuid "2cd7ed7a-ef4e-4e4f-b289-41ef10fac7c3")
		)
		(pad "27" smd roundrect
			(at 1.249999 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "unconnected-(D4-PB1-Pad27)")
			(pinfunction "PB1")
			(pintype "bidirectional+no_connect")
			(uuid "a8802a95-6203-44b2-9998-4f04febf4ff9")
		)
		(pad "28" smd roundrect
			(at 1.75 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "unconnected-(D4-PB2-Pad28)")
			(pinfunction "PB2")
			(pintype "bidirectional+no_connect")
			(uuid "1fc1a703-8de3-48a3-a79d-569eeb00fc15")
		)
		(pad "29" smd roundrect
			(at 2.25 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "unconnected-(D4-PB10-Pad29)")
			(pinfunction "PB10")
			(pintype "bidirectional+no_connect")
			(uuid "d8fa323d-308d-4530-920b-bcd72343835f")
		)
		(pad "30" smd roundrect
			(at 2.75 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "unconnected-(D4-PB11-Pad30)")
			(pinfunction "PB11")
			(pintype "bidirectional+no_connect")
			(uuid "bb9eb77b-c1d6-4ae5-a72a-083433ef622f")
		)
		(pad "31" smd roundrect
			(at 3.25 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "VSS")
			(pintype "passive")
			(uuid "551d9e2c-5d8a-4e76-8684-0cb004686d82")
		)
		(pad "32" smd roundrect
			(at 3.749999 5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
			(uuid "bb4d9820-2568-4ce9-866a-f453c2c6d7f5")
		)
		(pad "33" smd roundrect
			(at 5.675 3.749999 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 53 "Net-(D4-PB12)")
			(pinfunction "PB12")
			(pintype "bidirectional")
			(uuid "861e1947-e5b5-4243-b4a8-0110d5d1aa8c")
		)
		(pad "34" smd roundrect
			(at 5.675 3.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 63 "Net-(D4-PB13)")
			(pinfunction "PB13")
			(pintype "bidirectional")
			(uuid "5eb0dd64-9058-42ab-9aec-541616081e36")
		)
		(pad "35" smd roundrect
			(at 5.675 2.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "Net-(D4-PB14)")
			(pinfunction "PB14")
			(pintype "bidirectional")
			(uuid "a3aaf995-b414-40f5-a24c-b37e932c08ba")
		)
		(pad "36" smd roundrect
			(at 5.675 2.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 60 "Net-(D4-PB15)")
			(pinfunction "PB15")
			(pintype "bidirectional")
			(uuid "fc6b36d0-835e-4e7a-8c0e-6d47ef74628d")
		)
		(pad "37" smd roundrect
			(at 5.675 1.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "unconnected-(D4-PC6-Pad37)")
			(pinfunction "PC6")
			(pintype "bidirectional+no_connect")
			(uuid "78fd6393-d3bc-47de-beac-d4bb1e2cb694")
		)
		(pad "38" smd roundrect
			(at 5.675 1.249999 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "HV_ENABLE")
			(pinfunction "PC7")
			(pintype "bidirectional")
			(uuid "3e35a9e5-d91d-419a-b11d-90cd3cbbe957")
		)
		(pad "39" smd roundrect
			(at 5.675 0.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "OVERLOAD")
			(pinfunction "PC8")
			(pintype "bidirectional")
			(uuid "b2eafcf8-ccd6-4f62-951a-8894f99d464a")
		)
		(pad "40" smd roundrect
			(at 5.675 0.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "OVERHEAT")
			(pinfunction "PC9")
			(pintype "bidirectional")
			(uuid "661f55f5-3713-4c5c-b517-8814b0bfbefa")
		)
		(pad "41" smd roundrect
			(at 5.675 -0.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "NO_LINK")
			(pinfunction "PA8")
			(pintype "bidirectional")
			(uuid "808603f1-bb90-4231-a9af-7fde70acad87")
		)
		(pad "42" smd roundrect
			(at 5.675 -0.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "XRAY_ON")
			(pinfunction "PA9")
			(pintype "bidirectional")
			(uuid "7b40aae1-7532-45a2-a074-0b9d8cd949c7")
		)
		(pad "43" smd roundrect
			(at 5.675 -1.249999 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "UA_RDY")
			(pinfunction "PA10")
			(pintype "bidirectional")
			(uuid "1238630b-cd4d-450c-b4fc-89bc58ce25ce")
		)
		(pad "44" smd roundrect
			(at 5.675 -1.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "CONN")
			(pinfunction "PA11")
			(pintype "bidirectional")
			(uuid "2f429b79-d811-4d15-9695-fb3aded87701")
		)
		(pad "45" smd roundrect
			(at 5.675 -2.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "unconnected-(D4-PA12-Pad45)")
			(pinfunction "PA12")
			(pintype "bidirectional+no_connect")
			(uuid "18cebba1-20a9-4825-8f08-fd4d7616282a")
		)
		(pad "46" smd roundrect
			(at 5.675 -2.75 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "SWDIO")
			(pinfunction "PA13")
			(pintype "bidirectional")
			(uuid "9b5d1e6d-7a1f-48a6-880f-ad9292d396b8")
		)
		(pad "47" smd roundrect
			(at 5.675 -3.25 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "VSS")
			(pintype "passive")
			(uuid "bf1bfac9-4c24-4721-9eb5-1bda8c53042b")
		)
		(pad "48" smd roundrect
			(at 5.675 -3.749999 180)
			(size 1.55 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
			(uuid "9935f06e-0e46-4841-ba54-8fad458f7bed")
		)
		(pad "49" smd roundrect
			(at 3.749999 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 30 "SWCLK")
			(pinfunction "PA14")
			(pintype "bidirectional")
			(uuid "211df104-ac5c-47d0-a1d3-558fafef755e")
		)
		(pad "50" smd roundrect
			(at 3.25 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "unconnected-(D4-PA15-Pad50)")
			(pinfunction "PA15")
			(pintype "bidirectional+no_connect")
			(uuid "8b5258b5-9d08-4d6f-a1f9-5a4caee66096")
		)
		(pad "51" smd roundrect
			(at 2.75 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "Net-(D4-PC10)")
			(pinfunction "PC10")
			(pintype "bidirectional")
			(uuid "3fbe94df-f526-4f95-996d-2f1cdcc002de")
		)
		(pad "52" smd roundrect
			(at 2.25 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "Net-(D4-PC11)")
			(pinfunction "PC11")
			(pintype "bidirectional")
			(uuid "da6be103-bfd5-43ad-9e4e-8a1a4bfc906d")
		)
		(pad "53" smd roundrect
			(at 1.75 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "unconnected-(D4-PC12-Pad53)")
			(pinfunction "PC12")
			(pintype "bidirectional+no_connect")
			(uuid "36d73b07-77c2-4540-b83e-ac4854589e37")
		)
		(pad "54" smd roundrect
			(at 1.249999 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "unconnected-(D4-PD2-Pad54)")
			(pinfunction "PD2")
			(pintype "bidirectional+no_connect")
			(uuid "6ad69c15-518f-476a-b663-442f4c4d64fa")
		)
		(pad "55" smd roundrect
			(at 0.75 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "SWO")
			(pinfunction "PB3")
			(pintype "bidirectional")
			(uuid "ec3bc8fb-0250-4800-86a1-f62ad9e0cf39")
		)
		(pad "56" smd roundrect
			(at 0.25 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "unconnected-(D4-PB4-Pad56)")
			(pinfunction "PB4")
			(pintype "bidirectional+no_connect")
			(uuid "5b72eb8f-48b2-4923-be91-5833cf34651f")
		)
		(pad "57" smd roundrect
			(at -0.25 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "TXEN")
			(pinfunction "PB5")
			(pintype "bidirectional")
			(uuid "972d7f5b-eb85-4cab-87c1-0abad2d2d87f")
		)
		(pad "58" smd roundrect
			(at -0.75 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "U1_TX")
			(pinfunction "PB6")
			(pintype "bidirectional")
			(uuid "f5dc2a63-2906-4576-aa76-dd02f2d71f05")
		)
		(pad "59" smd roundrect
			(at -1.249999 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "U1_RX")
			(pinfunction "PB7")
			(pintype "bidirectional")
			(uuid "7884b1e0-b854-43c9-87e9-012f89783b42")
		)
		(pad "60" smd roundrect
			(at -1.75 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "BOOT0")
			(pintype "input")
			(uuid "0bd77e58-867a-48bc-bace-cf2ea2adfefd")
		)
		(pad "61" smd roundrect
			(at -2.25 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "unconnected-(D4-PB8-Pad61)")
			(pinfunction "PB8")
			(pintype "bidirectional+no_connect")
			(uuid "78e794ff-59c2-40f6-8481-36593b47ab43")
		)
		(pad "62" smd roundrect
			(at -2.75 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "unconnected-(D4-PB9-Pad62)")
			(pinfunction "PB9")
			(pintype "bidirectional+no_connect")
			(uuid "2d8ddcd3-ce4c-49e7-af7a-a0cc3ace89d0")
		)
		(pad "63" smd roundrect
			(at -3.25 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "VSS")
			(pintype "passive")
			(uuid "6a93a2fe-9cb6-4d9c-a107-5c6640cd4c8e")
		)
		(pad "64" smd roundrect
			(at -3.749999 -5.675 180)
			(size 0.3 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
			(uuid "0aa5f084-b6c4-46d2-8f32-433ab7db2b32")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-64_10x10mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm"
		(layer "F.Cu")
		(uuid "2f865d5b-04ae-408c-a4ee-bc7c3a5292af")
		(at 43.3 60.6)
		(descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
		(tags "test point THT pad")
		(property "Reference" "TP11"
			(at 1 1.8 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "3dc37a9b-5fe2-401d-b830-4799ad24e324")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(uuid "815bfb79-129d-4401-9227-65fdce7f2b67")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d9366e06-a816-42dc-861c-10a86cb678ee")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "59ef5c76-8316-44d7-9697-da12bddf8af4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d375553e-f39a-49b4-93fc-ffb208366ce3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/04ecfff6-e67e-40e2-ae46-8bd4a567dc6d")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 0 0.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "74e17469-b6d2-4440-befe-7645d2b75d95")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "787c3faa-8bfd-4965-8ce1-bdeac0bdedeb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
			(uuid "cb4acb68-aea5-4cb4-b95f-ab0eb527a46d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1 1)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "X_Ia_MON")
			(pinfunction "1")
			(pintype "passive")
			(uuid "337aa519-df2b-40cc-ac81-c3eb8f89856f")
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "31818754-a1de-4dc9-be6e-36b78dac0c43")
		(at 63.9 50.862499 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at -1.6 0.3 90)
			(layer "F.SilkS")
			(uuid "16538372-719c-4738-8280-a96a022ccdfc")
			(effects
				(font
					(size 0.9 0.9)
					(thickness 0.15)
				)
				(justify right)
			)
		)
		(property "Value" "1k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "d8276911-5a05-4d32-a290-5d00608790b1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3e7031ca-d31a-47a2-8f11-93f9a7148ffa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4e2a413d-df4e-48ef-bc6e-5935136635c9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a5217d81-7dea-4a28-b630-63fe47086db1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/9dec5e88-7f55-47b9-9bae-28af8880661c")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "44868f3b-c7da-4865-a621-bf822fdd8a3a")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d66e3b31-721c-4eb9-bb1a-0460709b75ef")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2ce29552-cb3f-43ca-a3cc-99ebc6cff006")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "71e7c32f-0afc-4df3-afbc-70aaa0b531ce")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4e1bfc5b-2f73-4ae4-8cad-3169d70dcf44")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "79873827-50bf-4ac1-b825-9beac425cd22")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de6dcfa3-8692-4000-a132-ee72af8413d0")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "614e6a5b-c5ff-4b48-98d6-d8c8451639d4")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9b602b74-f48a-465a-a2fe-27750a0dd44e")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d14dd4d9-9e92-4dc2-b2f2-64dce27c9602")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "3455ec18-310b-4060-b4b1-acc1fa2aff68")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 79 "/X_NO_LINK")
			(pintype "passive")
			(uuid "719c673f-d352-4a98-9fdd-1c5c0505dddd")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 9 "NO_LINK")
			(pintype "passive")
			(uuid "808a4d72-8e48-438a-a33b-68a84c5d05aa")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric"
		(layer "F.Cu")
		(uuid "397b7287-00b5-4383-b8a4-c5109442ffe3")
		(at 75 56.1 -90)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "HL2"
			(at 3.1 0.4 90)
			(layer "F.SilkS")
			(uuid "833df4b1-5c46-492b-ba61-c3f841a21b43")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "KP-2012SGD"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "591fe306-2e7b-4f17-9d92-8500c10f88c2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "LED_SMD:LED_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "954b8f6a-59e5-448a-b9a8-2fee4d1dde00")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8caa3223-822a-4e2a-93b4-2e5d29f6eaa1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1c1e8c5d-ea3d-4346-93f1-60b30c30bbf0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Label" "24V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "03eb2d13-9a34-4ba9-8e26-41dde5fb5f1d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Alternative" "Green"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "07e337bc-b3b8-404d-8cc8-9f17dac89ec0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/24eb8cbf-0099-48a7-9b19-d1704c7abe05")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.684999 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "50587971-3f06-4e1f-8783-1f71cbf2ad28")
		)
		(fp_line
			(start -1.684999 -0.96)
			(end -1.684999 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e1ef4921-b298-4817-9ea7-0fca74508183")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.684999 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e99decb6-0423-4dfb-b975-98d10ed8a4f5")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "51abce34-d624-473c-aabf-74dcd2974f0d")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "91774393-2d06-493f-9425-5e97b60d59d5")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4df60ce1-a6f6-43f6-91db-1dfebadfa09b")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3d32a7c0-0b17-4204-bcaf-0a96b44f3ff2")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a3646ee4-dce0-4585-af4d-77bc03e34c4c")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d4e74dd4-cd8d-4f7f-913a-26e08e95ab6b")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1002924a-33d6-4d4e-b8a6-4597909120f1")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "30480ec8-38bd-4554-82de-de553be5d816")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5485b532-5d49-400a-9073-2fb63f15fc35")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "b1ad2a3f-ce6d-4903-9f4b-6d3334a95b9f")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.937501 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 73 "Net-(HL2-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "00ee57b2-9fc2-4166-9c5a-1b153ee0fa38")
		)
		(pad "2" smd roundrect
			(at 0.937501 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "X_HV_24V")
			(pinfunction "A")
			(pintype "passive")
			(uuid "1ddd73fc-3d00-49ac-a316-af3480ec78a5")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "3aaf938e-0dc7-48ff-a3b1-9afa03bc8898")
		(at 71.9 50.862499 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at -1.6 0.1 90)
			(layer "F.SilkS")
			(uuid "d0757e93-add6-4870-8fe8-6b6d49ae8d4a")
			(effects
				(font
					(size 0.9 0.9)
					(thickness 0.15)
				)
				(justify right)
			)
		)
		(property "Value" "1k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "a8a9ba7c-50c1-4f83-a6a8-bc32157caabf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "349b8ea9-556d-42f2-be14-f64866871235")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "984011dd-503a-4d8f-970d-dc2c25de2470")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a2abc9ac-c761-4e7a-a212-d5be6ade69b7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/5535e249-bdaa-463c-9d9e-89aef369755d")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f09577bd-453a-4947-8821-011df17a858d")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "65c302de-9b16-491b-84df-5696bb877524")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f1d34884-b7d4-4fec-8d37-f97b99e0229c")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "720551e0-80e0-4637-a494-fd193f0c7d71")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "26b7bebd-5210-44ce-a061-691c5c24719e")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "13def790-ec58-4be9-88f3-48800ca883ec")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e9977cf8-1023-48be-9552-76e570e109f8")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de4b2a72-5394-457d-979a-16918fa5d03c")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0bcf4b03-8c07-4511-9490-3c389436fc97")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "29138487-955e-4148-9194-627504a51726")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "64896385-d474-4993-b17c-3cd117a4133a")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 77 "/X_UA_RDY")
			(pintype "passive")
			(uuid "d3088268-f1e6-4714-85f3-d3e36da60761")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 7 "UA_RDY")
			(pintype "passive")
			(uuid "35d636ec-2fd0-4f10-9254-f6b8412f4b96")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm"
		(layer "F.Cu")
		(uuid "3feaa31c-aa60-429f-8c61-ee262a570803")
		(at 50.6 43.649999 180)
		(descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
		(tags "test point THT pad")
		(property "Reference" "TP14"
			(at 0 -1.448001 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "2565e862-0a6c-4b57-95f2-ba23a581ac13")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 1.550001 0)
			(layer "F.Fab")
			(uuid "f08d2bd6-d9f9-4709-a6f9-79840d72ddfd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a0a8f851-a87a-49cb-b22e-988dc530797d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a424ef5c-57af-49dc-8f2c-92c20bd4c7b9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e6107766-04e5-4cd2-91c3-453ad48687e7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/eb6fbf8c-9c34-45c5-aa63-c25b31f76097")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 0 0.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "5040990f-a57f-44a9-8040-cdd0ca01e25b")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "477bea88-7448-49db-9f7d-501a7f6fffa8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
			(uuid "25edfb5d-fccb-4fec-8a48-1ab281b070ea")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1 1)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "X_Ia_CTRL")
			(pinfunction "1")
			(pintype "passive")
			(uuid "4fa30587-f724-4f43-96fd-3a96f69a7a80")
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "44084569-a770-4126-8df2-23a3e428f3dc")
		(at 55.9 50.862499 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at -1.5 0 90)
			(layer "F.SilkS")
			(uuid "3f8ade9c-c3ba-4f40-bc57-fbc620314702")
			(effects
				(font
					(size 0.9 0.7)
					(thickness 0.15)
				)
				(justify right)
			)
		)
		(property "Value" "1k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "70b84ffc-710d-4c10-b7b0-221fcd747732")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0a040c07-e244-4534-8168-3e8249e281cb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e0abc657-cc0f-4c27-b516-e15877ed88f0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "75e8a255-0136-46c2-a4ca-f1ed04678bec")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/3bdadb91-a740-4542-b394-ddd2d87186fc")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "94fe2ec9-a5fe-4110-8795-4209c00a34b0")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6de52d82-86f8-43be-950b-379b86630f9f")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5664330d-f9e5-4477-81fc-1018e1ec8f5e")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e5809596-7c4a-4f2a-9270-1772bc60d22a")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "485e8e1b-e3d0-4c59-8485-3a3df6c5f0d4")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dbff6615-9317-470a-8c96-4e2685b6eb41")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8c2a8c71-283c-455c-bb64-892821c2af40")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "da97548e-2b2e-4562-9607-4907cd45e744")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3c570319-bb9b-4601-9bdb-942330330f5f")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8fca9858-40be-46f2-9096-c0215cd0eac4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "ab0f2c04-b33e-4d94-9285-d5621d0e6fcd")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 80 "/X_OVERLOAD")
			(pintype "passive")
			(uuid "3b751ba5-d6c1-4c7d-a37c-479f6e2ed2d0")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 10 "OVERLOAD")
			(pintype "passive")
			(uuid "1d6cc918-c271-494c-9edb-06ec210a47bd")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Ecohim:TestPoint_Pad_D0.8mm_no_circle"
		(layer "F.Cu")
		(uuid "4956364e-a5ad-42ed-8984-e8436ecb4537")
		(at 82 49 -90)
		(descr "SMD pad as test Point, diameter 0.8mm")
		(tags "test point SMD pad")
		(property "Reference" "TP8"
			(at 0 -1.448001 90)
			(layer "F.SilkS")
			(hide yes)
			(uuid "931913b6-6f4c-43b8-8433-a1ca326b3e59")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 1.550001 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "e8fd5a84-2631-4692-9721-7c6abf591baa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Ecohim:TestPoint_Pad_D0.8mm_no_circle"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "5a57b942-5eef-49ac-b110-ed07fa7e64e5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "bf447e1a-5e0d-48b8-a79f-0da3730b0b42")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "41d71af8-93c6-4079-af19-eeee30b4627e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/c793bd18-021c-4ed8-866f-fcd65055cf0a")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 0.381 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "c962221d-33f6-4c7a-b907-0fddb7a2512d")
		)
		(pad "1" smd circle
			(at 0 0 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask")
			(net 41 "Net-(D4-PB14)")
			(pinfunction "1")
			(pintype "passive")
			(uuid "cc9e6895-2eba-46e4-b9c6-bfecda75c697")
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric"
		(layer "F.Cu")
		(uuid "4a67761b-9a26-48c7-96b1-ce122a250a3d")
		(at 75 51.7 -90)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "HL4"
			(at -3.1 0.1 90)
			(layer "F.SilkS")
			(uuid "d9aeb377-6874-444c-84dd-95ac7515d546")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "KP-2012ID"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "cbacf7ab-9755-4a96-bba6-f659b5bd722e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "LED_SMD:LED_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b30b1d69-829b-4d96-9f5e-579a0035a328")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7212e852-8a6b-48ad-8e1b-c1f1594ac3a9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4d0a5932-fe45-4749-9aa8-8642dfe71398")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Label" "ENABLE"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "10dbb30a-7cfa-4605-85aa-951b7f549aad")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Alternative" "Red"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "884351f7-3a26-4126-bb8e-52c152dc355f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/de4eb2c4-9a55-46d2-883e-13331899dde5")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.684999 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ef14c61a-c904-4cee-8484-efba9f37e5cc")
		)
		(fp_line
			(start -1.684999 -0.96)
			(end -1.684999 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e4331859-a5ac-40dc-9ebb-db4b9a8d1663")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.684999 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bce7b9e7-950c-417f-adf1-91b9f6dc862d")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dc306947-e08e-4be1-a0ef-59edc407a3eb")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b3428e45-481a-4a45-b0e0-993be6b1f89f")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6bf41a2a-a388-419b-9184-8c4c64cc1679")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "296d5794-90d9-4976-add6-35d5920fc92b")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e89c2c44-8713-45de-a888-c9f13b125f06")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eb7d51e8-bee4-4bdd-a33e-c9947d1104f4")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5344db8b-f8e2-4645-8e76-8d41ae605fee")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6d8aa572-a0f3-4930-b6fb-14758962c715")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "16849a2b-363d-410e-8982-eb4e6fca221d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "ce20fd43-f40a-4602-a00c-1842dfcf524b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.937501 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 76 "Net-(HL4-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "92f45916-9795-4c67-b92a-cc4474201937")
		)
		(pad "2" smd roundrect
			(at 0.937501 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "X_HV_ENABLE")
			(pinfunction "A")
			(pintype "passive")
			(uuid "c1bbc8d5-18f4-4869-acb2-37c5a7ee7f45")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "4e1d211a-846b-4462-b735-327ef19fc027")
		(at 58.9 47.162499 -90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "VD5"
			(at -2.5 -0.9 180)
			(layer "F.SilkS")
			(uuid "62e8a0d4-4c62-4148-b29a-60a2fe8b1f5b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BAT54S"
			(at 0 2.4 90)
			(layer "F.Fab")
			(uuid "2b441721-4ac3-40ce-b3cf-fcc1f5912b2b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "35418725-67f2-457d-918b-204525ce80b7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds11005.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "83c4d1c5-7018-45a7-b0bc-0587d952229e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "dual schottky barrier diode, in series"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5a92ca40-ca90-41c7-8aa3-b45cd8d9bfed")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Link" "https://www.chipdip.ru/product/bat54s-nxp"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6d2b1985-8427-49e5-a2f4-7b069885c76e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/fc342fd5-2e88-4629-b261-4eb6559f3f86")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 1.560001)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f9b56f68-a77c-40c0-a817-a2ef6535393d")
		)
		(fp_line
			(start 0 1.560001)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6df590d6-4c3d-40a2-81d1-3363d256ce40")
		)
		(fp_line
			(start 0 -1.560001)
			(end -0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bb6cee8c-4c63-4e6f-809d-912d08052553")
		)
		(fp_line
			(start 0 -1.560001)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "38e2dd7f-42b6-47ed-bbca-f72f34004fde")
		)
		(fp_poly
			(pts
				(xy -1.1625 -1.51) (xy -1.4025 -1.84) (xy -0.9225 -1.839999) (xy -1.1625 -1.51)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "9dde0238-a007-4867-95e9-e10b6f1f3396")
		)
		(fp_line
			(start -1.92 1.700001)
			(end 1.92 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "774c3ee8-b282-4db0-ace2-53f4373df935")
		)
		(fp_line
			(start 1.92 1.700001)
			(end 1.92 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "39bad030-0d0e-4206-b911-b93d6206f2e4")
		)
		(fp_line
			(start -1.92 -1.700001)
			(end -1.92 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "050a6bc7-f4b7-48db-a23b-6509363f495a")
		)
		(fp_line
			(start 1.92 -1.700001)
			(end -1.92 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "34e88780-2f72-4b58-bbb6-594ec01551db")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9ddfdf24-e619-4354-b4cc-2aa1e126b2bd")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "256016fd-9bc2-48d9-89a7-5381b5c3211b")
		)
		(fp_line
			(start -0.65 -1.125001)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "18a23094-3de1-4f47-abee-4e4bb4bdb27e")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "040932b5-2084-49f0-bf9e-743664f7dcd7")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fbd2bce9-29c8-42e1-af8a-325dd149a789")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "dd48ff86-7dc0-4f82-9b46-4a6f73f70710")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "9c785232-2f8f-451d-876d-3a939db24b52")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pintype "passive")
			(uuid "62608519-c6f9-40b8-bd39-e7a111f1f88f")
		)
		(pad "3" smd roundrect
			(at 0.937501 0 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "OVERHEAT")
			(pintype "passive")
			(uuid "8367ce54-2b14-4c4b-9593-602efc526b9a")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm"
		(layer "F.Cu")
		(uuid "51f72bf6-7f2d-40a4-976b-0a5ec9708a76")
		(at 38.3 60.6)
		(descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
		(tags "test point THT pad")
		(property "Reference" "TP10"
			(at -1.1 1.7 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "d665096d-7f03-4899-bd29-b80adf01cd89")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(uuid "62d1bb0f-4c5a-4573-af11-45401a829634")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "82a4abd9-5b38-4265-9516-f2de5371b3bd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4e3aeb9f-71ad-4080-a372-907d14dc955f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2af27946-e7f3-4c92-bff1-fb11c9393d06")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/6c508ac5-4e0f-4371-8506-3f0fbe2facc6")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 0 0.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "b42e5f5b-4852-4fec-8d4e-3feb0d95baff")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "c4ae1a43-af1b-4ff8-aac1-3ccc1096b8ad")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
			(uuid "7d84c104-365e-4193-91b5-d3c2b807aa49")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1 1)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "X_Ua_MON")
			(pinfunction "1")
			(pintype "passive")
			(uuid "0417678f-acdd-4a3e-b879-0a75a236e93b")
		)
	)
	(footprint "Ecohim:TestPoint_Pad_D0.8mm_no_circle"
		(layer "F.Cu")
		(uuid "54eb938a-472f-4a80-8f2d-9497e85e90cb")
		(at 82 46.6 -90)
		(descr "SMD pad as test Point, diameter 0.8mm")
		(tags "test point SMD pad")
		(property "Reference" "TP6"
			(at 0 -1.448001 90)
			(layer "F.SilkS")
			(hide yes)
			(uuid "33742dd1-0178-49b2-8d25-64b6559854c0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 1.550001 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "88188a8c-029b-4bc1-98b6-89cfc9c14847")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Ecohim:TestPoint_Pad_D0.8mm_no_circle"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "45abe849-a211-4812-8c06-e0de3399d54a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "040ae057-5c58-4748-95d8-54b484186211")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "60a0c345-d6e4-4d85-8a72-65aeecbb1e4e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/09073773-b1c9-4c92-b2ed-40e4ee048435")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 0.381 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "890683f0-6479-4d4e-a5a6-7ec5d7bfc874")
		)
		(pad "1" smd circle
			(at 0 0 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask")
			(net 53 "Net-(D4-PB12)")
			(pinfunction "1")
			(pintype "passive")
			(uuid "6c9806cc-45bb-4eca-9a5f-c663d813daad")
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(uuid "5d806f2e-ea67-4dfc-a9e4-c25773a05cd7")
		(at 39.2 47.550001)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "VD10"
			(at -0.7 -1.800003 0)
			(layer "F.SilkS")
			(uuid "e4a7a739-ec79-4639-9daa-e9f80179eda9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MMSZ5234B"
			(at 0 2.1 0)
			(layer "F.Fab")
			(uuid "41e94b40-dd88-4dee-8259-ee99b8cca0d3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "503c9705-b8b3-49e7-99dc-4155bfde223d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4de3840a-b659-4429-9084-9b389bbf89da")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8c3a2c2b-8db5-4026-a946-f931004ba7d4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/8017539211"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "90af6798-e202-4ac7-bdbd-23dff9f55bb8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/bc9e05b3-24c0-4c49-ba69-80504db63a68")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.36 -1)
			(end -2.36 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b3b31c9e-e939-47f0-9298-f37d0a4a3489")
		)
		(fp_line
			(start -2.36 -1)
			(end 1.65 -1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f1ac2cc8-43c9-4240-9884-40bc9f543e5e")
		)
		(fp_line
			(start -2.36 1)
			(end 1.65 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eaf6bf48-b5a6-4655-999d-b88331f87245")
		)
		(fp_line
			(start -2.35 -1.15)
			(end -2.35 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ffc5d9ff-9009-4d5b-95c9-cf4c8f1afedb")
		)
		(fp_line
			(start -2.35 -1.15)
			(end 2.35 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9c1484bc-15bb-47bd-8dda-62c5ab38dfde")
		)
		(fp_line
			(start 2.35 -1.15)
			(end 2.35 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e8dd0cb6-6303-4fca-b2d2-38b8ac27199d")
		)
		(fp_line
			(start 2.35 1.15)
			(end -2.35 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d33d8b79-9965-4e79-a516-c4b5ae8f009d")
		)
		(fp_line
			(start -1.4 -0.900001)
			(end 1.4 -0.900001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9ac7520f-8c7d-4c49-be43-348c3b105b55")
		)
		(fp_line
			(start -1.4 0.900001)
			(end -1.4 -0.900001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "384f6ba0-b5ac-4b0b-879f-d1ed49308807")
		)
		(fp_line
			(start -0.75 0)
			(end -0.349999 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4ee85a0d-dd87-40cc-a27f-8f235063a971")
		)
		(fp_line
			(start -0.349999 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d27ae5bf-ff65-4b6c-a008-8b8b713ea32f")
		)
		(fp_line
			(start -0.349999 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6be1b8fd-d6ca-42cd-9827-6d2046d5d23a")
		)
		(fp_line
			(start -0.349999 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b7f24a75-e119-4397-add0-115b509296f5")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aef2141e-4ed9-4d1f-8e22-64fb4b1a223c")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6004c55c-bed0-4232-81a5-1f7c3abd6fd3")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.349999 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a2c7b5cc-306c-4dc6-88fe-7d3c87ab959f")
		)
		(fp_line
			(start 1.4 -0.900001)
			(end 1.4 0.900001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2d833452-00c6-4ce8-b4f4-f562c03a0abe")
		)
		(fp_line
			(start 1.4 0.900001)
			(end -1.4 0.900001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "90e5bf3b-472e-4761-91cd-41c97d4161f5")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2.000001 0)
			(layer "F.Fab")
			(uuid "bcb6d32b-aebd-4f04-8d34-7672f7edbeef")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 87 "Net-(VD10-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "10b546d4-bcf6-440c-9a26-adb71bedd56f")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "797480c1-98cd-4afe-b2ad-bfbe0a6203ae")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_HC49-4H_Vertical"
		(layer "F.Cu")
		(uuid "60b1871f-bed6-4f36-b5cc-f9e3741398f6")
		(at 101.1 55.050001 90)
		(descr "Crystal THT HC-49-4H http://5hertz.com/pdfs/04404_D.pdf")
		(tags "THT crystalHC-49-4H")
		(property "Reference" "BQ1"
			(at 2.44 -3.525 90)
			(layer "F.SilkS")
			(uuid "6d7b3521-725a-449f-9743-415103a94c76")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "8MHz"
			(at 2.44 3.525 90)
			(layer "F.Fab")
			(uuid "1264a425-b2c2-4a96-932b-262a2c09c382")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Crystal:Crystal_HC49-4H_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3798aa2d-c5a4-4bba-9754-964a645dfcb6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6aa55e7b-0c76-415c-ae26-3f8a7f0c05fa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c5bfea51-9a12-4ccd-8304-176ae40f4f42")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Crystal*")
		(path "/765c30b6-9e03-468b-9670-9bf6289067dd")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -0.76 -2.525)
			(end 5.64 -2.525)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2b57682f-efe1-4205-b71e-8b93896596c9")
		)
		(fp_line
			(start -0.76 2.525)
			(end 5.64 2.525)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1142ba49-b34f-44a8-a406-5b8c124feb81")
		)
		(fp_arc
			(start 5.64 -2.525)
			(mid 8.165 0)
			(end 5.64 2.525)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "621c8620-1f24-4912-b669-650594117e7b")
		)
		(fp_arc
			(start -0.76 2.525)
			(mid -3.285 0)
			(end -0.76 -2.525)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c7be9148-c6cd-423f-a144-7b8515dd0eb1")
		)
		(fp_line
			(start 8.500001 -2.8)
			(end -3.599999 -2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "92646171-b348-4f79-8ccd-7d86e3e6f5f1")
		)
		(fp_line
			(start -3.599999 -2.8)
			(end -3.599999 2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b07095fd-81c1-4e61-9196-77f89236222a")
		)
		(fp_line
			(start 8.500001 2.8)
			(end 8.500001 -2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "26c6317a-cab9-4b2c-b1eb-9ea0aaaff011")
		)
		(fp_line
			(start -3.599999 2.8)
			(end 8.500001 2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f04fa5a4-761a-41c9-b1f1-9f488e0ee0f8")
		)
		(fp_line
			(start -0.76 -2.325)
			(end 5.64 -2.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fd340299-b790-4ae9-bb08-60b163b0ee3b")
		)
		(fp_line
			(start -0.56 -2)
			(end 5.439999 -2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "13cd64bf-6045-4358-8640-be82fcb62494")
		)
		(fp_line
			(start -0.56 2)
			(end 5.439999 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6c652221-8fb4-40d6-a2db-8ffedb27bc7c")
		)
		(fp_line
			(start -0.76 2.325)
			(end 5.64 2.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "25380a0b-ef74-4b76-82c8-4719d57161a6")
		)
		(fp_arc
			(start 5.64 -2.325)
			(mid 7.965 0)
			(end 5.64 2.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f5a78e75-73a5-4edf-b2a6-7545e4420333")
		)
		(fp_arc
			(start 5.439999 -2)
			(mid 7.44 0)
			(end 5.439999 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "152be621-70d7-4f94-ad7c-46571e93adc9")
		)
		(fp_arc
			(start -0.56 2)
			(mid -2.56 0)
			(end -0.56 -2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0ea1754a-95cf-4032-a6b0-73758e703470")
		)
		(fp_arc
			(start -0.76 2.325)
			(mid -3.085 0)
			(end -0.76 -2.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d888764f-8318-42da-957f-355779f77120")
		)
		(fp_text user "${REFERENCE}"
			(at 2.440001 0 90)
			(layer "F.Fab")
			(uuid "8854a2a9-8bd0-41cc-a1a4-2f4c108def5a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D4-PD0)")
			(pinfunction "1")
			(pintype "passive")
			(uuid "9aff7208-6f94-4760-a8b3-5bff63bd18ca")
		)
		(pad "2" thru_hole circle
			(at 4.88 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(D4-PD1)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "34466cf8-46da-47c3-ae5b-31ed01c358d1")
		)
		(model "${KICAD8_3DMODEL_DIR}/Crystal.3dshapes/Crystal_HC49-4H_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "6ca7daa3-69b4-4299-a4ca-da09463f169d")
		(at 54.9 47.162499 -90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "VD4"
			(at -2.5 -1.8 180)
			(layer "F.SilkS")
			(uuid "ca07ceb4-f892-4077-8fb5-a1aa14eb7a5c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BAT54S"
			(at 0 2.4 90)
			(layer "F.Fab")
			(uuid "7e2bff4e-d7ed-47c8-a198-2badd806af24")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "26accdad-102d-4104-be50-530dc5257651")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds11005.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "235da5fc-cecf-46c9-b8dc-44aae45ac733")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "dual schottky barrier diode, in series"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "009677e6-f7c9-4b8e-b364-e464b9644c63")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Link" "https://www.chipdip.ru/product/bat54s-nxp"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "652840cd-b953-402c-8e96-9a349dec5366")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/c4de1c61-4657-4094-9657-728d9a1ec762")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 1.560001)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cba60767-b695-4023-a413-1627af3613dd")
		)
		(fp_line
			(start 0 1.560001)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2319beca-0207-434d-b735-4d89d3b2b2fd")
		)
		(fp_line
			(start 0 -1.560001)
			(end -0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d0f5d7a2-1201-4901-a133-c519410bbbbb")
		)
		(fp_line
			(start 0 -1.560001)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4fa7feee-dabf-45f0-905a-670609d28903")
		)
		(fp_poly
			(pts
				(xy -1.1625 -1.51) (xy -1.4025 -1.84) (xy -0.9225 -1.839999) (xy -1.1625 -1.51)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "297731ff-57a4-4fb5-8efd-9470358da256")
		)
		(fp_line
			(start -1.92 1.700001)
			(end 1.92 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9035f8c4-f5e9-4778-bb57-9dee526e0211")
		)
		(fp_line
			(start 1.92 1.700001)
			(end 1.92 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "acfa7f0f-1022-45bb-9781-e60182accefe")
		)
		(fp_line
			(start -1.92 -1.700001)
			(end -1.92 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e6e4c398-71e4-4e02-87e4-b8a31ce93c2a")
		)
		(fp_line
			(start 1.92 -1.700001)
			(end -1.92 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e31ed2f3-5cdf-4343-a6ad-a1614995996c")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f6cf4452-bf93-41ce-a6b8-6c0a97b96597")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "927a784e-09d8-4aae-894a-146c7de1ad58")
		)
		(fp_line
			(start -0.65 -1.125001)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "72e84877-b1f8-4bcc-ab89-bfdd1e367f48")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bef36ffb-78ef-4878-98ed-0f7c7b303f29")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "320fa725-d0c8-45af-8869-e5f5561f3e9c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "912a2de0-e8bc-4fd3-abdc-0958e272f8c0")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "b0d22d3e-b818-4aad-935e-85a9d0980017")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pintype "passive")
			(uuid "c4ff49cb-1049-464a-a4d2-5732b15d813d")
		)
		(pad "3" smd roundrect
			(at 0.937501 0 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "OVERLOAD")
			(pintype "passive")
			(uuid "ad7dbfa5-a994-4c59-bafc-67a0f739d865")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(uuid "6e91051b-cd5b-47c6-ad77-e05b86662b30")
		(at 101.2 40.8)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "TP1"
			(at 0 -1.998 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "f3474c64-98b5-4044-8b2b-88d563d21798")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.Fab")
			(uuid "e7fe8024-b595-4a13-af56-5d9321c68893")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "090d5e15-c8db-47ff-ae66-5233ac94afa5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8f46bd62-bc11-4751-9d7e-9f78a6252543")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ca1fdcad-9c3e-4639-80a3-cd3a91f07cda")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/47313c9f-88dc-489c-9bda-3f04832ea38d")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 0 1.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "1cbfa672-6644-4e37-9084-7067eba51ea6")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "f1626124-3d45-41c2-9e5a-705e2af47fe6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
			(uuid "e7829b15-b5ca-47f1-9745-89ea73351fab")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "1")
			(pintype "passive")
			(uuid "2703a47d-8228-478b-9828-d45826c20608")
		)
	)
	(footprint "Ecohim:DS1070-4MR_WF-4RA_CONNFLY"
		(layer "F.Cu")
		(uuid "7575392b-ed1b-4e4f-bcec-ebd0ef559075")
		(at 126.3 39.3 -90)
		(descr "Connfly DS1070-4MR, WF-4RA")
		(tags "connector")
		(property "Reference" "X2"
			(at -1.2 2.3 90)
			(layer "F.SilkS")
			(uuid "a6e249e5-dc97-4b1b-a6a2-57dbdad377f3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "WF-4R"
			(at 1.2 2.4 90)
			(layer "F.Fab")
			(uuid "b731b0db-f093-45cf-8a99-607954706d3e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Ecohim:DS1070-4MR_WF-4RA_CONNFLY"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "d05c40a0-914a-4ecf-90fc-9b3cf0b3ac0a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "10bbd309-b6ff-4ae8-bf4d-92bf90f578d3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "152cec09-e8d8-4fff-90a5-ddfec947dec3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Label" "RS-485"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ab583387-9e9f-414a-8551-6af3c544b522")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Link" "https://www.chipdip.ru/product/wf-4r"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ee688e4b-dac5-4aba-ac12-af5ca0b811b2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/692694bf-5218-45cb-8d47-5ebd9c6c398d")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -0.2 -1.6)
			(end 0.2 -1.6)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "099af9ed-74ad-4950-b560-e1df5abaebe8")
		)
		(fp_line
			(start 2.34 -1.6)
			(end 2.74 -1.6)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "4da11b79-0266-40e6-9c70-01bf959c8b1f")
		)
		(fp_line
			(start 4.88 -1.6)
			(end 5.28 -1.6)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "a2665fe6-73b4-4a0b-b8ba-f078d6b91867")
		)
		(fp_line
			(start 7.42 -1.6)
			(end 7.82 -1.6)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "b577180e-85a7-417b-adfd-1068df0ee9f7")
		)
		(fp_line
			(start -1.27 -2.4)
			(end -0.65 -2.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "98ef1abf-a4c3-4e55-82f5-f7b13b8fe358")
		)
		(fp_line
			(start -0.65 -2.4)
			(end -0.65 -3.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "07d794ac-2dce-44f7-8bd8-9d891f3baf2b")
		)
		(fp_line
			(start 0.65 -2.4)
			(end 1.89 -2.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "3c4170fe-ae0a-45a3-82ce-ed3e11bf603c")
		)
		(fp_line
			(start 3.19 -2.4)
			(end 3.19 -3.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "2180c087-377b-4af6-8686-21e6650a0cd4")
		)
		(fp_line
			(start 4.43 -2.4)
			(end 3.19 -2.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "382e22c5-a796-4822-9b82-3299252b221e")
		)
		(fp_line
			(start 5.73 -2.4)
			(end 5.73 -3.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "cd123900-5b50-4056-aec3-11255317ef59")
		)
		(fp_line
			(start 6.97 -2.4)
			(end 5.73 -2.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "c4b41c50-a05e-4592-a96f-dbc26c658ba3")
		)
		(fp_line
			(start 8.27 -2.4)
			(end 8.27 -3.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "c8903145-5b85-4614-acd0-91a9e275dc9c")
		)
		(fp_line
			(start 8.89 -2.4)
			(end 8.27 -2.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "01afd23b-aeeb-4443-ab7b-4c9191b99dd1")
		)
		(fp_line
			(start -0.2 -3.4)
			(end -0.2 -1.6)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "31e027c3-857b-4110-84a3-b036fd3005fd")
		)
		(fp_line
			(start 0.2 -3.4)
			(end 0.2 -1.6)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "581d53c7-e249-4945-9cf9-0fb55abb2026")
		)
		(fp_line
			(start 0.65 -3.4)
			(end 0.65 -2.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "4ce9dcb4-e217-40b6-82b7-63438b9668fd")
		)
		(fp_line
			(start 0.65 -3.4)
			(end -0.65 -3.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "60646690-530f-4d61-8481-05faa78567b8")
		)
		(fp_line
			(start 1.89 -3.4)
			(end 1.89 -2.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "bf0d534a-035a-463b-a4ce-a2a02dc635fe")
		)
		(fp_line
			(start 2.34 -3.4)
			(end 2.34 -1.6)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "c5f9316f-0290-43e1-9822-8490d622acc4")
		)
		(fp_line
			(start 2.74 -3.4)
			(end 2.74 -1.6)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "35262830-a0e0-4d2d-9064-f927cd806e5b")
		)
		(fp_line
			(start 3.19 -3.4)
			(end 1.89 -3.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "dd1e77af-2e57-4de9-8a08-6e2e5f040494")
		)
		(fp_line
			(start 4.43 -3.4)
			(end 4.43 -2.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "51952889-bb20-441f-abf3-acf0bbaf8337")
		)
		(fp_line
			(start 4.88 -3.4)
			(end 4.88 -1.6)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "bc95fe10-6a76-4893-88f7-70bae4f5d87d")
		)
		(fp_line
			(start 5.28 -3.4)
			(end 5.28 -1.6)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "a415f459-136e-43e1-817c-602063f052e9")
		)
		(fp_line
			(start 5.73 -3.4)
			(end 4.43 -3.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "e25fc096-23c1-43e7-b59a-8ca9ffb8a2de")
		)
		(fp_line
			(start 6.97 -3.4)
			(end 6.97 -2.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "025135c2-b1cd-4b6c-a9e3-8084a8ce12ad")
		)
		(fp_line
			(start 7.42 -3.4)
			(end 7.42 -1.6)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "3392c4fb-538d-48dd-9c8b-fac68d1d02cd")
		)
		(fp_line
			(start 7.82 -3.4)
			(end 7.82 -1.6)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "bee3eb7a-e61b-44a6-a4fa-5547fa327141")
		)
		(fp_line
			(start 8.27 -3.4)
			(end 6.97 -3.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "93143797-ae8d-4ee6-bf98-518c2d038e72")
		)
		(fp_line
			(start -1.27 -5.4)
			(end -1.27 -2.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "16dabbe5-2d15-4142-adc5-da06575d5c39")
		)
		(fp_line
			(start -1.27 -5.4)
			(end 8.89 -5.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "30e92c2b-9be9-4e79-9aea-d414417104c0")
		)
		(fp_line
			(start -0.2 -5.4)
			(end -0.2 -13.3)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "90e6366b-bf26-4517-b43f-6563d805a85b")
		)
		(fp_line
			(start 2.74 -5.4)
			(end 2.74 -13.3)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "fbf24bc7-d399-41e0-8e12-b54a0da64d49")
		)
		(fp_line
			(start 5.28 -5.4)
			(end 5.28 -13.3)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "0a994f4e-aeea-4b7d-a62e-7a32a9972d81")
		)
		(fp_line
			(start 7.82 -5.4)
			(end 7.82 -13.3)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "753bdffc-f3ec-4349-a71e-a124af30797e")
		)
		(fp_line
			(start 8.89 -5.4)
			(end 8.89 -2.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "53a2f279-a1d7-4a63-a649-7208653b8fa4")
		)
		(fp_line
			(start 0.2 -7.62)
			(end 2.3 -7.62)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "ef9a060c-5d14-46ef-b113-242cbfd3c373")
		)
		(fp_line
			(start 2.75 -7.62)
			(end 4.85 -7.62)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "be0ec2c4-34a7-46cd-aa44-85086efe730c")
		)
		(fp_line
			(start 5.29 -7.62)
			(end 7.39 -7.62)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "8ded1d76-6c39-4452-b820-a8dccf96c3ca")
		)
		(fp_line
			(start 0.2 -9.65)
			(end 2.3 -9.65)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "f9e5c63f-e05b-452c-b4fd-3df086ce6467")
		)
		(fp_line
			(start 2.75 -9.65)
			(end 4.85 -9.65)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "6b02b4f6-5a44-4eaa-abbf-ef5e907061ab")
		)
		(fp_line
			(start 5.29 -9.65)
			(end 7.39 -9.65)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "710a69bd-2f29-44be-8fdc-f3cbe955414b")
		)
		(fp_line
			(start -0.2 -13.3)
			(end -0.1 -13.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "0a3b9059-855c-4631-a7b5-d5f8298e289d")
		)
		(fp_line
			(start 0.2 -13.3)
			(end 0.2 -5.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "cc0cbfdb-10b6-4dbf-8ced-670696d67afc")
		)
		(fp_line
			(start 2.34 -13.3)
			(end 2.34 -5.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "f0be1f2a-c183-4e5c-85b6-93f93dd579e0")
		)
		(fp_line
			(start 2.74 -13.3)
			(end 2.64 -13.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "7f41381d-613c-435b-b30d-d9c57a307453")
		)
		(fp_line
			(start 4.88 -13.3)
			(end 4.88 -5.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "03d49e88-b785-455a-8315-3c4384c7ec37")
		)
		(fp_line
			(start 5.28 -13.3)
			(end 5.18 -13.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "91d213cf-84ba-4bce-bf47-fe7f980c37be")
		)
		(fp_line
			(start 7.42 -13.3)
			(end 7.42 -5.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "b61836ba-a3ab-4a8c-9546-b34a4c3699f6")
		)
		(fp_line
			(start 7.82 -13.3)
			(end 7.72 -13.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "e0a0a15f-6c41-40f8-802d-edc66cb0d6ce")
		)
		(fp_line
			(start -0.1 -13.4)
			(end 0.1 -13.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "73f352b2-58d3-4cd6-bf79-8a16e0c00675")
		)
		(fp_line
			(start 0 -13.4)
			(end 0 -13.9)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "ce985b79-f029-46dd-9ad3-d90dfcafa495")
		)
		(fp_line
			(start 0.1 -13.4)
			(end 0.2 -13.3)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "581640f1-b31e-4161-99dc-9f11e0070484")
		)
		(fp_line
			(start 2.44 -13.4)
			(end 2.34 -13.3)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "84c593dd-3efc-478a-873d-01f11e90dc01")
		)
		(fp_line
			(start 2.64 -13.4)
			(end 2.44 -13.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "c1154f52-12ba-4ebd-b454-45ebe82e137a")
		)
		(fp_line
			(start 4.98 -13.4)
			(end 4.88 -13.3)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "a6270410-92be-4689-89cc-ebd6a31d8c66")
		)
		(fp_line
			(start 5.18 -13.4)
			(end 4.98 -13.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "045b7c0f-51bb-4524-9f2d-3d6679f24d53")
		)
		(fp_line
			(start 7.52 -13.4)
			(end 7.42 -13.3)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "4fdd4442-0164-48bc-ab5d-4758f43d09d9")
		)
		(fp_line
			(start 7.72 -13.4)
			(end 7.52 -13.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "2624c7cb-cca9-49fe-8223-8987808ac0dd")
		)
		(fp_line
			(start 0 -13.9)
			(end 7.62 -13.9)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "19a6d09a-1b79-468c-b38f-79b7866d3177")
		)
		(fp_line
			(start 7.62 -13.9)
			(end 7.62 -13.4)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "8bdacc53-b4c6-4e6e-8c38-d1af74e1349f")
		)
		(fp_rect
			(start -1.4 -14)
			(end 9.08 1.4)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "8a41921b-d60a-4fb5-8879-99f99bc1570b")
		)
		(fp_rect
			(start -1.4 -14)
			(end 9.08 -1.4)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "9da3601a-5a22-4137-b0eb-f50b571960f4")
		)
		(fp_text user "${REFERENCE}"
			(at 1.200001 3.9 90)
			(layer "F.Fab")
			(uuid "2ec07be7-6134-4589-a851-12dcee414afb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole roundrect
			(at 7.62 0 270)
			(size 1.6 2.54)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 71 "Net-(X2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "2ecadb06-5dee-4fc6-b261-c8cea0c5af42")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 270)
			(size 1.6 2.54)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(D2-A)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "022fd24c-69d0-47f1-ab90-33d2b89a6420")
		)
		(pad "3" thru_hole oval
			(at 2.54 0 270)
			(size 1.6 2.54)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(D2-B)")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "b36f2434-3f7c-45ec-889f-b7e9ffff9aa4")
		)
		(pad "4" thru_hole oval
			(at 0 0 270)
			(size 1.6 2.54)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "fcd83ba7-732b-4c6d-83b0-6be3ddbd8777")
		)
		(model "${ECOHIM_LIB}/Ecohim.3dmodels/DS1070-4MR_WF-4RA_CONNFLY.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Ecohim:TestPoint_Pad_D0.8mm_no_circle"
		(layer "F.Cu")
		(uuid "77c9a524-d2ee-49f1-9439-80f4dee10ff9")
		(at 94.5 46.5 -90)
		(descr "SMD pad as test Point, diameter 0.8mm")
		(tags "test point SMD pad")
		(property "Reference" "TP5"
			(at 0 -1.448001 90)
			(layer "F.SilkS")
			(hide yes)
			(uuid "026c663b-bd9e-48d2-9885-6b95185bb50d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 1.550001 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "60f06f70-6406-424e-87e9-fe1071b01ce0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Ecohim:TestPoint_Pad_D0.8mm_no_circle"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "02ce1e03-4e69-4195-8cbb-ead07c3954e0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "5a0f33c2-d4af-48b0-b72e-46ece0cfab24")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "10c49f7d-00f9-41bc-8585-c6f4141b2efe")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/ddbdacc6-155d-4dd6-8260-306452675304")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 0.381 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "810f6e4d-bf9c-48b6-a221-52ebeac6133b")
		)
		(pad "1" smd circle
			(at 0 0 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask")
			(net 56 "Net-(D4-PA3)")
			(pinfunction "1")
			(pintype "passive")
			(uuid "9ff02abb-78ee-4140-94f4-8df357c75867")
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm"
		(layer "F.Cu")
		(uuid "7da391c5-9299-45c5-a4db-611a9ed2a7f6")
		(at 43.3 51.2)
		(descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
		(tags "test point THT pad")
		(property "Reference" "TP17"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "5fb9498a-1752-4548-b77e-459daa30858f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(uuid "dda3370c-a439-467d-94a2-f9dbb5624051")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "00c62aa7-2b65-4b4d-a561-fe10525fcf0b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f7297ffc-9a42-4219-880d-8084f0292478")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ba79e0cf-6b3b-4fdb-b8c0-57adcf54fd50")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/467561fc-cf5c-44a4-92a9-6b24430244bd")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 0 0.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "33ee2411-547b-4eb9-878e-bfcd0318c172")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "53376afa-55a8-4856-bc9f-7c862d05e644")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
			(uuid "0b918f38-ffa1-4113-aeb3-809704d711bb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1 1)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "Ia_MON")
			(pinfunction "1")
			(pintype "passive")
			(uuid "a8a2933c-9e09-4d71-a2a3-000a7ee92791")
		)
	)
	(footprint "Ecohim:TestPoint_Pad_D0.8mm_no_circle"
		(layer "F.Cu")
		(uuid "7f89a9a6-e784-4ec3-80be-72b3b4efedcf")
		(at 82 50.2 -90)
		(descr "SMD pad as test Point, diameter 0.8mm")
		(tags "test point SMD pad")
		(property "Reference" "TP9"
			(at 0 -1.448001 90)
			(layer "F.SilkS")
			(hide yes)
			(uuid "7d12b27c-6b85-478e-8609-c0f3d8e4c7da")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 1.550001 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "b7ad059f-940e-45dc-9a00-d7013af13e15")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Ecohim:TestPoint_Pad_D0.8mm_no_circle"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "5f152050-e6fa-44c1-a955-473c9d5e2a9b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "b9d155b5-7c1b-47ef-a753-1eb28dc77844")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "2f41b4e7-2a3a-4da9-a627-e3207bdfadc1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/bcae8217-3338-40f9-8797-38e6737fd095")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 0.381 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "2a95bf60-f6ab-4b09-9fb9-c35468607caf")
		)
		(pad "1" smd circle
			(at 0 0 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask")
			(net 60 "Net-(D4-PB15)")
			(pinfunction "1")
			(pintype "passive")
			(uuid "613d5d06-caac-4570-b20a-ab50b8da38b8")
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric"
		(layer "F.Cu")
		(uuid "848a0f0c-a0ea-4358-a5e1-8d2ba9cc6b5e")
		(at 120.5 44.9)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "HL1"
			(at -1.8 0.4 180)
			(layer "F.SilkS")
			(uuid "74bb00ac-41fb-41d2-b821-7f6d764f82c1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify right)
			)
		)
		(property "Value" "KP-2012SGD"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "2bacc910-528f-4941-8370-d20b61d77bb3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "LED_SMD:LED_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "11a359af-0455-4fde-a450-263604a151ba")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3ab360db-0b6e-43e5-a709-db7ed5a90227")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9ad8dc8c-1126-4c09-89a5-7595092b0dd0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Label" "Power"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "20feee35-2a95-4f2a-b529-b8361ceeffd6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Alternative" "Green"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "935e56a5-c699-47a8-8538-3b7532c51a66")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/e4ccd2c2-e9c1-465a-aa74-7adacefb2cd6")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.685 -0.96)
			(end -1.685 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "363773d7-6a37-43dd-b7aa-30c9a2a789de")
		)
		(fp_line
			(start -1.685 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b262b978-0a50-42d9-8ff2-d6f00b39baec")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.685 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2ec147e3-758a-4cb5-a033-0fa2ca3acb7b")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "17e85f3c-c9ef-4c1b-b59e-d2d79584642e")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "28327497-eab1-47ed-9706-90cc3ebd61ef")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2e0b259e-6ec2-4c32-b0ee-fa0807c070e1")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fd458f38-ccbd-4e9d-b2b6-e31706164fb1")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0c8e6f7a-92b7-4e17-92b0-639e8ff35a3b")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c4570fa8-35a4-42da-af5f-995df4274e09")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4310d769-2f0f-482f-8e65-d43f9cb7afcd")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "da3e090b-21f1-4302-8f7f-72da875db55b")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "08cd2c2a-0835-4a2a-a3da-48b847a9ad6c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b1d85f71-a298-44cb-b29d-492bff98be8f")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 72 "Net-(HL1-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "6f84601e-068e-4900-bbc3-a261678af928")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+12V")
			(pinfunction "A")
			(pintype "passive")
			(uuid "692b6036-6fa5-4cef-bd79-ffa156b57b1f")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fiducial:Fiducial_1mm_Mask3mm"
		(layer "F.Cu")
		(uuid "8b06bebc-3b21-49d0-b3cc-ae8d4fda1b71")
		(at 32 60.5)
		(descr "Circular Fiducial, 1mm bare copper, 3mm soldermask opening (recommended)")
		(tags "fiducial")
		(property "Reference" "FID2"
			(at 0 -2.54 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "e80d9a8a-3d7b-4e10-8578-9bfc0337977f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Fiducial"
			(at 0 2.286 0)
			(layer "F.Fab")
			(uuid "bc01485f-f696-411a-970e-cc2547c0aefb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Fiducial:Fiducial_1mm_Mask3mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "94be1097-01bd-44e1-92f5-7d9472a2fc0b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c701cebb-a236-428c-9059-fe61c21fde32")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Fiducial Marker"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "90b40d73-94b2-4dda-8ccb-6f9e177df32b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Fiducial*")
		(path "/a175c4ff-635d-450a-a1ff-966b40b3092e")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1.75 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "d895f830-6e9d-4484-968f-b3d7c3ace2b3")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "c21ed427-4b00-4078-be5f-a53b27f0a2c0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3661a228-d421-4111-a62f-2910114942f6")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 1)
			(clearance 1)
			(uuid "f063e840-8638-4e44-af97-c975a0f7e487")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "911e7df9-3165-4b65-afb3-8df8d6933ea8")
		(at 62.9 47.162499 -90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "VD3"
			(at -2.5 -1.1 180)
			(layer "F.SilkS")
			(uuid "d824a9aa-e7c1-4cbb-91da-700f027dcf11")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BAT54S"
			(at 0 2.4 90)
			(layer "F.Fab")
			(uuid "a41d9852-0b4e-4b2f-83d1-ad5e78166522")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a3215d81-3b9f-442b-ad75-34526fb1f7e9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds11005.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8a96bf62-ae86-4e46-b50a-657d68672817")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "dual schottky barrier diode, in series"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "51a38945-927a-44ba-907a-8579f284cd45")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Link" "https://www.chipdip.ru/product/bat54s-nxp"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "876ce418-106e-43ed-8531-3c7c56568065")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/1a910bf6-5f2c-46c9-bcfc-02e0bc63a3d0")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 1.560001)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1aefc03c-fccb-47ae-afc5-2ff6e3bae209")
		)
		(fp_line
			(start 0 1.560001)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b93e7ced-f512-44e4-b011-148a0578ec02")
		)
		(fp_line
			(start 0 -1.560001)
			(end -0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "36d46e02-2942-4eba-9477-a05364c04699")
		)
		(fp_line
			(start 0 -1.560001)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dca0e1c2-4631-4cad-8063-758823ac5d27")
		)
		(fp_poly
			(pts
				(xy -1.1625 -1.51) (xy -1.4025 -1.84) (xy -0.9225 -1.839999) (xy -1.1625 -1.51)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "f9cad5a7-ab63-485e-914b-09ace5aeed7d")
		)
		(fp_line
			(start -1.92 1.700001)
			(end 1.92 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b54bdd47-9602-44b4-bf6b-e5d316552634")
		)
		(fp_line
			(start 1.92 1.700001)
			(end 1.92 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "094810dc-9bc5-44b7-a797-c0f35339af68")
		)
		(fp_line
			(start -1.92 -1.700001)
			(end -1.92 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c540abe4-d27e-4bd2-87ac-79a0b753b026")
		)
		(fp_line
			(start 1.92 -1.700001)
			(end -1.92 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "46cf35ad-1317-488a-a473-d7fcbabf0172")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a7d311d9-422c-47f8-ab6d-fe29d2297344")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f786efe6-2897-4505-869c-a073cc0fd41c")
		)
		(fp_line
			(start -0.65 -1.125001)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "10d05b2e-3230-4379-a362-a741446edc7e")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "721b4168-4d63-4d76-8ce8-ba7b4d7955c2")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "371ca178-a081-4bbc-9a53-2415fad9d409")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "6655112a-f96b-4a84-a2e4-22f73447af65")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "bc7a5a79-5e5d-41ed-879b-7b85644a2a04")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pintype "passive")
			(uuid "c37315e1-528f-4bcd-ac8b-f6437bfd4b7d")
		)
		(pad "3" smd roundrect
			(at 0.937501 0 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "NO_LINK")
			(pintype "passive")
			(uuid "351c6eb8-842c-4940-be25-0ef1df7b2c28")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(uuid "937277e2-1f91-4595-bafe-0cf53cc8ac79")
		(at 41.8 43.4 180)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "D6"
			(at 0 -3.4 0)
			(layer "F.SilkS")
			(uuid "f89f0334-20b4-4237-82f8-bc7d3e15acf3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LM358"
			(at 0 3.4 0)
			(layer "F.Fab")
			(uuid "f0e87da0-bfc5-49ea-b00d-ac96efd99b78")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2b21481e-def0-4ee9-b47e-e51b5153b3db")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2904-n.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "45494cf1-149d-4be6-a6b2-ec62028c7b3d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Low-Power, Dual Operational Amplifiers, DIP-8/SOIC-8/TO-99-8"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a34b7541-0479-43a9-a54e-30d3d1b0d7fa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Link" "https://www.chipdip.ru/product/lm358-sop-8"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "18d40d0b-9de0-41ef-98aa-59cc4df16ff4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*")
		(path "/e90a0ee0-3c79-4842-a0d8-2625dd0326aa")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 2.559999)
			(end 1.95 2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "77ee12f3-0e6d-42ec-9bc2-2380f5f848fd")
		)
		(fp_line
			(start 0 2.559999)
			(end -1.95 2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bf5a9e27-f310-4160-af7e-5d00b4409bd6")
		)
		(fp_line
			(start 0 -2.559999)
			(end 1.95 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c2d25348-4196-4bc4-8e72-9c22522609a2")
		)
		(fp_line
			(start 0 -2.559999)
			(end -1.95 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dda9d623-af8b-4aeb-8cb1-4594220fd268")
		)
		(fp_poly
			(pts
				(xy -2.7 -2.465) (xy -2.939999 -2.795) (xy -2.46 -2.795) (xy -2.7 -2.465)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "decad0d3-8228-4a9b-abfd-06582fa6fc12")
		)
		(fp_line
			(start 3.7 2.7)
			(end 3.7 -2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ec30bfda-8508-4479-986d-78a0fa07e23d")
		)
		(fp_line
			(start 3.7 -2.7)
			(end -3.7 -2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ac2d5d25-c47b-4701-8f2b-6fa705f40f4f")
		)
		(fp_line
			(start -3.7 2.7)
			(end 3.7 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a601eee7-08ad-4f97-9587-173dd565e594")
		)
		(fp_line
			(start -3.7 -2.7)
			(end -3.7 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5c4e3fb2-3134-4159-af49-377d94976282")
		)
		(fp_line
			(start 1.95 2.45)
			(end -1.95 2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a0160633-b6e1-4d39-bc78-48348260364d")
		)
		(fp_line
			(start 1.95 -2.45)
			(end 1.95 2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b0a9fc25-a182-4ffd-8858-bf8b436d1112")
		)
		(fp_line
			(start -0.975 -2.450001)
			(end 1.95 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bcb21255-ec53-44ac-b810-28b808d931a8")
		)
		(fp_line
			(start -1.95 2.45)
			(end -1.95 -1.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3be5bd1a-97f3-4a4b-b64a-fdfff67ba7f7")
		)
		(fp_line
			(start -1.95 -1.475)
			(end -0.975 -2.450001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1f90c144-614b-4421-ae07-32d9fb73185c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c4211876-619e-48f1-ac5e-dd1d6fcdd768")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 88 "Net-(VD9-K)")
			(pintype "output")
			(uuid "a06186ca-a658-450f-a058-9b8887aa8aed")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 68 "Net-(D6A--)")
			(pinfunction "-")
			(pintype "input")
			(uuid "8f673c41-38fc-4d6d-b9c3-985c439ce461")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "Net-(D6A-+)")
			(pinfunction "+")
			(pintype "input")
			(uuid "a102ce16-3a98-4ac0-9958-f60e59e0bf41")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "V-")
			(pintype "power_in")
			(uuid "70a35702-b215-4915-afb1-067db77c4182")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "Net-(D6B-+)")
			(pinfunction "+")
			(pintype "input")
			(uuid "224f07ef-d082-4e01-a6d1-d36f215efbc6")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 67 "Net-(D6B--)")
			(pinfunction "-")
			(pintype "input")
			(uuid "73a790ff-2421-4f40-965a-035c825e3e4c")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 87 "Net-(VD10-K)")
			(pintype "output")
			(uuid "aca4ca2b-0346-4ec8-a7f8-740c86112255")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "+12VA")
			(pinfunction "V+")
			(pintype "power_in")
			(uuid "5a897666-9952-4fdf-b864-34809cfc3607")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fiducial:Fiducial_1mm_Mask3mm"
		(layer "F.Cu")
		(uuid "93ef1ac3-a1cf-400b-9465-ad7e90d4625e")
		(at 32 37.5)
		(descr "Circular Fiducial, 1mm bare copper, 3mm soldermask opening (recommended)")
		(tags "fiducial")
		(property "Reference" "FID1"
			(at 0 -2.54 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "d61485bd-8fd8-4f34-b166-efefbef24eda")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Fiducial"
			(at 0 2.286 0)
			(layer "F.Fab")
			(uuid "f7e36d74-115c-434b-bb04-8480510d4e44")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Fiducial:Fiducial_1mm_Mask3mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a400a6a7-5d4f-477a-8499-c9f1dd6b73f3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "54818965-89ad-4ec3-9a53-07c62246963c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Fiducial Marker"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7d00e080-7a48-466b-a174-fd0fe45b18b5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Fiducial*")
		(path "/645d0afe-b2a6-4a83-a4e9-e56ae79fa1a3")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1.75 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "b4af578a-0128-43bc-b456-bb168c508fc5")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "96cdb426-b78e-4747-9086-d5888fa9889d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "054ee2b7-66fe-434d-b0d6-1fefdebb64fc")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 1)
			(clearance 1)
			(uuid "ba489851-eb89-4836-b64a-c363991bc78e")
		)
	)
	(footprint "Ecohim:TestPoint_Pad_D0.8mm_no_circle"
		(layer "F.Cu")
		(uuid "994e962f-6f8c-4506-95e2-692a998de945")
		(at 87.800001 60.1 -90)
		(descr "SMD pad as test Point, diameter 0.8mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at 0 -1.448001 90)
			(layer "F.SilkS")
			(hide yes)
			(uuid "a7cf7626-7b2f-4ba4-81bd-d2dc5d83f453")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 1.550001 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "6df85dba-4838-47dd-9172-088c7b593623")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Ecohim:TestPoint_Pad_D0.8mm_no_circle"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "29358d4a-4997-41c9-bb7a-1761f74586ba")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "58c16a85-9df6-45c5-8d8e-4b54ef990bfb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "951b29fb-2560-43a3-bcf3-e322e2e8284b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/1623ae2c-6ba6-45fa-b5d3-974561191afe")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 0.381 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "1866185a-3854-45e8-afc6-3c0c6e8df9ac")
		)
		(pad "1" smd circle
			(at 0 0 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask")
			(net 46 "Net-(D4-PC11)")
			(pinfunction "1")
			(pintype "passive")
			(uuid "8ba5a79d-d64a-40b9-b848-d77ed2cba6ba")
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "9f9a2978-8f61-47bf-8376-322bebd262b7")
		(at 35.000001 43.4 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R27"
			(at -3.250001 -0.3 90)
			(layer "F.SilkS")
			(uuid "492dc044-1ebf-4f70-ba52-194984179ede")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "150"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "51490646-ae2b-4e38-a972-b46d7c91ba97")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0fa926d1-551f-46f0-92fd-d67312eb2d75")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d7ad92fd-5771-4fc1-b6e8-133843d322be")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cdeb09ea-d3c9-494e-9272-ac6914a19bed")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/505d53f2-627a-4cae-b931-907964dd4080")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5cb59e53-7240-4166-a3ed-cf7d30ac256c")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e0051f20-d9a7-4ad8-ae99-6a2ceac65b67")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cf9bea74-e398-4294-a997-e3d9f2af3249")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2604b6e8-e570-4f81-9769-acb759ddbf3d")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "54d50fcf-7331-4f31-866d-4c0aa674b8e6")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d06372e5-2f97-4537-a9e7-695a04e18d92")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e91a331a-59f6-4fec-9a63-a0424b959b75")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cd687d7c-4ec4-460a-b1d2-1ee799dde3b1")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8293f19c-3741-4648-bcc8-5b4abcba9701")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7d3564e2-0037-4a3d-86d6-e4186b92b106")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "b6fc108d-9a9e-4cf1-815e-00c8a47f95a9")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 87 "Net-(VD10-K)")
			(pintype "passive")
			(uuid "8ceae2dc-0bd7-46f2-b3ce-aa492e5b3008")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 84 "X_Ua_CTRL")
			(pintype "passive")
			(uuid "0c52ca3a-ab8a-4429-9f11-379ea56edb64")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "a0bc011c-a672-4c6b-9825-559de8955e8d")
		(at 87.5 40.5 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R31"
			(at 0 0 90)
			(layer "F.SilkS")
			(uuid "82efcd88-0d4c-418b-a34c-373ba9e9d5c2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "ffc91726-6c22-414b-b6ef-4a3c94db8682")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a00272b6-291f-4ed2-b7f6-b4feb86d46b0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e8cb9d37-5118-43c8-ba2b-63f791b9968a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "356b8029-cde5-41f2-9d98-8365319766e5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/467d9d70-58b6-42ce-a2d3-2acf076cb231")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7d7d05c8-dfa3-483f-9db9-e43c6c7e2ade")
		)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "89d02e24-4752-4ff3-9e98-a08a1903c836")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "63dc060b-c24c-4a75-be8b-a0222234589f")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cfb95d8b-2015-47f4-9b63-5db65b9306cc")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f3dcbdaa-d46c-4fee-8c3c-710b6de54e74")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "45dfc1c6-f978-46c9-8bd0-639ebafba0a5")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e6e0b42b-1d9a-41ef-b108-f79cef1bbbe3")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37569b98-53b2-428d-9340-05b1364edd90")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7aa7e98d-3c4b-4567-8bc2-ce0281ca4cf2")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c6b94460-14b9-4c14-9b93-9d4e4c2b9a25")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "b39727d6-bad3-40b5-b2fa-33d7001193d8")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 18 "HV_24V")
			(pintype "passive")
			(uuid "5f916aef-9de1-4ae1-bd2b-f7c1764ed231")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 4 "GND")
			(pintype "passive")
			(uuid "0eccc1cd-d7aa-4786-8482-10b8cab38f64")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric"
		(layer "F.Cu")
		(uuid "a1609a9c-7a58-44a8-9d03-4553fdd0b3e6")
		(at 120.5 39.9)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "HL3"
			(at -2.4 0 90)
			(layer "F.SilkS")
			(uuid "323e5d97-c212-4a08-86d2-daf1c5fdeb34")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "KP-2012SGD"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "5db14ddd-47ba-42ea-bd33-7ef8956993df")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "LED_SMD:LED_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0ef8c38d-437f-4078-9da5-c44ed859a663")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6e61e1c6-0c22-49bb-bd09-3e22740bd49d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "29573915-c17a-4037-906e-e20c43917597")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Label" "ACT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d7ba5d42-56eb-4113-a116-420e656e16a6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Alternative" "Green"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "44621a05-f7c3-485f-9b69-7c63d0d3998d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/96d7b829-fdf5-4980-9b30-1c0c488c74a0")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -1.685 -0.96)
			(end -1.685 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5b1e44c9-7cd0-47f7-a71c-c96efe776e27")
		)
		(fp_line
			(start -1.685 0.96)
			(end 1 0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "92298778-cb71-40f9-beb2-9f09c98cbbd0")
		)
		(fp_line
			(start 1 -0.96)
			(end -1.685 -0.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9ef17d28-e666-4ebd-b4ba-07ed4a39a9cc")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d78ec8da-8e6b-488f-9855-ff162b954d20")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e9a687f3-4c17-41e0-b5f8-8dcb9bb5b442")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d433e30b-d95c-4710-ad7d-d7f2f68fbfed")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "78f566e0-b7ab-4c2b-ab80-d78c2f02a4b8")
		)
		(fp_line
			(start -1 -0.3)
			(end -1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "09c5ae6a-38bb-46eb-86cc-f79549aa1412")
		)
		(fp_line
			(start -1 0.6)
			(end 1 0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "41f1ccd6-b54c-42fe-9d14-d4f1748bff16")
		)
		(fp_line
			(start -0.7 -0.6)
			(end -1 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4b094292-9032-4187-bfca-d5cba063f853")
		)
		(fp_line
			(start 1 -0.6)
			(end -0.7 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f889b8d3-5242-473a-97f7-92cdbb6b3d2d")
		)
		(fp_line
			(start 1 0.6)
			(end 1 -0.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ddfbf4ea-1fd0-48d9-ba08-2c6b2ee177e7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "9f72b094-7b52-4622-ab90-be189ccc1556")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 75 "Net-(HL3-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "2c12dddc-c94a-46f8-aa46-1240805fb23b")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "LED_ACT")
			(pinfunction "A")
			(pintype "passive")
			(uuid "c47bc3ed-f6ca-43fe-8f88-155bfa894367")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "a29ca08b-d161-49e3-ad5b-cee428ee2a84")
		(at 33.2 53.1 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "VD11"
			(at 0.4 2.3 90)
			(layer "F.SilkS")
			(uuid "adb50790-35e2-4bde-be6a-4faa2a647b84")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BAT54S"
			(at 0 2.4 90)
			(layer "F.Fab")
			(uuid "32b900eb-76a4-4259-9fc5-3e57d1677e56")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c8a2d3f1-85ee-4209-8d9b-da6330e2fd1d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds11005.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "23488c26-9a48-4466-9c8f-8167e39f0a7c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "dual schottky barrier diode, in series"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "435643c9-32f6-46cc-ab75-d122cecf6a49")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Link" "https://www.chipdip.ru/product/bat54s-nxp"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "17cc7c0b-36da-4250-ad03-5b1351696c16")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/ba004796-eaa6-461f-b2f1-9d2aff8b71b6")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.560001)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b0dddd1a-80ee-4267-a8a2-3d1012ffe025")
		)
		(fp_line
			(start 0 -1.560001)
			(end -0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b4b21c89-ec1e-44fd-8870-5b2b57979e36")
		)
		(fp_line
			(start 0 1.560001)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "26c50798-21bf-406e-9422-724199ed0db9")
		)
		(fp_line
			(start 0 1.560001)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e7a17c92-0854-419a-997a-c9a8d3481f31")
		)
		(fp_poly
			(pts
				(xy -1.1625 -1.51) (xy -1.4025 -1.84) (xy -0.9225 -1.839999) (xy -1.1625 -1.51)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "85a736e9-9b66-42ce-818d-13a2573f7fe9")
		)
		(fp_line
			(start 1.92 -1.700001)
			(end -1.92 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "55e45f8d-15b2-4773-aab3-d226f8b35ffc")
		)
		(fp_line
			(start -1.92 -1.700001)
			(end -1.92 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "07154a62-18c6-45f3-8fd9-4c9fb3e584dd")
		)
		(fp_line
			(start 1.92 1.700001)
			(end 1.92 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d2f128d1-df2c-44a1-82db-ed7bc7e3b386")
		)
		(fp_line
			(start -1.92 1.700001)
			(end 1.92 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "85a47431-c634-4923-8b2c-d8a20d343d44")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "19cc16bf-7a3b-4e6f-9ef7-bdd65412483b")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ee7057c9-76a3-427f-a46f-b8c30f0f1e96")
		)
		(fp_line
			(start -0.65 -1.125001)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "27e8f92a-4694-4e5b-acce-4b45cc148d32")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d106a739-00f6-4b5b-a254-374ab57ea9e9")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bd415ff5-7af2-49b5-9315-adb3cc6c4028")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "2283861e-dfcf-49b7-9953-7e392516fc7b")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "da75880a-cccb-406a-b316-0520deffc75a")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pintype "passive")
			(uuid "f33d85cc-ae9d-4359-a71f-13458381a4fc")
		)
		(pad "3" smd roundrect
			(at 0.937501 0 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "Ua_MON")
			(pintype "passive")
			(uuid "88dd2220-95fd-4d62-80d7-403ecfae7cad")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "a3aa6679-b6c4-4680-8a3e-27b3748d4d16")
		(at 37 43.4 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R23"
			(at -3.250001 -0.999999 90)
			(layer "F.SilkS")
			(uuid "d0008541-5243-4919-b71a-d2d273e15ac0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "0"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "c6c71481-c334-48d2-9d21-42ce00edce92")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "afcb3399-255b-45a8-854f-fd30f058dbb7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3e9beaf7-a4d6-4203-b0f8-dceffa180484")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2dc93927-8f11-4e18-8e57-426c50b5180d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/e25873e4-f7a9-4052-b2c4-6e9495fffedf")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b1effc36-9be3-4168-8da1-fdc7ee4c112b")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "86d1f969-d5f6-424b-8fd6-5aeb40f28bee")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "22551522-0c43-4753-a497-ba038cb1f75a")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7e59f19b-6950-486c-900b-b4b8e7548394")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "74ec45e0-aa0b-47d0-9af6-f5b2dff0f84a")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9bc39577-6559-4bb3-941c-bd8a2c88bfdf")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "39ff792b-a084-49f1-a273-b1364fe37d3e")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "11b13db6-b000-4f71-bb63-2fe2933f9e09")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5ad2bcb9-71b4-41e2-acc5-189f3757980e")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cb91e233-7762-44cd-a201-834c0df9aee5")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "700d156e-1d10-4789-b597-b1fdffbd0800")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 87 "Net-(VD10-K)")
			(pintype "passive")
			(uuid "dbdca6a8-7724-47fa-8368-c40e0a415d63")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 67 "Net-(D6B--)")
			(pintype "passive")
			(uuid "ffc2cb39-16da-4065-ba10-41eec6511ead")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "a96566ab-3494-4b30-81c0-ee20635381ae")
		(at 67.9 50.862499 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at -1.6 0 90)
			(layer "F.SilkS")
			(uuid "4c4b446d-750d-4f04-b31d-ffd46cfaebb5")
			(effects
				(font
					(size 0.9 0.9)
					(thickness 0.15)
				)
				(justify right)
			)
		)
		(property "Value" "1k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "6d96d4fd-1d80-4cb0-b6aa-79fa775c1290")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5bcd8712-eb80-4d6e-80d3-3afbe9865827")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9465d697-b407-4bac-b2ff-27f48723f83e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d7096315-da80-4bd9-83f6-8a0686454a7a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/06164042-00b7-43e0-affd-cff99171ed1a")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "95258c26-b55b-4467-ab3f-545bd691d511")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "41e545ee-5fa2-416e-ac82-53b9a73c32d3")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b908926a-09a2-4ed4-bc30-11f22429eaac")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "62443194-eb96-4a42-a498-6f2fa1efde7b")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4cf4bb5a-4f5a-4a09-b3d0-4240d5d76a84")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3f7902ba-0f27-43d4-aa26-225a007e3bd1")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c25c0987-bf0a-4642-9331-c0e5076b1d8e")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a37de698-fce5-4e32-b96d-83db3efcd392")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2cae8391-0502-462c-bec1-b8dbfb199e93")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8026247e-e1c5-4608-bac6-61be3f020e02")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "c5e53b98-5575-4989-bf5d-5553e4960665")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 78 "/X_XRAY_ON")
			(pintype "passive")
			(uuid "e10d9438-7677-4d66-92ac-264fa98cef5c")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 8 "XRAY_ON")
			(pintype "passive")
			(uuid "31861b48-1f39-4087-b0db-9c405275de56")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(uuid "aff16daa-498d-4ed8-9dd6-ea8ade7d7c09")
		(at 40.8 55)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "D5"
			(at 2.3 3.4 0)
			(layer "F.SilkS")
			(uuid "039c99c2-6bcb-4529-acec-5006585c8dd9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "LM358"
			(at 0 3.4 0)
			(layer "F.Fab")
			(uuid "a77700ef-48d8-4a34-b460-1182d8818d08")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0d7f6beb-d20e-4e5b-8261-76e678c39b46")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2904-n.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e260a7c9-0b42-4dc3-908e-98f837f9973e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Low-Power, Dual Operational Amplifiers, DIP-8/SOIC-8/TO-99-8"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "793723b7-a4e1-4142-b1eb-33f1aca23a38")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Link" "https://www.chipdip.ru/product/lm358-sop-8"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "19c94387-cf8c-474c-a0b0-38f51ed74b23")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*")
		(path "/d3b56b8e-4f02-4ec8-9145-a9142ab0be84")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -2.56)
			(end -1.95 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3250311f-6d13-4b48-8f0d-0621d66154c5")
		)
		(fp_line
			(start 0 -2.56)
			(end 1.95 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c285206e-99b7-443c-ac8a-97d3903725ec")
		)
		(fp_line
			(start 0 2.56)
			(end -1.95 2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5625a18a-d7e9-4ef6-90ab-c19590681ef5")
		)
		(fp_line
			(start 0 2.56)
			(end 1.95 2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6df778ec-fa69-418d-829d-1a0f49608662")
		)
		(fp_poly
			(pts
				(xy -2.7 -2.465) (xy -2.94 -2.795) (xy -2.46 -2.795) (xy -2.7 -2.465)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "5a6400ae-b321-4959-aad8-4b550cff90bf")
		)
		(fp_line
			(start -3.7 -2.7)
			(end -3.7 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7195cb2c-4e93-4e03-8a60-55f4b2f37950")
		)
		(fp_line
			(start -3.7 2.7)
			(end 3.7 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2ef50398-4476-4529-bcf7-53bb60261962")
		)
		(fp_line
			(start 3.7 -2.7)
			(end -3.7 -2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2bbe5965-e04a-4d1b-a067-b73a41aa2ed0")
		)
		(fp_line
			(start 3.7 2.7)
			(end 3.7 -2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0032c3f3-a9ee-45f9-804f-cd274b91f8ad")
		)
		(fp_line
			(start -1.95 -1.475)
			(end -0.975 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "060dd28d-fa74-4ed4-815c-303c7712d984")
		)
		(fp_line
			(start -1.95 2.45)
			(end -1.95 -1.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9fab1840-1b07-409c-854a-32dc1899baa1")
		)
		(fp_line
			(start -0.975 -2.45)
			(end 1.95 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b2cc04e0-c848-42f4-85cb-ba28a47e728f")
		)
		(fp_line
			(start 1.95 -2.45)
			(end 1.95 2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae9b4fc0-a85d-4bd8-82ae-4ed74a64e4ed")
		)
		(fp_line
			(start 1.95 2.45)
			(end -1.95 2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cb8ef206-a62f-437c-84d3-ee45eb3fe128")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "840de0d7-a034-4a94-aa6b-3857d61b21a3")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "Net-(D5A--)")
			(pintype "output")
			(uuid "58f94e8f-15cd-4508-b43a-8d3c3716c3cc")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "Net-(D5A--)")
			(pinfunction "-")
			(pintype "input")
			(uuid "90136079-1f5b-41c7-8cae-988b51ad046c")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "Net-(D5A-+)")
			(pinfunction "+")
			(pintype "input")
			(uuid "6df50cc1-d857-4d3b-ad8f-92b443775472")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "V-")
			(pintype "power_in")
			(uuid "35c12fe4-ebce-479d-98d7-f8322622caab")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(D5B-+)")
			(pinfunction "+")
			(pintype "input")
			(uuid "ae3a1f4b-7773-47d2-a6f7-92b1c3cd557c")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 66 "Net-(D5B--)")
			(pinfunction "-")
			(pintype "input")
			(uuid "abcd56d0-1825-4033-b5d6-951d3a9dcef2")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 66 "Net-(D5B--)")
			(pintype "output")
			(uuid "c64b87ad-5a58-49ec-83e9-9642b4f0fd8b")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "+12VA")
			(pinfunction "V+")
			(pintype "power_in")
			(uuid "ae6907ee-1267-4482-a81b-09f26a3391ac")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm"
		(layer "F.Cu")
		(uuid "b549947c-6dce-421f-b650-70c24de18047")
		(at 33 42.449999 180)
		(descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
		(tags "test point THT pad")
		(property "Reference" "TP15"
			(at 0 -1.448001 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "3902ebab-6ff9-43f8-8b22-f28de3c6f841")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 1.550001 0)
			(layer "F.Fab")
			(uuid "fe9d78cc-eeee-46f8-8c36-2a4ae994b9e2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b585b5bd-e074-472f-8b67-6ba949159463")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f4e8b422-e306-4a36-99aa-b47c38286e42")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2e016a11-b790-4e04-a179-c2714ca21cea")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/89490f73-b581-46e2-b970-21cf8c592966")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 0 0.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "0efee137-8d8c-4601-86ab-84696d7fdf6d")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "0c61a161-d679-4b1e-987c-870a2e110d1a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
			(uuid "fc1996f0-9d96-4bfd-875d-e0fd97d2c65c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1 1)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "X_Ua_CTRL")
			(pinfunction "1")
			(pintype "passive")
			(uuid "9c83032b-262f-48bf-be22-29069c1d8ccf")
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(uuid "b99d2fcd-2848-4876-8148-fa2c6eb1b33c")
		(at 53.9 50.862499 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 0 1.6 90)
			(layer "F.SilkS")
			(uuid "4cc00cc1-f3ba-4257-80b5-4108b0bd3483")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100p"
			(at 0 1.679999 90)
			(layer "F.Fab")
			(uuid "b9388073-583f-4e2f-87a7-227e31caedeb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c64176be-5c62-477d-844a-c52f28cdb45a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8493cda2-48f5-4909-8274-ce5032919956")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9e71015b-dd8b-4674-9ec5-1b948c17e702")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "873b0369-4eb2-4f3c-88bc-10cb6712e510")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/fb59875b-7a80-46e0-97d3-d7cad3391c0d")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eca90473-7d3b-41d0-a6a3-0091fde9f61b")
		)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "61f54c01-5677-495e-9888-2fea7dfdf2e4")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5f8b5322-1eef-400f-bf98-566ff42de962")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5144e2aa-14f0-47b1-b1bb-195340a83267")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c4349f8b-40eb-4d0a-a564-c0d511ebd529")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fd481b52-a642-497d-b917-6fff8b2585ed")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "07d2ee7a-15ff-4ac0-9ca8-ea7b4840184b")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a792e35d-907c-4dfe-a90e-02a9e2d9ceb5")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e934c308-c45b-4d44-92a8-c9759f9f2e98")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aefcbb47-f7cc-4d7f-9d6d-44d82ab15f0e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "8827a828-00fd-4663-afa3-aaea07009a22")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "OVERLOAD")
			(pintype "passive")
			(uuid "08da791b-87b7-43f2-b418-585f0225527e")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "1fd9572b-1b23-4368-b098-69ddcf28961c")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "ba02693a-6f7b-4386-bd69-a94c545ef00d")
		(at 47.4 41.7 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at 0 2.499997 0)
			(layer "F.SilkS")
			(uuid "e3630173-132c-4730-b023-31ee54e0df74")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "150"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "871422f3-ba1e-4fdf-b0dc-cb2bf178553f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ff7e2850-1a1b-4212-8d07-11fbf0721ab3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ca448a44-b450-4c5b-9214-39bd4662ff46")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2b1067f3-8fa6-4f14-8b03-d09d0490c026")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/14414bd4-d0a2-4eee-b9e3-f7231051f202")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c1988243-bedf-4d13-a336-327f3c5ca542")
		)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "45adc87a-74df-40a8-804a-89a764ee8cdf")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a7649bfc-1262-4def-b107-ec45f19cbb26")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ac939f10-c275-40db-8d43-e44565d7cd61")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dd1445af-b2fe-412b-b7de-4385ec68ee47")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "40368818-dd47-47ce-9013-0191056173df")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c804328e-3753-4f9a-b359-bd35e6565b30")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b183f50b-ced3-44f4-ada6-4be686967d50")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d2e7afb3-be73-46e4-a6cb-732b828809f3")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f748ab8b-6eea-4a22-b04b-415e2235b875")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f58964b9-e90e-4c66-a473-1312233b11ee")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 29 "Ia_CTRL")
			(pintype "passive")
			(uuid "71023a94-1fc3-45a6-8c94-9309b033b6f3")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 16 "Net-(D6A-+)")
			(pintype "passive")
			(uuid "71422e4c-c07b-40e3-8125-d4c2c1f722f4")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(uuid "c5579b37-7a4e-4326-a3c6-8922ade9b186")
		(at 61.9 50.862499 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 1.6 -1 90)
			(layer "F.SilkS")
			(uuid "592d3617-8c95-4801-b15e-b807bbe7233b")
			(effects
				(font
					(size 0.9 0.9)
					(thickness 0.15)
				)
				(justify right)
			)
		)
		(property "Value" "100p"
			(at 0 1.679999 90)
			(layer "F.Fab")
			(uuid "aa51fef4-30b1-4f96-bcaf-20fe0e4a00c6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d08ee4ea-9c39-4bd0-b188-39abecb93b80")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "49b188e9-339b-4e1c-aa22-b42fdee61242")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "35b38401-9d93-4fa6-8837-f58e9eecacca")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d2f3163d-40fe-4964-a4cf-044171f0322b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/44d19cd9-c079-48ea-aadb-6ed31261528d")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8b6afaaf-d5e3-4126-b154-ef932e73682b")
		)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0ba2a3b7-aeba-471d-9301-02abbe6b9442")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "23ae58b7-c42e-453f-bc3d-c7679396ed75")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "788a0ba5-f36f-44b2-8461-54f985913b2f")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bc9a3afd-c788-4419-96e4-7540cba0bc7d")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "20699bcd-a1b3-4f21-8610-78bacdca2343")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cc353809-bb8a-4023-b86f-b06257f8a414")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "270f3741-e1db-446f-94f5-0ed2fb687051")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c67115d0-3508-4f6c-b3fe-e0aa1d3d7013")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "48576e64-b1f8-453f-a081-fb481780b682")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "7582276a-5a0b-4a2f-915b-dad9e305577e")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "NO_LINK")
			(pintype "passive")
			(uuid "51434290-537f-4453-9ecb-abcb8288df4b")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "80ff5602-f6a6-4b02-b78b-c1f7f8bbf09a")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(uuid "c6d637de-d0eb-46b0-ae3e-e4e1ca6203de")
		(at 69.9 50.862499 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 1.6 -0.1 90)
			(layer "F.SilkS")
			(uuid "dac98f29-1b54-4005-b84e-0ba0a609795b")
			(effects
				(font
					(size 0.9 0.9)
					(thickness 0.15)
				)
				(justify right)
			)
		)
		(property "Value" "100p"
			(at 0 1.679999 90)
			(layer "F.Fab")
			(uuid "31776602-8d96-4034-a36c-a40608f9fbeb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e4703c60-afd8-41fe-be54-46050123bc6a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0fcf710d-02fe-4434-94fe-83abfed7af5f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "57f7fea7-04c2-4641-a88b-c7449d99e96c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fa9bbabe-c68f-40f5-8bc6-7dac9b0db947")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/feed856d-da6d-4103-a8db-551ab45767af")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8e39b68e-6d16-4111-b23b-5f0150dedb91")
		)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "98c3b3c2-d3c2-474f-bc67-291b96a704ce")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e5bef952-1d96-4d25-8a72-1dd98b1678be")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cf0815c1-94e3-470d-8059-24c19ce20e86")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5f149be7-0768-429b-8b3c-2f043b9111f3")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "48aea80a-7048-42d8-85b4-3e8cee3549a8")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c71cd319-3108-44ec-84c9-28796e8da8ac")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c9e827fe-5abf-4f63-b06c-7f9cf74b7a2f")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b4c963d7-7a27-4ae4-b2fa-c6a51694c41c")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2ae36ba8-d424-44ee-a46b-ec66f7d954ca")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "0fdbcddc-0e9d-47ea-81e4-b91677bc16ba")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "UA_RDY")
			(pintype "passive")
			(uuid "cebe40c1-38c2-44de-be58-9e393f8a8bd7")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "0be960eb-6611-4be1-bb71-e21eb6d0ffc3")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "d1da5a88-0995-436d-b870-a8d4008fb0c0")
		(at 59.9 50.862499 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at -1.5 0.1 90)
			(layer "F.SilkS")
			(uuid "46aa98da-da3d-4c63-af64-10d4c8bc3590")
			(effects
				(font
					(size 0.9 0.7)
					(thickness 0.15)
				)
				(justify right)
			)
		)
		(property "Value" "1k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "0ecdb236-3968-4dfb-8d62-e205665e065a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "06c17920-b1b2-49d3-b338-6b798e486b04")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "35c128f6-f962-4ae6-b9de-4b12acf0ee5d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8acdca37-d23b-4a76-a081-3e07e4209ae0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/43d426c3-9384-4828-804b-7a835f6678fb")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "83005153-9aa4-4eff-b1e0-4dd93b3cf37a")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "93f72f28-cd92-4fa7-867a-1833e67d504c")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d8a81c44-6e65-430c-bbef-e20b07293b4e")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "70bee74e-20cc-465e-8163-aba48be77fd7")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "06d4801e-48d4-4fd9-a747-d74b79bb995b")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "46e1aac7-7fcc-46a2-876c-93753f0d09f1")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "07b356f4-9a15-4a63-96df-880690776756")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "77a2764f-d3a3-4087-9989-56382e1c49dc")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "74fd6f7b-213d-4808-bc35-7abd5474476f")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "476502b3-3095-453b-887a-d88b00e4324c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "4f3e39f3-c0aa-4750-9d33-a7e27897a921")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 81 "/X_OVERHEAT")
			(pintype "passive")
			(uuid "d34934ac-685d-472e-965e-dc9b26a06df4")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 11 "OVERHEAT")
			(pintype "passive")
			(uuid "b1217377-7cfe-464e-a5a2-35727a5084e8")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "d90ccba6-6ad9-4ec2-a12c-2f628508fdf6")
		(at 36 56.6 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at -1.1 -1.7 90)
			(layer "F.SilkS")
			(uuid "bf00806c-be78-4057-9f6f-0c14190a4128")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "150"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "b9b6991b-58eb-4ca1-bbc1-e91a6b0645ae")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "071c0ec1-4d29-4fa2-9fc6-bd495be8a9c6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4c96c6f0-5f78-4852-bce4-04033d443cf3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "30e0c58e-277a-4d6e-accf-2af329941517")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/7efcb0cb-5195-485c-af8a-ec3314f6d4ac")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fa732d88-09c5-41f9-8cf9-e3e42ee44466")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6e81bc08-44bf-4ea6-8bfd-4a607b4e6c8f")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cc6a8ad6-e3e5-4f41-b7fc-9317ee92f6d6")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a2bb1b62-b56e-413d-acae-a08a8faed255")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "99061d1e-ee8b-44c8-910e-2a30bea0efd1")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c6f8e7c3-8f69-4dc5-9c83-08d8a03af205")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "78776c71-e3ff-498b-b4b6-47c138140461")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "edc77644-3b73-40db-b453-7a75b2672c3a")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eaca6e4d-43f0-46fc-91c2-1b96d8a8bfca")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ad8748d9-5525-4f65-a02c-ac3a78d20a0e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "2cf7c539-f09e-48fe-a81f-44ac19d7ed22")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 82 "X_Ua_MON")
			(pintype "passive")
			(uuid "a37c1281-0c21-471e-9576-c5a5b6570157")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 14 "Net-(D5A-+)")
			(pintype "passive")
			(uuid "ce71540d-5b9e-48a6-be59-e8657f36cbae")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm"
		(layer "F.Cu")
		(uuid "db4a3f61-36ea-49ef-8809-ecd4daa79003")
		(at 33.4 40.350001 180)
		(descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
		(tags "test point THT pad")
		(property "Reference" "TP13"
			(at 0 -1.448001 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "febaed87-d7ff-4e1e-abd3-4712c10947bc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 1.550001 0)
			(layer "F.Fab")
			(uuid "b2c9ec1d-25f5-4b7f-acee-5154acd77fb6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6d866e43-1b46-4b48-8518-8045f05d4fda")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "acad9c65-2d1e-4e46-9848-0c773f61c49c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "26fe3773-fcbe-40ee-bbbf-d6432fb62347")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/ff4b4291-57ab-4613-9c23-3469d29f7ce2")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 0 0.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "85ea5c94-f2d2-4232-9fa6-b8cd2246f28f")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "dc7fcb4f-b3b2-4482-b1b4-251e93d21b0d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
			(uuid "209cb79b-a531-400d-abb9-f5320d18eaeb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1 1)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Ua_CTRL")
			(pinfunction "1")
			(pintype "passive")
			(uuid "51c511c8-7aa2-49a6-952f-5b38daeef0cf")
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(uuid "e08a4773-de34-4255-93cb-69bccb751e58")
		(at 111.8 40.8)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "D2"
			(at 0 -3.4 0)
			(layer "F.SilkS")
			(uuid "765c52dc-9df6-41bb-a23c-0b43f23801fa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SP3078E"
			(at 0 3.4 0)
			(layer "F.Fab")
			(uuid "339095b4-bfe8-4a3a-9c7d-7f59a7f1d283")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e26a9fd2-66a5-452c-837c-dda72cb7e749")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e94ca9bb-f8af-4e63-a0df-3f90636fde84")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4e1014a0-0196-4028-b950-ca2fa1a7d7bc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/8024375843"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d11fac16-f6f0-4ed9-a6a6-82163aad679f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*")
		(path "/ff5a735d-a89d-4bc7-bb99-e72bcabfa5e3")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -2.56)
			(end -1.95 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1327aac8-f20a-406c-962f-34233e204300")
		)
		(fp_line
			(start 0 -2.56)
			(end 1.95 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "62d1d8e5-31c7-4e5c-a280-c5e0c2014239")
		)
		(fp_line
			(start 0 2.56)
			(end -1.95 2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "59df895d-c05b-4cf1-aa5b-63b57af32afc")
		)
		(fp_line
			(start 0 2.56)
			(end 1.95 2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "85a0cb9e-3be1-4966-976a-5dd75d8f1c4e")
		)
		(fp_poly
			(pts
				(xy -2.7 -2.465) (xy -2.94 -2.795) (xy -2.46 -2.795) (xy -2.7 -2.465)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "4beaa7e5-f842-4107-bbf1-5fb56f0beb43")
		)
		(fp_line
			(start -3.7 -2.7)
			(end -3.7 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a76c0db9-917f-4482-9962-cbd8c4f441f6")
		)
		(fp_line
			(start -3.7 2.7)
			(end 3.7 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "080080ae-9783-488d-baab-e68070b7e798")
		)
		(fp_line
			(start 3.7 -2.7)
			(end -3.7 -2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1fa5243d-e040-461c-89c2-19dff709c1cf")
		)
		(fp_line
			(start 3.7 2.7)
			(end 3.7 -2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b773d4b1-a1a9-4d66-87a4-c1ee5f2d321b")
		)
		(fp_line
			(start -1.95 -1.475)
			(end -0.975 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4dd14286-dbc8-41ab-bd04-c42d3ff966f2")
		)
		(fp_line
			(start -1.95 2.45)
			(end -1.95 -1.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "83b3934a-7887-4c5c-8629-86179620bb21")
		)
		(fp_line
			(start -0.975 -2.45)
			(end 1.95 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "60a97d4a-ae46-4f1a-a01d-62018d071916")
		)
		(fp_line
			(start 1.95 -2.45)
			(end 1.95 2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e5d7c2ac-c502-4b9d-88f0-03576c2d7f25")
		)
		(fp_line
			(start 1.95 2.45)
			(end -1.95 2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fe21a121-fac5-4986-a57a-791fbb4307d7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e86b185b-3a5c-4496-826f-b6cddde27378")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "U1_RX")
			(pinfunction "RO")
			(pintype "output")
			(uuid "2d682ebd-64bc-42da-877c-e060ad28c6e1")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "TXEN")
			(pinfunction "~{RE}")
			(pintype "input")
			(uuid "fc9d9c35-c2d6-4cf6-80e1-f2f523326b95")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "TXEN")
			(pinfunction "DE")
			(pintype "input")
			(uuid "384c13c0-2afa-43a0-b6de-305f358be963")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "U1_TX")
			(pinfunction "DI")
			(pintype "input")
			(uuid "71c59912-3c6e-4527-af47-da7f4d5e07f1")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "1f2b375d-b233-437a-ac67-108c5248caf4")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "bidirectional")
			(uuid "484d94a3-b697-4ff0-845e-027494c817a1")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(D2-B)")
			(pinfunction "B")
			(pintype "bidirectional")
			(uuid "0ec5b801-bb38-420a-b14b-f86eac456dc6")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "c16f1a11-42e1-44af-9d55-4fc617c38c35")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "e0e3b06d-82be-4204-a35f-221b0c596c12")
		(at 45.6 57.8 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at -3.1 0 90)
			(layer "F.SilkS")
			(uuid "e800a310-7119-47bc-b394-8bed16eb25b4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "150"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "fd898fcd-2033-4fa9-89a8-2618ec614cfe")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "68568fd9-8eaf-4631-b79d-8a9e9da532e0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0b7e1ff3-6ec8-400c-b125-d66ad3cace9f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9189e6f2-d1b1-4519-b576-99bc1f3b0c7e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1dc64f8f-8bb9-4269-9551-8f74074a2c88")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5eec470a-88f4-475f-a986-6c72d05c1a39")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e442efd4-a9e5-4886-a568-c7e2a79adffb")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8fa5ff15-ab4f-4a22-9906-329a73ca7980")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "55fa7c61-0140-45e8-8e08-05c5318d0b37")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eec59697-f7d9-4386-814e-6350abcf3ff7")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "135553f1-e23a-4294-b689-2d22e08d84b8")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "20ac1727-6ea3-4ec5-b2bb-03084deafe7f")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb75ca4a-d581-42ae-944a-3ec75406bb6c")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "41028b69-e6b0-408d-b417-f9e52305cb7c")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "629735af-e343-49ad-bd75-b5d5834d5868")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "1be4eae1-321d-4175-8ecd-e50fa33e7d62")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 83 "X_Ia_MON")
			(pintype "passive")
			(uuid "0b202863-b3cd-40ab-a506-66b2badab1b2")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 15 "Net-(D5B-+)")
			(pintype "passive")
			(uuid "0f34b778-68fc-403f-9402-4176820534ae")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "e8438922-22b3-46db-8828-b368df414f6c")
		(at 47.4 39.750001 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R32"
			(at 0 1.700001 0)
			(layer "F.SilkS")
			(uuid "93629159-96be-48f3-8693-99a1885431e2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "cc08487a-ddbe-41f0-8e33-eede592e4d39")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1f35dc27-16d2-4633-8488-afaef52b47b8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4ef88fc6-b28d-4b67-b31a-82e76d9839dd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e677db9a-3d34-4331-91fc-ef034b7c8524")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/06be4eaf-7779-4243-b8dd-2cb3dcbd3866")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "afc51fac-1df4-4573-9a79-1c89ea5915e8")
		)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d77c7716-1535-49b1-918b-6a4ede28e5f2")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d11c8665-2591-49dd-94b5-7e1cb5ba50f6")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2f4eb3d4-46f2-48f7-aeca-cd5f932f3753")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0571eda1-be89-4bbe-9c9d-ebbf0c3478d4")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7c9a21a0-3ef6-4b9b-9927-8f6eda981c3f")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a3d74f80-bf35-4683-ad27-6b2515bd88d7")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4369802d-2ff6-4b6c-8548-2ec6ffb39d16")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "30515df2-4be7-4471-9c3e-c067c553211a")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b6a16efc-e078-441f-b30b-ec93dd7da4ce")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "211cca0e-0991-4390-b567-cccf2ef553e1")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 29 "Ia_CTRL")
			(pintype "passive")
			(uuid "aea8a002-c3ea-4ad8-84bd-ebaa5fc38432")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 4 "GND")
			(pintype "passive")
			(uuid "b21f1109-e62f-41f8-8577-bbba8cb0dfbe")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "e91821db-26dc-4e1b-b033-ae6edc08fdcc")
		(at 36.1 40.6)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 0 -2.55 0)
			(layer "F.SilkS")
			(uuid "6321355f-6eae-41e8-8045-5418fc083518")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "150"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "35ba4a0a-4589-4b23-ad1d-8ffcbdfbe001")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1ac63464-50c3-4757-b3ab-36ac05d4c880")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9717842a-107d-4c08-9223-149c52c18dd1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e4094bf1-a50d-4ba1-9e62-e8b9331ec074")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/4a3bb054-ea39-4a83-a985-23ae80d65373")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f1beea28-d655-4960-991d-863bda5f8a13")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "feacbfcd-82da-4821-92fd-3989724e7819")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a445b802-3a35-4249-8a0a-a38702181fb6")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e6eb3e4b-b31e-4b37-8d37-bd99deb5eaa5")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "647433b8-6e56-4974-b3b4-fed979d30d53")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7edaff4d-cd7a-4862-9fb8-1f4557aa6fdd")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bd7c2e22-2e08-4fb7-b6a2-eedbc4f5cb04")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4a61d66d-f471-4d90-989c-4c40368806d8")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9414b266-2754-45e4-a75a-96976770ece5")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "895566d9-a2ae-44af-93d1-9205b6140959")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c859638f-b15d-4fd6-a621-8ba2d4f62f52")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 51 "Ua_CTRL")
			(pintype "passive")
			(uuid "56a4ab78-ecb8-47bc-a5eb-c573cb584b3b")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 17 "Net-(D6B-+)")
			(pintype "passive")
			(uuid "9b319124-91ca-4c1b-ae68-52d2216d80cf")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "eb0cc512-7bc2-4783-b6f0-6278ec7b2bb1")
		(at 92.3 40.5 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "VD13"
			(at 0.02265 2.289849 90)
			(layer "F.SilkS")
			(uuid "f9471f65-b513-432e-b2d3-3d53c69e6a45")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BAT54S"
			(at 0 2.4 90)
			(layer "F.Fab")
			(uuid "fdd56bd9-1aa2-4d03-9baa-8992bfd82e89")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8e8c65a5-2e33-48cc-88ca-146f201b6b2e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds11005.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "be340668-5542-47bf-9d32-d0b785157c6d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "dual schottky barrier diode, in series"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "23930372-29fa-4c56-9492-1f15953605fb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Link" "https://www.chipdip.ru/product/bat54s-nxp"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "05d9f261-d331-4d70-9b61-505c5e831edd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/30f45cc8-e449-41fd-a090-7c6a6f125c69")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.560001)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2f70f162-bdec-494f-8649-9529b284a909")
		)
		(fp_line
			(start 0 -1.560001)
			(end -0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "21fa1494-7224-463c-b267-fa9efe78baff")
		)
		(fp_line
			(start 0 1.560001)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5d1d5a0a-d0fa-4e50-aa33-eda72ddfd349")
		)
		(fp_line
			(start 0 1.560001)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d3ce63ad-831c-41aa-abec-b515ff4d3999")
		)
		(fp_poly
			(pts
				(xy -1.1625 -1.51) (xy -1.4025 -1.84) (xy -0.9225 -1.839999) (xy -1.1625 -1.51)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "a4cfa87a-b0fd-4905-b993-8ca5c24081a1")
		)
		(fp_line
			(start 1.92 -1.700001)
			(end -1.92 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6ad280e4-16da-48d0-8ea6-a3259266653b")
		)
		(fp_line
			(start -1.92 -1.700001)
			(end -1.92 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f5f4a0f6-8640-4839-bce7-bb42cfbe9fa0")
		)
		(fp_line
			(start 1.92 1.700001)
			(end 1.92 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "639b15f8-b0cd-488d-b2f9-bd4baa7378e8")
		)
		(fp_line
			(start -1.92 1.700001)
			(end 1.92 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a7554ced-7cbc-495e-92db-30d4d85fd2d8")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a3aaca2c-7abb-43e5-81b4-52b79f8e36fc")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "80a43232-0ad5-441c-a98d-7feb166a4f42")
		)
		(fp_line
			(start -0.65 -1.125001)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "caeabd98-418a-4f9f-922f-ac3532235a59")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "173703fc-c12a-40f0-b461-40c67f071b81")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5c22d5d6-d8c2-40a8-8d29-f06c2b26749b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "1e70e90e-a553-49f2-aa55-bc13c3c8e783")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "2cf77a65-5881-46ee-b7c8-93ab4b69a143")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pintype "passive")
			(uuid "2707f4fd-5c60-451f-bce4-a050e6db5758")
		)
		(pad "3" smd roundrect
			(at 0.937501 0 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "HV_24V")
			(pintype "passive")
			(uuid "8845cfe2-9418-4019-abe8-6ab764d75479")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Ecohim:Ecohim-logo_5x6mm"
		(layer "F.Cu")
		(uuid "ed4a59e1-bea0-44e1-998f-070585492812")
		(at 101.2 67)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "048664d5-9447-4ce3-9f1c-81288ba16a1e")
			(effects
				(font
					(size 1.5 1.5)
					(thickness 0.3)
				)
			)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "4c436f04-ceeb-4938-aad5-daa9ad930a74")
			(effects
				(font
					(size 1.5 1.5)
					(thickness 0.3)
				)
			)
		)
		(property "Footprint" "Ecohim:Ecohim-logo_5x6mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "44a797c5-a8ef-4375-a38f-d03945878ba9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7f6581ad-4655-4684-aae8-110dc7bde74a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1af86709-07f6-49a8-bdab-3b133fe8b1b1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(fp_poly
			(pts
				(xy 0.740019 -0.852416) (xy 0.825569 -0.799204) (xy 0.895688 -0.752191) (xy 1.012886 -0.654401)
				(xy 1.112393 -0.541313) (xy 1.176424 -0.435434) (xy 1.190625 -0.379002) (xy 1.154417 -0.367892)
				(xy 1.059683 -0.360034) (xy 0.932656 -0.357187) (xy 0.674688 -0.357187) (xy 0.674688 -0.615156)
				(xy 0.677862 -0.746543) (xy 0.686166 -0.839459) (xy 0.697302 -0.873125)
			)
			(stroke
				(width 0)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "fa721d54-6063-4ee8-96aa-17e75d51bb9c")
		)
		(fp_poly
			(pts
				(xy -0.475161 0.042577) (xy -0.328779 0.050432) (xy -0.231364 0.062031) (xy -0.198437 0.075264)
				(xy -0.225903 0.120459) (xy -0.295503 0.194326) (xy -0.338725 0.234014) (xy -0.455549 0.318477)
				(xy -0.571367 0.352442) (xy -0.646303 0.355599) (xy -0.781825 0.340255) (xy -0.903029 0.304405)
				(xy -0.921737 0.295323) (xy -1.017722 0.221977) (xy -1.088731 0.130845) (xy -1.11125 0.06214) (xy -1.074176 0.053301)
				(xy -0.973399 0.046099) (xy -0.824585 0.041307) (xy -0.654844 0.039688)
			)
			(stroke
				(width 0)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "4d0a9a90-bcae-4400-aebb-45ff13197cce")
		)
		(fp_poly
			(pts
				(xy -1.06376 1.23419) (xy 0.000386 2.321719) (xy 1.050055 1.250156) (xy 2.099725 0.178594) (xy 2.267142 0.344738)
				(xy 2.434558 0.510882) (xy 1.211995 1.763566) (xy 0.957467 2.024232) (xy 0.720618 2.266537) (xy 0.507067 2.484752)
				(xy 0.322434 2.673147) (xy 0.172337 2.825989) (xy 0.062396 2.937551) (xy -0.001768 3.0021) (xy -0.016462 3.01625)
				(xy -0.044459 2.988843) (xy -0.121369 2.910952) (xy -0.240845 2.789073) (xy -0.396539 2.629702)
				(xy -0.582103 2.439335) (xy -0.791189 2.224468) (xy -0.976292 2.033984) (xy -1.213824 1.789085)
				(xy -1.444982 1.550175) (xy -1.661043 1.326311) (xy -1.853288 1.126549) (xy -2.012996 0.959945)
				(xy -2.131447 0.835554) (xy -2.180256 0.783697) (xy -2.430284 0.515675) (xy -2.279095 0.331168)
				(xy -2.127905 0.146662)
			)
			(stroke
				(width 0)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "edd140d8-67dc-4d71-98b7-339f05821a91")
		)
		(fp_poly
			(pts
				(xy 0.783852 -2.172932) (xy 1.018357 -1.932083) (xy 1.263435 -1.680495) (xy 1.505202 -1.432413)
				(xy 1.729772 -1.202082) (xy 1.923259 -1.00375) (xy 2.039288 -0.884912) (xy 2.512402 -0.400605) (xy 1.270586 0.87126)
				(xy 1.013258 1.134194) (xy 0.772723 1.378776) (xy 0.554673 1.599302) (xy 0.3648 1.790073) (xy 0.208796 1.945385)
				(xy 0.092354 2.059538) (xy 0.021166 2.126831) (xy 0.000792 2.143125) (xy -0.031861 2.115613) (xy -0.114139 2.036876)
				(xy -0.240349 1.912614) (xy -0.404801 1.748527) (xy -0.601801 1.550315) (xy -0.825657 1.323677)
				(xy -1.070678 1.074315) (xy -1.269571 0.871034) (xy -1.425801 0.711068) (xy -0.833437 0.711068)
				(xy -0.82181 0.816561) (xy -0.792736 0.881739) (xy -0.783828 0.888063) (xy -0.691523 0.900059) (xy -0.553161 0.887017)
				(xy -0.396235 0.85374) (xy -0.248241 0.805032) (xy -0.208465 0.787545) (xy -0.026552 0.665991) (xy 0.138627 0.492829)
				(xy 0.262735 0.295465) (xy 0.293006 0.222831) (xy 0.318521 0.153541) (xy 0.335287 0.123702) (xy 0.345294 0.141904)
				(xy 0.350535 0.216739) (xy 0.353001 0.356799) (xy 0.354054 0.486172) (xy 0.357188 0.912813) (xy 0.515938 0.912813)
				(xy 0.674688 0.912813) (xy 0.674688 0.47625) (xy 0.674688 0.039688) (xy 1.11125 0.039688) (xy 1.30823 0.036238)
				(xy 1.452378 0.026502) (xy 1.533552 0.011404) (xy 1.547813 0) (xy 1.508984 -0.014904) (xy 1.395824 -0.02655)
				(xy 1.21332 -0.034674) (xy 0.966456 -0.039011) (xy 0.798565 -0.039687) (xy 0.049317 -0.039687) (xy -0.002184 0.084648)
				(xy -0.127156 0.300139) (xy -0.294529 0.452999) (xy -0.497709 0.538454) (xy -0.652873 0.555625)
				(xy -0.833437 0.555625) (xy -0.833437 0.711068) (xy -1.425801 0.711068) (xy -2.072296 0.049115)
				(xy -1.222541 0.049115) (xy -1.195833 0.113043) (xy -1.149969 0.190823) (xy -1.017911 0.337148)
				(xy -0.845862 0.424827) (xy -0.650795 0.450494) (xy -0.449683 0.410779) (xy -0.331647 0.35323) (xy -0.245038 0.27742)
				(xy -0.160763 0.169307) (xy -0.09903 0.058461) (xy -0.079375 -0.01592) (xy -0.116735 -0.024323)
				(xy -0.219515 -0.031422) (xy -0.37376 -0.036639) (xy -0.565519 -0.0394) (xy -0.654844 -0.039687)
				(xy -0.891541 -0.038897) (xy -1.057761 -0.033764) (xy -1.162403 -0.020146) (xy -1.214363 0.006099)
				(xy -1.222541 0.049115) (xy -2.072296 0.049115) (xy -2.275307 -0.15875) (xy -1.27 -0.15875) (xy -1.230669 -0.147104)
				(xy -1.114058 -0.137393) (xy -0.922241 -0.129677) (xy -0.65729 -0.124014) (xy -0.321278 -0.120462)
				(xy 0.083721 -0.11908) (xy 0.138906 -0.119062) (xy 0.552355 -0.12017) (xy 0.897074 -0.123455) (xy 1.170991 -0.128859)
				(xy 1.372033 -0.136322) (xy 1.498126 -0.145787) (xy 1.547197 -0.157195) (xy 1.547813 -0.15875) (xy 1.508482 -0.170396)
				(xy 1.391871 -0.180107) (xy 1.200054 -0.187823) (xy 0.935103 -0.193486) (xy 0.599091 -0.197038)
				(xy 0.194091 -0.19842) (xy 0.138906 -0.198437) (xy -0.274542 -0.19733) (xy -0.619262 -0.194045)
				(xy -0.893179 -0.188641) (xy -1.09422 -0.181178) (xy -1.220313 -0.171713) (xy -1.269385 -0.160305)
				(xy -1.27 -0.15875) (xy -2.275307 -0.15875) (xy -2.43035 -0.3175) (xy -1.230312 -0.3175) (xy -1.190989 -0.305788)
				(xy -1.074426 -0.296035) (xy -0.882738 -0.288301) (xy -0.618039 -0.282648) (xy -0.282441 -0.279134)
				(xy 0.121941 -0.277821) (xy 0.159506 -0.277812) (xy 1.549325 -0.277812) (xy 1.523093 -0.386953)
				(xy 1.449115 -0.597833) (xy 1.3286 -0.787245) (xy 1.150317 -0.970064) (xy 0.980238 -1.105694) (xy 0.820168 -1.23923)
				(xy 0.723798 -1.362458) (xy 0.680171 -1.492034) (xy 0.674688 -1.57024) (xy 0.665593 -1.63257) (xy 0.623503 -1.660268)
				(xy 0.526207 -1.666855) (xy 0.515938 -1.666875) (xy 0.357188 -1.666875) (xy 0.3568 -1.021953) (xy 0.356412 -0.377031)
				(xy 0.262368 -0.575469) (xy 0.188783 -0.715593) (xy 0.107519 -0.829775) (xy 0.000754 -0.937835)
				(xy -0.149335 -1.059596) (xy -0.221527 -1.113648) (xy -0.379487 -1.247374) (xy -0.472887 -1.373375)
				(xy -0.512625 -1.508554) (xy -0.515937 -1.57024) (xy -0.525032 -1.63257) (xy -0.567122 -1.660268)
				(xy -0.664418 -1.666855) (xy -0.674687 -1.666875) (xy -0.833437 -1.666875) (xy -0.833437 -1.485672)
				(xy -0.813907 -1.30581) (xy -0.749057 -1.151) (xy -0.629494 -1.007637) (xy -0.445828 -0.862116)
				(xy -0.366645 -0.80943) (xy -0.235445 -0.709453) (xy -0.119588 -0.593855) (xy -0.035693 -0.481794)
				(xy -0.000377 -0.392424) (xy -0.000148 -0.386953) (xy -0.037532 -0.376753) (xy -0.140795 -0.368059)
				(xy -0.296447 -0.361524) (xy -0.490999 -0.357801) (xy -0.615156 -0.357187) (xy -0.86302 -0.354699)
				(xy -1.052273 -0.347514) (xy -1.176418 -0.33605) (xy -1.22896 -0.320727) (xy -1.230312 -0.3175)
				(xy -2.43035 -0.3175) (xy -2.511955 -0.401056) (xy -2.430102 -0.484896) (xy -1.164823 -0.484896)
				(xy -1.160333 -0.462224) (xy -1.124735 -0.44805) (xy -1.046433 -0.440379) (xy -0.913832 -0.437216)
				(xy -0.715335 -0.436566) (xy -0.676084 -0.436562) (xy -0.483881 -0.438884) (xy -0.32403 -0.445238)
				(xy -0.211246 -0.454706) (xy -0.160243 -0.466371) (xy -0.15875 -0.468825) (xy -0.184999 -0.514126)
				(xy -0.250617 -0.588249) (xy -0.277772 -0.615118) (xy -0.422922 -0.706853) (xy -0.598469 -0.748429)
				(xy -0.782847 -0.742247) (xy -0.954493 -0.690707) (xy -1.091841 -0.596208) (xy -1.149801 -0.518061)
				(xy -1.164823 -0.484896) (xy -2.430102 -0.484896) (xy -2.039349 -0.885137) (xy -1.878367 -1.050048)
				(xy -1.675829 -1.257563) (xy -1.445604 -1.493468) (xy -1.201564 -1.743551) (xy -0.957579 -1.993597)
				(xy -0.782606 -2.172932) (xy 0.00153 -2.976643)
			)
			(stroke
				(width 0)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "dbb0d802-19e8-461f-9aec-5965e66a4fc9")
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(uuid "edf6c644-c464-478c-a151-e1b117b7873a")
		(at 36 53.1 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R24"
			(at 0.1 -2.4 90)
			(layer "F.SilkS")
			(uuid "a09acd6c-b801-4803-8eaa-ed6d82794afb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(uuid "3f2374b0-3554-44c0-baa5-b01e8123ae7a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e8469bc0-f846-4f76-babc-d3f3df0b96db")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ef6c2e2d-1d24-4a11-9efe-02fbc53897b9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c820e002-806f-4351-b4cd-6fe49a9c4293")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/6107d97a-f6b0-448a-925a-8045d6cf4e97")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "556735dc-3323-42c3-a37d-c796fa9e45a7")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a814aaf7-5b6a-4cb9-878c-d72d03f5fada")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e32b413d-7cbc-4beb-8a81-5df85b5d6157")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "123d0fee-ce1d-4a23-a38f-0d9d56c389a4")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "72670e1c-25b8-4dc6-924b-6d201a85f002")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "43d21e60-4f7a-49c2-bc49-e74fbddcb9d2")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "448d620d-6994-4a79-bb10-250e99c5af45")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f7a64ebb-ef1c-4a0f-9738-db63acfb14a8")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "18d97a9b-4427-4d3e-ba17-88df9c83c3e8")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dad7bb96-f386-4cb4-b793-163c2023bf0d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "57277b75-366e-41bc-b3fb-4740792c5263")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 65 "Net-(D5A--)")
			(pintype "passive")
			(uuid "fef155e2-0c60-4aca-83cc-6898f505541b")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 43 "Ua_MON")
			(pintype "passive")
			(uuid "178d3d2a-ce45-4b85-99da-4a02b24bf9ee")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "efacf996-a5a3-461b-8939-3d0fcb677f7d")
		(at 48.4 54.3 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "VD12"
			(at -0.7 2.2 90)
			(layer "F.SilkS")
			(uuid "4f1887df-38bd-48b2-ba2f-0f11dc7bfa02")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BAT54S"
			(at 0 2.4 90)
			(layer "F.Fab")
			(uuid "298848e4-3833-4e83-9c37-649b2d02d258")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b651a8e7-f6b8-4ac2-84ef-ad0623c80fd6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds11005.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "97baf0b2-da71-49ec-98e7-e98966cb8f5b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "dual schottky barrier diode, in series"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c40c0f66-a36d-4f04-b7a9-285881b8ed97")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Link" "https://www.chipdip.ru/product/bat54s-nxp"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "560525cb-71c8-4bf2-af47-a6eb2cd99e4b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/3cb3cd7a-78a2-41be-9d09-f0b24f4d9b69")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.560001)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f207f600-9350-4c67-b74c-d9b4cd8fd9c1")
		)
		(fp_line
			(start 0 -1.560001)
			(end -0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8d5da655-f811-4dde-b3ff-5762ffaa4708")
		)
		(fp_line
			(start 0 1.560001)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7928f973-594b-4d48-9752-4945103ec16b")
		)
		(fp_line
			(start 0 1.560001)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7384d57d-3b6e-4b40-9ef8-4a5248533019")
		)
		(fp_poly
			(pts
				(xy -1.1625 -1.51) (xy -1.4025 -1.84) (xy -0.9225 -1.839999) (xy -1.1625 -1.51)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "ffad503c-04e9-47a6-9a0c-eae4c08ad407")
		)
		(fp_line
			(start 1.92 -1.700001)
			(end -1.92 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bd5ea762-7b91-41ea-aae3-ea2d096a3687")
		)
		(fp_line
			(start -1.92 -1.700001)
			(end -1.92 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3ef2f996-2c0a-44e3-9d97-b95dc5d65a1d")
		)
		(fp_line
			(start 1.92 1.700001)
			(end 1.92 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8c8cc956-0412-4fc1-8835-3e20cc86619b")
		)
		(fp_line
			(start -1.92 1.700001)
			(end 1.92 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4b36cef7-4707-4556-b4eb-07198af33976")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5a8f51c7-358e-4ba0-84a3-4a6ed60ad1be")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5bcabb11-e4f9-4323-9beb-25bcbeebdeef")
		)
		(fp_line
			(start -0.65 -1.125001)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4106589e-7094-4d2c-b20d-3f28142c10e3")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "401f6980-9217-435e-ab47-f1f5c7af34cd")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8017c2ab-ebc5-46bb-ac58-2cd1fb38b4c6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "6c49eabe-434d-4d57-ac18-5540b201880e")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "c61bc2a9-918f-4920-adf1-db602d8eadf8")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pintype "passive")
			(uuid "d1502c6b-c777-4b74-99ab-6bfc5ad81d7f")
		)
		(pad "3" smd roundrect
			(at 0.937501 0 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 55 "Ia_MON")
			(pintype "passive")
			(uuid "5971c3e1-66c1-4631-a822-37fa16eca755")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_Tantalum_SMD:CP_EIA-7343-31_Kemet-D"
		(layer "F.Cu")
		(uuid "f07619bd-a84b-41cc-a69d-8be87c48e561")
		(at 114.9 49.299999 180)
		(descr "Tantalum Capacitor SMD Kemet-D (7343-31 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
		(tags "capacitor tantalum")
		(property "Reference" "C5"
			(at 0 3 0)
			(layer "F.SilkS")
			(uuid "13db6371-348f-4d64-89af-b490c018880b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "47u/25V"
			(at 0 3.1 0)
			(layer "F.Fab")
			(uuid "c6712bb7-20c8-4db9-a4fb-7b9f6edd4f9d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_Tantalum_SMD:CP_EIA-7343-31_Kemet-D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9c79a582-521b-47fb-b01b-90912d5e87d4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c9c9fafe-0dac-41f5-add9-2a68cb79bb62")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c873b54a-bf51-4bd4-ab3a-834edacf7ced")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Link" "https://www.chipdip.ru/product/tecap-47-mkf-10-v-tip-b-10"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "83b2e749-0451-463f-95f7-20c757958900")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "CP_*")
		(path "/14b91df0-5725-4b02-9b13-1d2bd430e786")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 3.65 -2.26)
			(end -4.41 -2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b9e7e52f-3e37-4f82-a0d9-c9262449a35e")
		)
		(fp_line
			(start -4.41 2.26)
			(end 3.65 2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1805949d-196b-4b88-a770-063adc5be69c")
		)
		(fp_line
			(start -4.41 -2.26)
			(end -4.41 2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ea63af50-c752-4469-971d-52976287dd56")
		)
		(fp_line
			(start 4.4 2.4)
			(end -4.4 2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5e95207a-3ec9-4787-8d9c-8ca09c6359f7")
		)
		(fp_line
			(start 4.4 -2.4)
			(end 4.4 2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "052c7cae-afc1-48d7-bd2d-37920ff2a3f2")
		)
		(fp_line
			(start -4.4 2.4)
			(end -4.4 -2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bdf27feb-a8e0-4d19-a09f-c942f8971682")
		)
		(fp_line
			(start -4.4 -2.4)
			(end 4.4 -2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "24959c60-89e1-40ce-a41a-b54386cbe6f9")
		)
		(fp_line
			(start 3.65 2.15)
			(end 3.65 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "890b75f1-6035-4ee0-9ea8-6a698e92e378")
		)
		(fp_line
			(start 3.65 -2.15)
			(end -2.65 -2.150001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ed9af27d-b3f1-4597-b12d-47932c555f75")
		)
		(fp_line
			(start -2.65 -2.150001)
			(end -3.65 -1.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "030e685e-b972-479d-b434-1b4d91664007")
		)
		(fp_line
			(start -3.65 2.15)
			(end 3.65 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1bf9d7de-8416-4605-932f-896987ae83b1")
		)
		(fp_line
			(start -3.65 -1.15)
			(end -3.65 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f618869b-480c-4983-8b82-94bbdbdefdbc")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b1d7f5b4-57ca-4245-ae36-e9f3707e4a52")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -3.1125 0 180)
			(size 2.075 2.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.120482)
			(net 6 "+5V")
			(pintype "passive")
			(uuid "88b2a75c-f1d4-48fd-8ed2-153ba37a45f1")
		)
		(pad "2" smd roundrect
			(at 3.1125 0 180)
			(size 2.075 2.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.120482)
			(net 4 "GND")
			(pintype "passive")
			(uuid "a8114e39-1aab-485b-bccc-97003c372ddb")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-31_Kemet-D.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Ecohim:TestPoint_Pad_D0.8mm_no_circle"
		(layer "F.Cu")
		(uuid "f4d0be1f-7c48-4ff9-95f3-7acbde0e7341")
		(at 86.6 60.100001 -90)
		(descr "SMD pad as test Point, diameter 0.8mm")
		(tags "test point SMD pad")
		(property "Reference" "TP2"
			(at 0 -1.448001 90)
			(layer "F.SilkS")
			(hide yes)
			(uuid "150fa866-6a7b-42cc-a8a1-9d3f867e4b52")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TestPoint"
			(at 0 1.550001 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "e4af34a8-298a-4e0a-b214-46990dc9f75c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Ecohim:TestPoint_Pad_D0.8mm_no_circle"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "1f808f08-e272-4a9d-9b2a-e362cd5791d7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "7c7e75bd-729d-4d41-960a-528ab5aa4517")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "056419e6-78ae-4843-b142-9334cb150149")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Pin* Test*")
		(path "/5f5f8096-ea7c-4b8b-bea8-8837b931a6fc")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 0.381 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "F.CrtYd")
			(uuid "b8383559-ac37-4938-8bfa-83753b0fd430")
		)
		(pad "1" smd circle
			(at 0 0 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask")
			(net 36 "Net-(D4-PC10)")
			(pinfunction "1")
			(pintype "passive")
			(uuid "804d6c81-275e-4fd9-ade4-bc8e2b283256")
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(uuid "f657a609-8a6f-4766-8fd5-ba0e7b50a8e3")
		(at 65.9 50.862499 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 1.6 -0.6 90)
			(layer "F.SilkS")
			(uuid "0ef85fd9-f7d2-41bc-8fa5-280534578cc7")
			(effects
				(font
					(size 0.9 0.9)
					(thickness 0.15)
				)
				(justify right)
			)
		)
		(property "Value" "100p"
			(at 0 1.679999 90)
			(layer "F.Fab")
			(uuid "f01dab67-3da8-477e-960b-487010a162bf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ca46b93f-893e-44ca-98bb-8a2f29f1d723")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "26b4aa7d-7898-48cf-b0b1-8d54f0ad1087")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "84a84606-7f7f-4f16-9f20-5c5c0c1cef78")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7a35176f-9a5b-4bab-b918-e0a4290f7e37")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/4e61dc92-c04a-4865-a995-9484b18220c1")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.261253 0.735)
			(end 0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fe987919-9f74-4db6-aae7-90fa4d01a4c5")
		)
		(fp_line
			(start -0.261253 -0.735)
			(end 0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8018139a-202c-4ae4-b5f5-9af677b18101")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "11c14fc2-12ef-4652-82ca-f9f6b8e88ee9")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0a9d170a-bb62-4456-9c49-b0e969efac34")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "78f35a80-83a7-4f5d-b57f-1d68a438deb0")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "827902e5-b4cb-4f74-9a44-db2dbacf79b5")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0a7aafa5-c1c0-4367-a389-e1cc21a49093")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ab41be54-65f4-4ed9-aa17-021ecbafafdc")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2b2010ca-0dc5-4c7c-b28d-941d425388e4")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0d9d61ff-d40a-4e14-8d99-111f0695a7df")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "609c0be8-8dbd-472e-a1c3-bd829cc22c6e")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "XRAY_ON")
			(pintype "passive")
			(uuid "32c05e66-1a62-4ea3-8132-46dc0c7aacb7")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "9d580e9b-0d10-4c90-8c34-b04db0e58b45")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(uuid "fa4c54d9-3fb1-4677-94f7-46a4bc6c8346")
		(at 44.45 47.550002 180)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "VD9"
			(at 0.7 1.8 0)
			(layer "F.SilkS")
			(uuid "0b3e19af-f2de-46c7-8581-4de24919ce0f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MMSZ5234B"
			(at 0 2.1 0)
			(layer "F.Fab")
			(uuid "1bf042a7-7bb9-4bad-9a89-c4eabe1b4893")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "76193316-2887-47e4-8a40-e6372854a6b8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4f9855af-fc69-439e-b01f-9d5905dc9a5e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cc7a34b1-f7f1-43cb-8140-e5e4ccbe9a01")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/8017539211"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bf203a84-c6b8-4735-9b68-6f7c701e443c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/aad97402-333f-481c-ba65-19c69e682163")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.36 1)
			(end 1.65 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9648928b-3228-4005-a05d-0706f1c6daf9")
		)
		(fp_line
			(start -2.36 -1)
			(end 1.65 -1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8b3d5dff-2ff5-48a9-b432-29c749265929")
		)
		(fp_line
			(start -2.36 -1)
			(end -2.36 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c29e4be5-d1bb-424c-9445-833941469601")
		)
		(fp_line
			(start 2.35 1.15)
			(end -2.35 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "006a8396-6a45-46c2-9ef2-964ac46959e3")
		)
		(fp_line
			(start 2.35 -1.15)
			(end 2.35 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "22596110-8fb6-44cd-bd19-93749ee171c7")
		)
		(fp_line
			(start -2.35 -1.15)
			(end 2.35 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "358fc5b6-45b3-466f-a53c-48035674917a")
		)
		(fp_line
			(start -2.35 -1.15)
			(end -2.35 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c437f5cc-554b-49fe-8fee-47a6b9d59576")
		)
		(fp_line
			(start 1.4 0.900001)
			(end -1.4 0.900001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7a6dc50e-f20e-4619-8f3f-c1d453212f46")
		)
		(fp_line
			(start 1.4 -0.900001)
			(end 1.4 0.900001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d88b7562-3daf-4f24-94db-78434e2a46e8")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.349999 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a15e3ac6-6c7f-42ea-9681-51e3e5534b96")
		)
		(fp_line
			(start 0.25 0)
			(end 0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ecc4ff6-c38b-484b-93b1-bf5638becaeb")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "204119ac-bb64-459e-a829-c3c262583879")
		)
		(fp_line
			(start -0.349999 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f4e44f1e-edd4-4049-8e53-b64e85f3fa33")
		)
		(fp_line
			(start -0.349999 0)
			(end -0.35 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c377c88f-a057-49c2-a8b2-344428d6f8e5")
		)
		(fp_line
			(start -0.349999 0)
			(end -0.35 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "90a3a859-c9bc-42fa-a909-4b087fae32e3")
		)
		(fp_line
			(start -0.75 0)
			(end -0.349999 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "db845747-c3a8-45a8-a41c-1a9a6dd6e969")
		)
		(fp_line
			(start -1.4 0.900001)
			(end -1.4 -0.900001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e0a2c247-7338-4ffb-9b3b-abfd06f4c18f")
		)
		(fp_line
			(start -1.4 -0.900001)
			(end 1.4 -0.900001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4e93639f-6e40-4346-b9ef-8a7e01b9f796")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2.000001 0)
			(layer "F.Fab")
			(uuid "49311f75-b467-48a1-ac3e-8c9e392c5bf7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.65 0 180)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 88 "Net-(VD9-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "adb89887-f781-4213-a034-3eef2383da6a")
		)
		(pad "2" smd roundrect
			(at 1.65 0 180)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "4424d55e-0203-40a6-9e29-262d30f72016")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(uuid "0753e797-ea7a-4851-9362-871faa881583")
		(at 75 56.1 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.7 90)
			(layer "B.SilkS")
			(uuid "78656b69-64b1-41d7-bb5e-a90189f45a6b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "2k"
			(at 0 -1.65 90)
			(layer "B.Fab")
			(uuid "6736563e-b2c3-4b3b-b0e1-22dc90b96b72")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "8f414cc0-a4d9-4d26-9fe0-ebe0439c6642")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "716139f1-e151-43a1-b381-3680e6d22af2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "96272ab9-b39a-4131-bb58-e49fcb05c9fb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/eb48f923-47bd-485b-af13-b816a73fc10f")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.227064 0.735)
			(end -0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "251edf84-d97e-45ff-9e8e-c28f78d5c1ed")
		)
		(fp_line
			(start 0.227064 -0.735)
			(end -0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "1134086b-33a8-4dce-9c99-362b8e6e0f4f")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "90f2c938-469b-4555-bec3-889a7eff0b78")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "78bf3a06-0ed6-4325-aa88-e75ef9c78b6c")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "64e5b4a5-c329-488e-833f-aeab48c2004e")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "6b216d88-2cd0-4045-bd71-60be8e7414be")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "48ab7a49-1d75-4908-a146-3d68b9671eae")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "28b8fe38-d008-43fd-95f6-e370d1d09ef6")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "aa4ef14d-c09b-496d-8c7b-804cc9526926")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "b54cb9ed-99e1-439a-9a5f-845aa210cb08")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "c70ca94e-ca29-40f1-b6da-a77aed50f736")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 73 "Net-(HL2-K)")
			(pintype "passive")
			(uuid "11c4e0f6-bdef-494d-8593-b497a09594e5")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 4 "GND")
			(pintype "passive")
			(uuid "3acc3030-9df7-45b4-a3b9-c2e3756e0016")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "0defc75d-cbeb-427b-89ec-6422c9a014fc")
		(at 40.8 54.5 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C29"
			(at -1 1.6 90)
			(layer "B.SilkS")
			(uuid "b3a66728-13b9-4c13-b465-554e766ed058")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "0.1u"
			(at 0 -1.679999 90)
			(layer "B.Fab")
			(uuid "89317dfb-90e4-4e98-8ad8-fbdaf3d0dbfc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "cde5cd17-6e0f-4604-801a-53af362a5a89")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "fc83e487-2212-4316-83c5-1d53f8c86a88")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "e2a5227d-69c2-4c2a-bb13-5ba64b00a752")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/43780"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "3897f601-fc4a-46fa-b996-467acdddaf32")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/e8c25edf-fe48-4cb3-9720-ce29e9a35b4d")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d0ced843-372d-405a-86fb-3f74060d86c3")
		)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "58af75d2-72e8-4a60-ad6c-4619b48fcb46")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "5b5f7e1d-7341-490c-b1a9-e13ad2ea7bdf")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "ef0dd0ae-c3cf-436a-a8f6-da13ccb44e47")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "c5168ad7-5127-43e9-aa25-b9aee53e9f90")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "0d73b946-e83a-4bfe-bf15-a6648469355f")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "eacc97e5-7b6b-413e-8891-a33b042e1c01")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "3ceac204-adeb-4d7f-93b0-32c2f0b44c4a")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "09d19ed4-0208-4d4f-a0c3-84c3e90374d1")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "cf6d1636-1d16-4cb5-b706-01a4bcc1d143")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "cd880e96-957a-47e0-8eeb-01f062e0175a")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 12 "+12VA")
			(pintype "passive")
			(uuid "3e6bebfa-b50e-4b24-afea-93afe25dd56b")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "2f7ba69f-e9ed-462a-89b4-6772fa52c90b")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "0e7c9028-d1c8-4ded-8115-bf69fcd136d7")
		(at 92.7 48.4)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 0 -1.6 0)
			(layer "B.SilkS")
			(uuid "6ad0bc5f-8d2c-479c-91be-f76faa073b5b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "0.1u"
			(at 0 -1.679999 0)
			(layer "B.Fab")
			(uuid "77a12308-abeb-45cc-bf2c-4e7a3d007467")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "622cd17e-9b23-40b1-860f-cc39abaffe8b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "84a3f67d-9268-4dc6-8be8-88b00f4788de")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "318c35be-f0e3-4497-8e06-fc92bf561b77")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/43780"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "5cf7a2e0-05d7-4d7c-af87-45d6de39d265")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/c17acf72-abb9-4dbb-86ef-ef12a37724b3")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "636d1bf6-88f8-4650-a947-903f5985e9eb")
		)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c533ac19-ce18-4518-b456-cebcb9e804f1")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "31eedb68-3cbd-40f6-b596-7db3966718d5")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "71d7eaa2-9d64-4153-8313-1d21f7706fed")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "24130b19-05f6-442e-b497-1d273ccf3309")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "bd84edf1-4098-48f8-aac4-81a5ca4d4e04")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "d15338e8-f9d1-4f23-8894-1e8f9ae76f02")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "60da8afd-a758-4b12-a17b-d5974d7b0dd4")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "5d871e5f-582c-463f-9699-b38db78de816")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "09c0a109-aced-4f56-b140-81c9aa5860d6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(uuid "d1ffff4f-3839-44f8-8e75-a6146d1b86f5")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pintype "passive")
			(uuid "31a7301d-5b7a-4c36-80bc-4928030c3136")
		)
		(pad "2" smd roundrect
			(at 0.949999 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "5f5e784b-18eb-4f08-9bbc-7b2ecc57d46c")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "B.Cu")
		(uuid "0eb3754b-a800-425e-8816-f17edcea3f93")
		(at 114.9 54.1 -90)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "D3"
			(at 0 -4.3 90)
			(layer "B.SilkS")
			(uuid "f09b3dcb-9123-4abc-ba45-8f46d4e15c6f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "LM1117MP-3.3"
			(at 0 -4.500001 90)
			(layer "B.Fab")
			(uuid "80e13671-4659-46cc-b40f-0ca08bc2307a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "7f1b7a5e-4a27-4498-81c3-fb1480222b15")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "52a516d7-249f-491a-84b1-ff6e9d04fee6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "6112f79c-4b93-4585-bff1-f576cc87c88b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Alternative" "AMS1117-3.3"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "93913c77-28fc-467d-b73d-efc296750432")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product/ams1117-3.3-umw"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "c43f972f-2c3e-4b63-9873-99ae87835d15")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "SOT?223*")
		(path "/d4b38d91-e71c-4e2e-9865-a67f8b39a7f6")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 1.91 3.41)
			(end -1.85 3.410001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b81ca1b7-4cd2-41a3-b721-e5df7b4e1f3a")
		)
		(fp_line
			(start 1.91 2.150001)
			(end 1.91 3.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "3d73b14c-007e-4688-8920-019d9455bc16")
		)
		(fp_line
			(start 1.91 -2.150001)
			(end 1.91 -3.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f3a1d1df-d1b0-41ea-acde-e6fec8fa5864")
		)
		(fp_line
			(start 1.91 -3.41)
			(end -1.85 -3.410001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "e7941445-1130-4667-98e6-98501ff34424")
		)
		(fp_poly
			(pts
				(xy -3.13 3.31) (xy -3.37 3.64) (xy -2.89 3.64) (xy -3.13 3.31)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "B.SilkS")
			(uuid "c960c5cf-0c80-4573-9e46-f1897c461ca7")
		)
		(fp_line
			(start -4.4 3.6)
			(end 4.4 3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "0bd43e38-6daa-414a-834f-850d1b1efe32")
		)
		(fp_line
			(start 4.4 3.6)
			(end 4.4 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "c2d5fcb1-6c34-440a-93af-dc33f23f6ad4")
		)
		(fp_line
			(start -4.4 -3.6)
			(end -4.4 3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "b99b4ee2-a5e7-49c4-a153-968b5b48fd78")
		)
		(fp_line
			(start 4.4 -3.6)
			(end -4.4 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "5dc20027-d659-4fcd-afe4-01a212d3b84e")
		)
		(fp_line
			(start -0.85 3.35)
			(end -1.85 2.349999)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "ab8a0061-9927-431e-8d25-8adf35c82ddc")
		)
		(fp_line
			(start 1.85 3.35)
			(end -0.85 3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "0cc32876-8cc1-4a33-afb8-ac031a3ead87")
		)
		(fp_line
			(start -1.85 -3.35)
			(end -1.85 2.349999)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "be53de3b-b36e-4f10-a0be-f516caa8411a")
		)
		(fp_line
			(start 1.85 -3.35)
			(end 1.85 3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "43a10a4f-b0bd-4b5e-b97e-e4414334db30")
		)
		(fp_line
			(start 1.85 -3.35)
			(end -1.85 -3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "7c0d162f-23eb-4068-86cb-68196fe168d4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(uuid "5fd95938-ed1f-4105-bba7-f3815b43274d")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -3.15 2.3 270)
			(size 2 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "aef54bd3-7cde-4540-82fa-a0dab6170aa0")
		)
		(pad "2" smd roundrect
			(at -3.149999 0 270)
			(size 2 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pinfunction "VO")
			(pintype "power_out")
			(uuid "475c792d-3263-4439-a099-39b1a0b58a4d")
		)
		(pad "2" smd roundrect
			(at 3.149999 0 270)
			(size 2 3.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pinfunction "VO")
			(pintype "power_out")
			(uuid "60772331-5082-435a-a635-dd4ddec63911")
		)
		(pad "3" smd roundrect
			(at -3.15 -2.3 270)
			(size 2 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 6 "+5V")
			(pinfunction "VI")
			(pintype "power_in")
			(uuid "28565d27-0fb3-4adc-bae5-fc310161a5d6")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_Tantalum_SMD:CP_EIA-7343-31_Kemet-D"
		(layer "B.Cu")
		(uuid "0fb65ea6-819b-4930-a05b-84d5c95609f0")
		(at 60.9 41.4 -90)
		(descr "Tantalum Capacitor SMD Kemet-D (7343-31 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
		(tags "capacitor tantalum")
		(property "Reference" "C15"
			(at 0 3.1 90)
			(layer "B.SilkS")
			(uuid "993f2402-9e5e-457f-a489-a3396c4bf3cd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "47u/25V"
			(at 0 -3.1 90)
			(layer "B.Fab")
			(uuid "37a4a7ca-1470-46c3-96f0-6f1b53c37c80")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_Tantalum_SMD:CP_EIA-7343-31_Kemet-D"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "41c0cf06-db8b-4666-995f-41862d33f91f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "f18c2e04-7866-4fdd-bdf3-9d004f72b58b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "58c52f45-48ea-4c3d-9709-b213d0938a00")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "CP_*")
		(path "/5427eb38-7a13-4967-b64f-d10fe660570a")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -4.41 2.26)
			(end 3.65 2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "65985e4d-b25f-4503-b4ed-578be89b6eb4")
		)
		(fp_line
			(start -4.41 -2.26)
			(end -4.41 2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "06e60673-b004-4e51-b630-8be9a3b04ecb")
		)
		(fp_line
			(start 3.65 -2.26)
			(end -4.41 -2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d0bb3082-451f-4dbe-9f03-f6070a42c349")
		)
		(fp_line
			(start -4.4 2.4)
			(end -4.4 -2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "b3b63a12-fc14-4ccc-bc3e-1539c0d6f7f6")
		)
		(fp_line
			(start 4.4 2.4)
			(end -4.4 2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "fb22c6d8-2b0d-4c70-aa53-0a2859c6a553")
		)
		(fp_line
			(start -4.4 -2.4)
			(end 4.4 -2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "b65ec8a4-80f4-491d-9a5f-aa6095127915")
		)
		(fp_line
			(start 4.4 -2.4)
			(end 4.4 2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "5c64a2bf-911c-4cc0-8124-6952b6b0cf41")
		)
		(fp_line
			(start -2.65 2.150001)
			(end 3.65 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f2f75b86-21b9-4737-aef8-8380327e3ff7")
		)
		(fp_line
			(start 3.65 2.15)
			(end 3.65 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "8eac3df2-347f-4293-9aeb-ca853c81fe25")
		)
		(fp_line
			(start -3.65 1.15)
			(end -2.65 2.150001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "2bec2bfc-9d3e-40aa-b338-20c1fa50e9b2")
		)
		(fp_line
			(start -3.65 -2.15)
			(end -3.65 1.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "3767a76a-a183-4152-8ef9-d9d99a2be200")
		)
		(fp_line
			(start 3.65 -2.15)
			(end -3.65 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "260de267-483c-4b38-81ae-8a26e1f7eae0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "c0981f3e-e234-42a6-b43c-49dbbb792c15")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -3.1125 0 270)
			(size 2.075 2.55)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.120482)
			(net 12 "+12VA")
			(pintype "passive")
			(uuid "bbd3240b-cf3e-4765-8e2f-9eb76b2636ec")
		)
		(pad "2" smd roundrect
			(at 3.1125 0 270)
			(size 2.075 2.55)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.120482)
			(net 4 "GND")
			(pintype "passive")
			(uuid "39fe4ccb-1fbe-4997-b331-8cf1a30b36c6")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-31_Kemet-D.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "124120d5-5875-47ce-9e5a-2ae6446daa61")
		(at 135.2 48.3 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 2.9 0 360)
			(layer "B.SilkS")
			(uuid "b679e3dc-69d8-4592-b013-b56eab72e7e8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "0.1u"
			(at 0 -1.679999 360)
			(layer "B.Fab")
			(uuid "c9384f59-aa28-4aff-95bd-710577b7d761")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "820f72ac-8b51-42f9-bf5a-c41b8a52b33a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "3d61c48b-09b7-411a-a97f-76e4ea484209")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "984f8342-2d38-418f-994c-5f376c105c16")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/43780"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "f0be8de3-6b03-4575-aa14-b16977f70196")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/3a66e05f-9e22-40ba-bf4c-0c160d5717e0")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f85a37cf-81d4-4137-a1a9-2adea4b84f23")
		)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c5ba8698-d2eb-40d2-a9d4-65d86e742cfc")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "bb414d3d-28bd-48e5-8fa2-7a52286693d5")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "b2d70fe8-e329-468f-9168-3659efb79a3f")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "2ccf0611-eb1b-446e-a97b-7765c33b357b")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "867feb33-2bec-4372-a872-23c9b30a32da")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "a5520119-5ab4-4b69-8b15-9077d50cedfc")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "24eee166-4e2a-447b-90cb-1d838ef24464")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "589d863c-a887-4983-8257-a93fa31b1fca")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "6b9b1007-ccb6-4508-b4ca-7721c2b4b762")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "B.Fab")
			(uuid "1ca8becc-782c-418f-a667-a7d7d041193b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+12V")
			(pintype "passive")
			(uuid "d6d81264-db31-46e9-b542-210eb6c44a1a")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "4a79c68b-9f23-4135-967a-d535717f7bed")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(uuid "1464cc43-7ea2-45ed-8dd2-7d09617b0cb9")
		(at 85.5 40.499999 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 2.022651 1.61015 90)
			(layer "B.SilkS")
			(uuid "4bb3c0b3-6d80-4e26-9066-42955876412f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "100k"
			(at 0 -1.65 90)
			(layer "B.Fab")
			(uuid "bd0dd733-6257-4a54-a64f-4abbfb3c27f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "ef92220e-c0fa-4258-9c39-339b59a1e245")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "0f7d83a5-ad41-4017-8cfd-fb20171cca3f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "51609633-099c-4c57-9a17-7e1cee8488eb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/8cd8f4a6-993b-47d5-affa-024567181969")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.227064 -0.735)
			(end -0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "bf9ba32b-e269-495d-8517-914cd0528191")
		)
		(fp_line
			(start 0.227064 0.735)
			(end -0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a3bf7308-a53f-4379-b533-95753cc88daa")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "9368a121-2eb2-49c7-92bf-6ded6b986ca5")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "7baa5883-89fa-4109-9bae-9a36d194c326")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "e480783a-f32f-4038-a11c-df5f1d44cb76")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "fbc8e9fb-c2be-459a-99ea-d09b741a89a8")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "8f227f43-362d-4736-9c20-ce33733f6e5b")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "b175d5fc-9b78-4828-af60-1a8963d1e6c0")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "5a31c0aa-f4c5-4261-a52d-3ebc41036e33")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "b8833381-22e2-4b7f-8850-d292e928c749")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "f271dbf5-9e29-4b3a-89ec-4f6d0ba7cae3")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 86 "X_HV_15V")
			(pintype "passive")
			(uuid "51c35203-a1aa-41e8-8ab8-90d08b257795")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 19 "HV_15V")
			(pintype "passive")
			(uuid "9bd0eabb-d3f0-43b1-aaf9-14a7b76b63f0")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "1575d3f8-a155-47dc-b679-4f6f4015bba7")
		(at 123.7 52.7 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at -2.600001 0 360)
			(layer "B.SilkS")
			(uuid "5d3fb7b6-349a-4251-8839-9b7a9caf7db6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "0.1u"
			(at 0 -1.679999 360)
			(layer "B.Fab")
			(uuid "26991842-6bbc-469d-954c-181a4108f533")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "cc69b6aa-f962-4f69-a61b-9498bab91da1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "44419e92-b56b-40e1-a9a1-9aeb694dadfc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "a7a9a8d8-d4e5-40bd-ab3f-3c5dbf7d034e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/43780"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "3bd06055-b41e-4b29-82b4-301bb8d8024b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/7140b136-d5da-4f62-8186-83641248129f")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "fcab98f5-23b0-4b3b-a3ed-142007367d00")
		)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f31540df-f2fd-486b-93c0-2666b5abdb40")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "d22bdf82-9b7b-4b9b-84d6-0c6b74818087")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "c103ed94-9105-4254-8f62-05463afaf3ec")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "4a9484a5-1b0d-42c9-a092-dd0980444bd1")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "17faac12-4417-4e4d-b7d6-d4d582dfdcb0")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "1d702785-8c53-4331-905d-b88bc0fbfdcc")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "138b0124-9f66-4f9e-a2f1-86fb436c59b4")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "60d28873-a681-40cf-9baf-5ac8270c08a5")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "bd8d217b-55dd-4dd5-9533-2b8836e5e241")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "B.Fab")
			(uuid "90253870-62e1-4d00-a5a7-8507b2ea438f")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 6 "+5V")
			(pintype "passive")
			(uuid "62066d45-da94-44f0-a7ae-a86d2122e669")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "29567b56-dfe5-497c-9d85-4c7bcf3e5c9c")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_Tantalum_SMD:CP_EIA-7343-31_Kemet-D"
		(layer "B.Cu")
		(uuid "15938f39-9526-496a-a87d-dfffd80fda86")
		(at 136.6 42.1 90)
		(descr "Tantalum Capacitor SMD Kemet-D (7343-31 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
		(tags "capacitor tantalum")
		(property "Reference" "C2"
			(at 2.4 3 90)
			(layer "B.SilkS")
			(uuid "6d5daf31-de86-4f0e-9802-521fe4d7e58f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "47u/25V"
			(at 0 -3.1 90)
			(layer "B.Fab")
			(uuid "3f0a55fe-2c48-417b-a907-323ceeeb9356")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_Tantalum_SMD:CP_EIA-7343-31_Kemet-D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "b702319b-8638-4a34-bd14-9d917cd96ff5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "66704bf6-1ea5-4c92-93b4-ab583c035560")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "2967c66a-a6aa-473b-8542-c35a4a620691")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "CP_*")
		(path "/81fb9b25-ffd3-45f4-8447-93186c4434c2")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 3.65 -2.26)
			(end -4.41 -2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c6b983b6-0d34-43c6-9e5c-2c0150ded5bd")
		)
		(fp_line
			(start -4.41 -2.26)
			(end -4.41 2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "35e85223-8d3f-4732-adcf-e99cd2a6556b")
		)
		(fp_line
			(start -4.41 2.26)
			(end 3.65 2.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c2c999bf-a4fe-4231-9b6f-bf788975d068")
		)
		(fp_line
			(start 4.4 -2.4)
			(end 4.4 2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "09460f8a-9f0d-4bf4-8eef-2e246f31d9c1")
		)
		(fp_line
			(start -4.4 -2.4)
			(end 4.4 -2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "3925d85a-e07c-4f2f-b10b-c61811a6951b")
		)
		(fp_line
			(start 4.4 2.4)
			(end -4.4 2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "d197c77d-1024-4d59-8471-5f911fde9fab")
		)
		(fp_line
			(start -4.4 2.4)
			(end -4.4 -2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "a481e594-c719-4d00-b50e-63ae30df67ee")
		)
		(fp_line
			(start 3.65 -2.15)
			(end -3.65 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "7403a761-f8f8-4f19-886f-200c4d0af4a9")
		)
		(fp_line
			(start -3.65 -2.15)
			(end -3.65 1.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "5994ad4c-dd47-4f65-a4e3-c2824479c6be")
		)
		(fp_line
			(start -3.65 1.15)
			(end -2.65 2.150001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "d1260eea-6b63-487d-9c2b-6e2a58e4b6f4")
		)
		(fp_line
			(start 3.65 2.15)
			(end 3.65 -2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "13aa235c-5f89-4eca-b4be-13d81838fb77")
		)
		(fp_line
			(start -2.65 2.150001)
			(end 3.65 2.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "b44d57a6-0be2-46d3-ac30-414cd1640b35")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "58cf4ed1-da46-4cbb-ae4e-24968691c395")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -3.1125 0 90)
			(size 2.075 2.55)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.120482)
			(net 5 "+12V")
			(pintype "passive")
			(uuid "3a3f226c-8065-41e2-971b-010d580d597f")
		)
		(pad "2" smd roundrect
			(at 3.1125 0 90)
			(size 2.075 2.55)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.120482)
			(net 4 "GND")
			(pintype "passive")
			(uuid "62e599ea-a596-4696-8965-46fec160fb10")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-31_Kemet-D.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(uuid "20445ef6-300b-41e7-874c-3ac1f16652c1")
		(at 36.1 42.6)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R21"
			(at 0 1.65 0)
			(layer "B.SilkS")
			(uuid "f9757772-4b2d-4f02-9df4-b72616c4b6f6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "none"
			(at 0 -1.65 0)
			(layer "B.Fab")
			(uuid "000ff628-639c-4c96-9361-d26fc94bb4ce")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "174ffc7c-6f9a-49af-bcf4-fc3ddfa3f934")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "0d700454-1425-46b7-9322-ecca6701b4a6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "0b23d4cd-407c-4800-ba4b-b278d9b3142f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/0542a7a1-fb15-4421-a37e-9d681ef58b49")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(fp_line
			(start 0.227064 -0.735)
			(end -0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "eb1e57f7-b1a3-4172-a89e-977976cf2f8e")
		)
		(fp_line
			(start 0.227064 0.735)
			(end -0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "24e369d5-671c-4629-aec3-8227f486c840")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "f77c7851-521f-48a6-b965-13c346eee908")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "70dec099-8b5e-45a2-9aa7-ca58ce60a41e")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "4056d233-ea49-40d3-b9f5-073f61f978dd")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "5a9f304f-cefc-4998-8e5e-8461d5707644")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "5c6e9c2c-2e06-4d52-828d-cd0327c5e648")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "ae18d8da-8876-4ef7-be63-6d9bcf841db7")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "b8d70c8f-1285-4263-856e-5cd4d4a97a48")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "1323e2ff-c7dc-466a-80f8-2aed6f886eac")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(uuid "80d6f595-7c4b-4776-b963-03167553bafb")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 4 "GND")
			(pintype "passive")
			(uuid "b9f69827-f2ed-4bdb-b1f9-75727f8805e7")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 67 "Net-(D6B--)")
			(pintype "passive")
			(uuid "20c15828-0773-419a-a520-1b2ac329c4d4")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "21f043c1-2bcd-472d-a870-dc7d06d88f48")
		(at 111.8 40.8 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 1.679999 90)
			(layer "B.SilkS")
			(uuid "3a426fd9-2385-4ee3-ac0d-e7f5085b04c1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "0.1u"
			(at 0 -1.679999 90)
			(layer "B.Fab")
			(uuid "5920e254-acc5-4883-9b0c-d78c5aa337c8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "8a680353-a0e1-47e1-8020-7c5ae083a41c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "1adc05b3-80cd-4f62-acb9-aec0bc0b0291")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "b315749f-7e24-45ea-b352-f50017b598be")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/43780"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "386b7ab5-d528-4ca2-8c6d-78321b403cc9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/134165e6-25bf-4cf6-984e-970ed9d1bd04")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f4c4e36a-93f3-4b90-b74d-49b1e8474c87")
		)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6c789362-d942-4a37-acfc-608582aa4c83")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "e6d4f38c-26b4-4d9e-a8ab-e158b4b7bf8d")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "eaebf30b-fc99-4d73-96ae-83b91fd5053b")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "c457195f-1021-49b8-beb4-f53457f7dd42")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "f03dddca-d7dc-4754-bf21-3a6ec47dc03c")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "46a2ec50-fa22-48b3-b165-b065fdb1b982")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "a46002e3-373d-4b66-ac05-aa7229467d92")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "a3fa9277-bc4c-4b9d-85ae-d0834d97c6c1")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "cf37988f-7611-49e3-8d4b-abf3cb548381")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "8d515ffb-9e5e-4247-af71-5da0ec6d8494")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pintype "passive")
			(uuid "acce3b30-6aeb-4fed-9a9a-f2b5152fd116")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "e20ffa40-e6b8-44f3-ab8b-2d494ee908c7")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "2498b149-21ad-4765-8ca9-41fb161ebb78")
		(at 86.2 48.4)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 0 -1.6 0)
			(layer "B.SilkS")
			(uuid "076faba3-3ffa-4da2-b612-4d5bb134db21")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "0.1u"
			(at 0 -1.679999 0)
			(layer "B.Fab")
			(uuid "1725f405-f605-45e4-aec8-f0f61dc3aa5d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "19e7b81b-b8da-4158-9bc1-5b1adf014e5d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "2e30ae7a-2630-44d3-924c-bfd8be44040c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "860dda4f-ded9-48f5-9764-850eed80c66c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/43780"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "02e50b77-099b-4a78-b1fb-7363bf35cd8b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/f52b8d43-f94b-4360-a216-88988a408bee")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c56ce78c-5994-4020-bca3-1a9a1a94c998")
		)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "38c6b634-ba63-4b5f-93e9-e1c82e005be7")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "5b0e6231-851e-4ee4-ad20-ee7229a52357")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "6b457b48-7050-400b-a902-77c653d9fb66")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "2a41e106-a8ac-4ea7-9c88-eaedad1550c4")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "937a5859-23be-4e0c-9f52-3a73ac3fde5d")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "db5da991-63b4-4b65-9c91-411786a63f80")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "a15bde36-59da-4309-966b-147ad026ca41")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "08721da5-5d79-4805-875e-fe22d673776b")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "639d30a1-8b08-41fc-8032-08e57f0b99ce")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(uuid "9ae76957-880c-4947-8795-b5f67b636f63")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pintype "passive")
			(uuid "c442ba99-c314-4143-9bcf-60205bd12d94")
		)
		(pad "2" smd roundrect
			(at 0.949999 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "0208f595-f0fb-491d-a93c-ebedabd694c6")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_1210_3225Metric"
		(layer "B.Cu")
		(uuid "25984de6-e872-4db7-ba84-5e0190200736")
		(at 92.7 51.1)
		(descr "Inductor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L2"
			(at 2.9 0 90)
			(layer "B.SilkS")
			(uuid "345c2596-f2bd-488e-b112-2daa0d360d06")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "4u7"
			(at 0 -2.279999 0)
			(layer "B.Fab")
			(uuid "b5d29468-2040-4ec2-909d-53766fff5d9a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Inductor_SMD:L_1210_3225Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "cebe4053-7201-4907-b938-cbb672378c13")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "c87531c4-59ce-4a32-bf8b-4b2f86401693")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "4b2ab968-7d68-411b-ba33-28ab92c2470b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product/lqh32mn4r7k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "a1643d27-87d1-427a-ae86-64f2343d3e24")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Alternative" "LQH31MN4R7K"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "9506876d-0352-4c7c-a738-616033aa21b3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(path "/2417eaef-a9ef-4125-be34-10c6335ca3fc")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.602064 -1.36)
			(end -0.602064 -1.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "cadec0a8-087f-40b5-a6ce-207c851f50ca")
		)
		(fp_line
			(start 0.602064 1.36)
			(end -0.602064 1.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4c5f574d-b588-4550-b1fb-3c9c5760cd89")
		)
		(fp_line
			(start -2.28 -1.58)
			(end 2.28 -1.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "d98a5fed-2a95-436c-8bbf-3c0dafc9c008")
		)
		(fp_line
			(start -2.28 1.58)
			(end -2.28 -1.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "44bda385-ef74-41c8-afb7-40f35f09a940")
		)
		(fp_line
			(start 2.28 -1.58)
			(end 2.28 1.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "61262daf-f0d2-410c-8e97-8d4d00fa8de6")
		)
		(fp_line
			(start 2.28 1.58)
			(end -2.28 1.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "7a521776-3f1c-4dfa-9fdb-ec4d1d5ba81d")
		)
		(fp_line
			(start -1.6 -1.25)
			(end 1.6 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f4af9c4b-22ea-4920-b262-7fe035e5f999")
		)
		(fp_line
			(start -1.6 1.25)
			(end -1.6 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "58f13968-7b7a-4e41-9ac3-f7677fe37d5d")
		)
		(fp_line
			(start 1.6 -1.25)
			(end 1.6 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c7db513e-2c9c-4c51-ba0c-fcf75b49560f")
		)
		(fp_line
			(start 1.6 1.25)
			(end -1.6 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "e4b15972-f584-4882-a689-45eef8e66359")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(uuid "c275b9bd-de6f-498e-a21d-f577d34e32cf")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.399999 0)
			(size 1.25 2.65)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.2)
			(net 3 "+3V3")
			(pintype "passive")
			(uuid "ff588332-7a72-45aa-92ed-b48f4fd04155")
		)
		(pad "2" smd roundrect
			(at 1.399999 0)
			(size 1.25 2.65)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.2)
			(net 13 "+3.3VA")
			(pintype "passive")
			(uuid "6bad58ba-23e6-462d-8f42-a1abe54a2308")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fiducial:Fiducial_1mm_Mask3mm"
		(layer "B.Cu")
		(uuid "2a1977ba-a08e-498a-86cf-4400398122d0")
		(at 80 60.5 180)
		(descr "Circular Fiducial, 1mm bare copper, 3mm soldermask opening (recommended)")
		(tags "fiducial")
		(property "Reference" "FID6"
			(at 0 2.54 0)
			(layer "B.SilkS")
			(hide yes)
			(uuid "f9c1bae3-de3d-415d-8995-137f57520cbf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "Fiducial"
			(at 0 -2.286 0)
			(layer "B.Fab")
			(uuid "920b985e-f3db-45e4-9426-6716bf6fc938")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Fiducial:Fiducial_1mm_Mask3mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "cd7ad135-2d38-4e36-9c24-dc39c0cab79b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "4eb85d05-6889-4a2a-9464-3d7ab0d4766a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Fiducial Marker"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "419facbc-b8ef-46e1-ab5b-f4eec546e067")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Fiducial*")
		(path "/5df4d828-4331-4a6a-97bf-c996cf818322")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1.75 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "B.CrtYd")
			(uuid "ae7656ec-9f12-4115-83cc-c298377085c0")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "B.Fab")
			(uuid "ffd5ceda-e6ad-4145-bbd9-6f91e52bc5c5")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(uuid "3d65886a-68ea-4140-93f3-85156c42aee5")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
				(justify mirror)
			)
		)
		(pad "" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(solder_mask_margin 1)
			(clearance 1)
			(uuid "6b890747-49e5-436a-a2ab-769a2ced5fe7")
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "2aac0422-196a-4071-89b3-8b0a2a2c2b82")
		(at 103.1 50.8 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0.3 1.679999 90)
			(layer "B.SilkS")
			(uuid "11ad3e47-537c-49e2-a95a-7ef9fcb5c911")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "22p"
			(at 0 -1.679999 90)
			(layer "B.Fab")
			(uuid "5e485810-0ff8-49a8-a4a0-f098e28a97cf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "026fba4c-4c85-4693-bf00-d15f368b2032")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "7baf2482-9fbe-4117-8b75-b9386ef82d37")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "2ad7eeba-d8fc-4182-baa3-6ed7b008f952")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/a2f29b43-e3a6-46eb-892b-5f1178d26f48")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "3dfc983e-8a48-4007-9e19-9453e4987a23")
		)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9d036674-a095-4ee3-8b7b-e35705a756d3")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "3b5bcf97-f350-45f0-9250-24536627e7f5")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "7ab83512-12cf-45e2-aa31-acd66fc3813e")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "930f3f78-cfe0-431f-a0ef-e58a52b1882d")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "9ae03cfb-876a-44a7-9251-60f1f1274fbe")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "d93c49e9-9bbd-4f14-9376-f43524c543f8")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "478591b6-b7ae-4da1-9129-a560458b3044")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c8152b47-36d4-40fc-8208-c884fe2932af")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "d520b260-35b9-4163-b06a-a3f80d843400")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "e735dbe0-8e44-4317-9220-790f6f8507a3")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "336a1362-7262-4771-bfd6-86c8fc69b5ad")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(D4-PD1)")
			(pintype "passive")
			(uuid "868a3ec7-06ba-4ece-b57f-979fab632ad6")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "2d87df26-9f94-45c6-bc32-986ea1263663")
		(at 38.3 56.6 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 3.1 0.3 90)
			(layer "B.SilkS")
			(uuid "653b7a97-aa85-4fee-8511-9213945d6cc3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "100p"
			(at 0 -1.679999 90)
			(layer "B.Fab")
			(uuid "299d1deb-3f56-491e-9381-3495545a393a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "82b21d1a-b34e-4c1d-99f2-81b4acbb90a6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "5e18fbf3-a33d-4a7f-8a51-0d94b6cea2c2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "5c81a9db-698c-49cd-936d-e94a64353213")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "f73c5656-9b27-4a1c-9456-41e8a0b08385")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/113f7385-fe68-46f4-96a0-15731959eb68")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c164fd80-e7ec-4c1d-a395-34885f18f75a")
		)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "30c47b10-8741-499c-8782-b46d787076c8")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "210a2651-7aa2-4b5b-9281-65836114461f")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "085bdb8d-6f89-463a-a925-74a0ae4a0229")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "824afd26-f529-4e1d-9ca2-fdf9e0771d36")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "8d62923e-ecbf-41b1-998b-1c5649339707")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "e2961764-11dd-4320-9709-3025559574ca")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "80c42a35-e054-438a-aa34-f4bc43f85648")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f4ffb22b-d761-401f-a0fa-d5ccb1d89a1a")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "94f96938-487a-4b06-ba6f-eb9e088d37c4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "01ac777d-4999-4f2a-928b-68af20a2762d")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 14 "Net-(D5A-+)")
			(pintype "passive")
			(uuid "0be80d5e-4be8-44a6-8c69-f4c726e830a4")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "4b4a4db2-a4f4-4795-b61c-62ca3694bae9")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "B.Cu")
		(uuid "2dca24e0-809f-413b-8b2b-31db41382318")
		(at 36 57.3 -90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "VD6"
			(at 0.3 1.8 90)
			(layer "B.SilkS")
			(uuid "81fda0e7-c063-4d0d-9f81-87aff1511cda")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "MMSZ5234B"
			(at 0 -2.1 90)
			(layer "B.Fab")
			(uuid "a64010cc-3ccc-44b4-9ef8-f2b4dc4d6f95")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "01bccdc6-2a6b-4912-820d-9cbcd25b4cc9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "4189a9c1-974c-44a4-ab78-1c7f79b3a630")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "09f07162-83ca-4caa-b3af-c212a616c694")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/8017539211"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "81112c9b-2249-418a-8bac-255449080970")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/fe0be6af-69ee-4ac8-968b-3a233e80e3b4")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 1.65 1)
			(end -2.36 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a7daa6c7-5180-4463-9de7-c1a81660ccc7")
		)
		(fp_line
			(start -2.36 -1)
			(end -2.36 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "dbb44e48-67db-4395-b66b-a36fc4f7be56")
		)
		(fp_line
			(start 1.65 -1)
			(end -2.36 -1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "86524159-ed45-4a84-808f-5c8967a40489")
		)
		(fp_line
			(start 2.35 1.15)
			(end -2.35 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "c5e4fc1a-f11b-41ba-91f1-e02add43b7d5")
		)
		(fp_line
			(start -2.35 -1.15)
			(end -2.35 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "2d26cb05-c590-455b-a555-25cece3649d6")
		)
		(fp_line
			(start -2.35 -1.15)
			(end 2.35 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "7b23eb91-7c4d-45f4-b4ef-985e2bed948c")
		)
		(fp_line
			(start 2.35 -1.15)
			(end 2.35 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "4e758897-192a-48d7-a7a7-7706280d0484")
		)
		(fp_line
			(start -1.4 0.900001)
			(end -1.4 -0.900001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "706de482-e021-4a80-8d75-cb91aa99e327")
		)
		(fp_line
			(start 1.4 0.900001)
			(end -1.4 0.900001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "d6d465fe-ebcd-4d91-861d-e2d025ea9f53")
		)
		(fp_line
			(start -0.35 0.55)
			(end -0.349999 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "709d4346-0b6c-444e-b3b9-669da337448e")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.349999 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "87a284f1-d765-4464-8e71-cc8f5441886a")
		)
		(fp_line
			(start -0.349999 0)
			(end -0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "9b73fcd0-c1e7-4ab3-b252-8eeece5612ac")
		)
		(fp_line
			(start -0.349999 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "b52eefbe-52d8-465d-b86e-d14acace3a07")
		)
		(fp_line
			(start 0.75 0)
			(end 0.25 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f3e955aa-3484-4336-a51f-10e1d4030ff2")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "32241511-31e6-4429-977d-e4178fb307d9")
		)
		(fp_line
			(start -0.35 -0.55)
			(end -0.349999 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "1d218d98-3c5f-47c9-b276-d2a48e7e99f0")
		)
		(fp_line
			(start -1.4 -0.900001)
			(end 1.4 -0.900001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "7f0e045c-76c4-492a-af84-5dbeab6f68ad")
		)
		(fp_line
			(start 1.4 -0.900001)
			(end 1.4 0.900001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "e52fcbe0-4c19-4c32-ada6-4b333f06ca35")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.000001 90)
			(layer "B.Fab")
			(uuid "64151cf2-b04e-4591-a937-8daa5a996d71")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 14 "Net-(D5A-+)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "b115bb5a-fa6c-48f0-af07-0fdb6101d834")
		)
		(pad "2" smd roundrect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "49d06f00-c8d4-447f-9aad-43aee4d0188b")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_2x08_P2.54mm_Horizontal"
		(layer "B.Cu")
		(uuid "2e2e6564-d893-4885-88ea-c1db17a1f2a3")
		(at 71.875 56.375 90)
		(descr "Through hole angled socket strip, 2x08, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated")
		(tags "Through hole angled socket strip THT 2x08 2.54mm double row")
		(property "Reference" "X1"
			(at -5.325 -19.975 -90)
			(layer "B.SilkS")
			(uuid "6a836d4f-7f34-4913-92fb-cb1db6f54f79")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "PBD-16R"
			(at -5.65 -20.55 -90)
			(layer "B.Fab")
			(uuid "44ccbf32-39ff-4507-b7eb-b8cf0e2b1fc1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Connector_PinSocket_2.54mm:PinSocket_2x08_P2.54mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "f5f35c36-4032-4efa-bf6c-ba08fbef9e78")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "9c0659e0-a925-4c14-8f74-6454a6eafdcb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Generic connector, double row, 02x08, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "db36b12d-c336-48ca-93dc-056913d0d034")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Label" "БСВ-33"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "ebe5dd14-d650-45e5-a843-af2dc95c34d2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Alternative" "KLS1-208-2-16-R"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "0b4c94b4-a359-44d4-8444-ddb2549905bf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/8871857750"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "927d3361-0d89-489e-b35b-e1f2134d86b6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(path "/5559ce43-6439-4b89-87ba-931c32012e51")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -4.000001 -19.11)
			(end -6.5 -19.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c3bbf3fe-2bf1-45e9-aa09-3ed9f87e985c")
		)
		(fp_line
			(start -4.000001 -19.11)
			(end -4 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b0bc2e71-66f3-4bd3-96fb-601ebd79aa45")
		)
		(fp_line
			(start -1.05 -18.14)
			(end -1.49 -18.14)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a9fcdbdc-8957-47cf-8ad7-f238914a1faf")
		)
		(fp_line
			(start -3.59 -18.14)
			(end -4 -18.14)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9bf5107b-1924-4db1-ab6d-56b62e33afa1")
		)
		(fp_line
			(start -1.05 -17.42)
			(end -1.49 -17.42)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f8d7afe0-85d9-40aa-8dbf-87ec2ffb0690")
		)
		(fp_line
			(start -3.59 -17.42)
			(end -4 -17.42)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "19c68858-6a95-4967-8728-091e66da2e5d")
		)
		(fp_line
			(start -4 -16.51)
			(end -6.5 -16.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "815f8679-11f4-4850-8df5-d34d554435e8")
		)
		(fp_line
			(start -1.05 -15.6)
			(end -1.49 -15.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "51b9a494-04e3-4928-a195-5f68d84d775c")
		)
		(fp_line
			(start -3.59 -15.6)
			(end -4 -15.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a44aab3f-73c1-4572-9ebc-2c0e6b0ea039")
		)
		(fp_line
			(start -1.05 -14.88)
			(end -1.49 -14.88)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "fb573169-1823-4096-aaaa-a41e7eb98297")
		)
		(fp_line
			(start -3.59 -14.88)
			(end -4 -14.88)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "505202f4-ce4a-4262-bda5-8a8b93b0c614")
		)
		(fp_line
			(start -4 -13.97)
			(end -6.5 -13.97)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "e3f365b4-45f9-44a4-8fe1-57d61ec10f11")
		)
		(fp_line
			(start -1.050001 -13.06)
			(end -1.490001 -13.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6bbd1983-19b6-4d84-9671-2c244281ffee")
		)
		(fp_line
			(start -3.59 -13.06)
			(end -4.000001 -13.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "5a3530da-8803-4373-a703-281dacfc5a39")
		)
		(fp_line
			(start -1.05 -12.34)
			(end -1.49 -12.34)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "edd7aa51-d274-4793-bd87-25e1abd8bc7c")
		)
		(fp_line
			(start -3.59 -12.34)
			(end -4 -12.34)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "bb38f7d0-4ce8-49b9-afeb-6d2e08d43bff")
		)
		(fp_line
			(start -4.000001 -11.43)
			(end -6.5 -11.43)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "e6b62afa-cf11-4a26-aafc-cfdf4f1f4106")
		)
		(fp_line
			(start -1.05 -10.52)
			(end -1.49 -10.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f6253342-ab39-4c2c-ba56-f05d0c325f78")
		)
		(fp_line
			(start -3.59 -10.52)
			(end -4 -10.52)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "32dc91a3-5f7c-4c98-9428-86194ee823ec")
		)
		(fp_line
			(start -1.050001 -9.8)
			(end -1.490001 -9.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "3b6c79e6-3b6a-4e7a-b9a0-ac299064d7b2")
		)
		(fp_line
			(start -3.59 -9.8)
			(end -4.000001 -9.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "e4782e5e-28f2-4c27-9158-4718e3a015fd")
		)
		(fp_line
			(start -4 -8.89)
			(end -6.5 -8.89)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "3ca97099-dacf-4998-bd05-212c32fc6a31")
		)
		(fp_line
			(start -1.05 -7.98)
			(end -1.49 -7.98)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "276444ca-7c7e-4f69-b281-0e72e0aa5f49")
		)
		(fp_line
			(start -3.59 -7.98)
			(end -4 -7.98)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "e948f9f7-6fc9-40c6-9603-849af4105069")
		)
		(fp_line
			(start -1.05 -7.26)
			(end -1.49 -7.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "e878543e-a9c8-4694-a9aa-23c088bfb397")
		)
		(fp_line
			(start -3.59 -7.26)
			(end -4 -7.26)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6dae5f32-a20e-4373-a7d3-a1627ef21293")
		)
		(fp_line
			(start -4 -6.35)
			(end -6.5 -6.35)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "1582dfe8-deba-4bc3-bbd0-a66a22c3586e")
		)
		(fp_line
			(start -1.05 -5.44)
			(end -1.49 -5.44)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "fb5785f3-1b20-4216-a036-5f49d86bc1df")
		)
		(fp_line
			(start -3.59 -5.44)
			(end -4 -5.44)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c0173785-b8f6-4aa9-88e2-670ce9b651f0")
		)
		(fp_line
			(start -1.05 -4.72)
			(end -1.49 -4.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "aa8b35cd-71b1-46ee-858c-b781cfe70b5e")
		)
		(fp_line
			(start -3.59 -4.72)
			(end -4 -4.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9299c2eb-4d04-43c6-8a6b-b3fee378928b")
		)
		(fp_line
			(start -4 -3.81)
			(end -6.5 -3.81)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "df24497b-e3a5-4b11-9a5c-ea25861f1d28")
		)
		(fp_line
			(start -1.05 -2.9)
			(end -1.49 -2.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4ad79bd1-b329-499c-b78d-cec9165dbe74")
		)
		(fp_line
			(start -3.59 -2.9)
			(end -4 -2.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "7be10154-dddd-4c13-9a75-a43727983ab4")
		)
		(fp_line
			(start -1.05 -2.18)
			(end -1.49 -2.18)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6d6ce83d-b23f-465d-8c87-a340e3cf1d37")
		)
		(fp_line
			(start -3.59 -2.18)
			(end -4 -2.18)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "fc6a6387-a513-4a28-b446-3eff65c875df")
		)
		(fp_line
			(start -4.000001 -1.27)
			(end -6.5 -1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f9b62b9b-9153-44a5-bb37-24a4c7f541e3")
		)
		(fp_line
			(start -4 -1.1519)
			(end -6.5 -1.1519)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "cc3cba69-b4f8-4e16-b520-dc5f14370df6")
		)
		(fp_line
			(start -4.000001 -1.033805)
			(end -6.5 -1.033805)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0fd1e531-0c66-414f-8d92-4af8a1df8b04")
		)
		(fp_line
			(start -4 -0.91571)
			(end -6.5 -0.91571)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6bb9705e-c06b-45b0-a648-e4f984f8ecf0")
		)
		(fp_line
			(start -4 -0.797615)
			(end -6.5 -0.797615)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "61dff16b-574c-475c-ba63-1556a2675c1c")
		)
		(fp_line
			(start -4 -0.67952)
			(end -6.5 -0.67952)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "59fb6f13-5092-48d5-95a0-5af733e5a7c0")
		)
		(fp_line
			(start -4.000001 -0.561425)
			(end -6.5 -0.561425)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c4800ee7-09ac-4de0-b70d-0f9ddfdbaf70")
		)
		(fp_line
			(start -4 -0.44333)
			(end -6.5 -0.44333)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "310b8adb-e28f-44ae-9922-623e37f21311")
		)
		(fp_line
			(start -1.11 -0.36)
			(end -1.490001 -0.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "877f9a8d-b57b-4444-8723-12cbc5925335")
		)
		(fp_line
			(start -3.59 -0.36)
			(end -4.000001 -0.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "7169148c-8289-402c-b692-7292f03078c7")
		)
		(fp_line
			(start -4 -0.325235)
			(end -6.5 -0.325235)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a96ad244-3071-4ef9-8178-b3464c2c5ab1")
		)
		(fp_line
			(start -4 -0.20714)
			(end -6.5 -0.20714)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d1ee5f82-0d4e-4a67-bc08-c45c727104cf")
		)
		(fp_line
			(start -4 -0.089045)
			(end -6.5 -0.089045)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "43280ff9-1079-4f13-bc16-a54f2fe87acf")
		)
		(fp_line
			(start 1.110001 0)
			(end 1.110001 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "61b5c091-df3c-4e8f-8dc4-17ea231556f2")
		)
		(fp_line
			(start -4.000001 0.02905)
			(end -6.5 0.02905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b0fffebe-0ada-46b2-8fea-b96ece56f618")
		)
		(fp_line
			(start -4 0.147145)
			(end -6.5 0.147145)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "abf8dfa7-b8f0-421c-b589-db0b9b2aeed5")
		)
		(fp_line
			(start -4 0.26524)
			(end -6.5 0.26524)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9eabcacf-a734-48ec-b0ec-bc4cc7d58643")
		)
		(fp_line
			(start -1.11 0.36)
			(end -1.490001 0.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "e460990a-8b1a-4595-8590-3dcfdd082c70")
		)
		(fp_line
			(start -3.59 0.36)
			(end -4.000001 0.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "19f1f48c-b9b1-4756-818c-730faf2eee7a")
		)
		(fp_line
			(start -4 0.383335)
			(end -6.5 0.383335)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "7aff6ea2-4d22-42d3-98c5-a0135614d80e")
		)
		(fp_line
			(start -4.000001 0.50143)
			(end -6.5 0.50143)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ad6c2cbe-f656-4154-a786-d3946fae9070")
		)
		(fp_line
			(start -4 0.619525)
			(end -6.5 0.619525)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6aa7f03f-9533-4a3e-bdec-f8e73a3cf41a")
		)
		(fp_line
			(start -4 0.73762)
			(end -6.5 0.73762)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0a846565-3806-4f6b-96cf-ee8bd39df447")
		)
		(fp_line
			(start -4 0.855715)
			(end -6.5 0.855715)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "147ea3a1-b6e1-4053-804c-8e11636a9dd5")
		)
		(fp_line
			(start -4 0.97381)
			(end -6.5 0.97381)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "d1aa76cb-0837-4d2f-8f8b-71b325af10ae")
		)
		(fp_line
			(start -4.000001 1.091905)
			(end -6.5 1.091905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "61e57474-f369-4f95-8073-9c6a894dbb14")
		)
		(fp_line
			(start -4 1.21)
			(end -6.5 1.21)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ac43d1b1-da56-413a-b404-57e751d98d59")
		)
		(fp_line
			(start 1.110001 1.33)
			(end 0 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6987866f-363b-4b7f-a059-3f6b391bf9f6")
		)
		(fp_line
			(start -4 1.33)
			(end -6.5 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4fe3ce7b-fbf0-48b9-98b2-6d3fa5746dc7")
		)
		(fp_line
			(start 1.8 -19.55)
			(end -13.05 -19.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "c25f4211-fa54-48dc-b4e4-7b3e9b2b833a")
		)
		(fp_line
			(start -13.05 -19.55)
			(end -13.05 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "eac66d85-40c8-4656-8e78-7f28179d9ac4")
		)
		(fp_line
			(start 1.8 1.8)
			(end 1.8 -19.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "c39ffea1-5193-4274-b711-3def7b2e4659")
		)
		(fp_line
			(start -13.05 1.8)
			(end 1.8 1.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "a9b25564-cf73-4ed9-a89d-6350658efef6")
		)
		(fp_line
			(start -4.06 -19.05)
			(end -4.06 0.300001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "aba3fc02-2b56-45e5-8764-2f4ca89576c7")
		)
		(fp_line
			(start -12.57 -19.05)
			(end -4.06 -19.05)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "6922b036-eb82-4a9e-a3e9-52c72b0da648")
		)
		(fp_line
			(start 0 -18.080001)
			(end -4.06 -18.08)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "0c3de842-e019-41b2-a860-2d87c805d4f3")
		)
		(fp_line
			(start 0 -17.480001)
			(end 0 -18.080001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "197b60d8-0da8-4524-a98e-3165505fbce1")
		)
		(fp_line
			(start -4.06 -17.48)
			(end 0 -17.480001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "04cfd3f9-1712-4d6f-9247-42f87d8bcd97")
		)
		(fp_line
			(start 0 -15.539999)
			(end -4.06 -15.54)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "6fdf9a41-4a82-485c-a2d0-f9f9668b875d")
		)
		(fp_line
			(start 0 -14.94)
			(end 0 -15.539999)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "172b070a-f43e-47cb-99a0-913beea35d0d")
		)
		(fp_line
			(start -4.06 -14.94)
			(end 0 -14.94)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "acde2023-252a-4b29-82a2-0ad35328993c")
		)
		(fp_line
			(start 0 -13)
			(end -4.06 -13)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "e8c03cf3-48e3-4c63-afde-e3b4dd32ed79")
		)
		(fp_line
			(start -4.06 -12.400001)
			(end 0 -12.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "40faf95d-ade4-46ae-837e-79cfc7a95776")
		)
		(fp_line
			(start 0 -12.4)
			(end 0 -13)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "28b05e57-d4b1-4b2d-835e-e48c89e8a49c")
		)
		(fp_line
			(start 0 -10.46)
			(end -4.06 -10.459999)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "476169b7-0c38-484e-a211-c9c9d3b9c652")
		)
		(fp_line
			(start 0 -9.86)
			(end 0 -10.46)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "46919496-1f7c-4fde-a11f-bffeb62de679")
		)
		(fp_line
			(start -4.06 -9.859999)
			(end 0 -9.86)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "efe37745-c2bf-430d-9b96-2953ae1dab7f")
		)
		(fp_line
			(start 0 -7.92)
			(end -4.06 -7.92)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "fab4b038-0d64-46df-824e-34830c751ad2")
		)
		(fp_line
			(start 0 -7.320001)
			(end 0 -7.92)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "83687f01-b53a-4dfd-a117-0f723a17a6d4")
		)
		(fp_line
			(start -4.06 -7.32)
			(end 0 -7.320001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "40f86dce-0417-4aaf-9936-7b7fc3eae283")
		)
		(fp_line
			(start 0 -5.379999)
			(end -4.06 -5.38)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "ebc8d423-391f-4339-8203-d52263f57a55")
		)
		(fp_line
			(start -4.06 -4.78)
			(end 0 -4.779999)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "fc95eb2d-a29a-4136-8d2c-58adbdb9b67e")
		)
		(fp_line
			(start 0 -4.779999)
			(end 0 -5.379999)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "a2af4cd4-2ba5-4391-a54d-ea82ed805c53")
		)
		(fp_line
			(start 0 -2.84)
			(end -4.06 -2.84)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f03a3fe0-4e7d-46c3-8645-050c406078a7")
		)
		(fp_line
			(start 0 -2.24)
			(end 0 -2.84)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "dae7a6b5-7487-49e1-807e-827f724d8108")
		)
		(fp_line
			(start -4.06 -2.24)
			(end 0 -2.24)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "db62140c-1fe8-46fd-ab97-482ad661e22e")
		)
		(fp_line
			(start 0 -0.3)
			(end -4.06 -0.300001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "a1200259-1c84-4dd3-b8cd-c8c9b4796205")
		)
		(fp_line
			(start 0 0.3)
			(end 0 -0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "e8ffcd3b-6e30-4545-8db7-c3b5650f176f")
		)
		(fp_line
			(start -4.06 0.300001)
			(end 0 0.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "90818b0d-8fe2-438a-9922-41e6c7dd4d5c")
		)
		(fp_line
			(start -4.06 0.300001)
			(end -5.03 1.270001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "bccbd493-5346-49c2-a6ac-c92a91187ef3")
		)
		(fp_line
			(start -12.57 1.27)
			(end -12.57 -19.05)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "14f19a87-1d8a-4794-bc94-333efa998d5a")
		)
		(fp_line
			(start -5.03 1.270001)
			(end -12.57 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c62f7870-0a27-4603-b466-e2bd0f844bfc")
		)
		(fp_text user "${REFERENCE}"
			(at -8.315 -8.89 0)
			(layer "B.Fab")
			(uuid "4098e149-2108-4075-9de8-0e891a3684f5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "X_HV_24V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "d437ecf7-8073-415d-9a58-26c6c7590bbf")
		)
		(pad "2" thru_hole oval
			(at -2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/X_UA_RDY")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "1e7446c6-581b-4552-8438-5614872ec043")
		)
		(pad "3" thru_hole oval
			(at 0 -2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "X_HV_15V")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "a2af638f-f016-4192-8e5c-f817dc573f2d")
		)
		(pad "4" thru_hole oval
			(at -2.54 -2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "X_Ua_MON")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "48606e85-73e3-40e1-ab23-86adaafa8228")
		)
		(pad "5" thru_hole oval
			(at 0 -5.079999 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "195dc8dc-f1fe-4936-9c8d-5ba07cb786b9")
		)
		(pad "6" thru_hole oval
			(at -2.54 -5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "X_Ua_CTRL")
			(pinfunction "Pin_6")
			(pintype "passive")
			(uuid "a05c6a20-27b7-4bda-b90a-fbf88b49d85d")
		)
		(pad "7" thru_hole oval
			(at 0 -7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "CONN")
			(pinfunction "Pin_7")
			(pintype "passive")
			(uuid "88a6bcca-1a24-4bd2-9d36-050692d0419b")
		)
		(pad "8" thru_hole oval
			(at -2.54 -7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "/X_XRAY_ON")
			(pinfunction "Pin_8")
			(pintype "passive")
			(uuid "bacb2a6c-041b-47f1-b740-b62869cb80e8")
		)
		(pad "9" thru_hole oval
			(at 0 -10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_9")
			(pintype "passive")
			(uuid "9a6759f9-951e-4b65-b1a4-a249f4504f05")
		)
		(pad "10" thru_hole oval
			(at -2.54 -10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "X_Ia_MON")
			(pinfunction "Pin_10")
			(pintype "passive")
			(uuid "e1ae523e-5036-4078-b2b5-5e782bbe0bf8")
		)
		(pad "11" thru_hole oval
			(at 0 -12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "GND")
			(pinfunction "Pin_11")
			(pintype "passive")
			(uuid "49889f27-6fc3-4154-b9ad-afb25132d714")
		)
		(pad "12" thru_hole oval
			(at -2.54 -12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "X_Ia_CTRL")
			(pinfunction "Pin_12")
			(pintype "passive")
			(uuid "7fc18dd1-a7d1-4dac-b3ae-e72c536de94c")
		)
		(pad "13" thru_hole oval
			(at 0 -15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "X_HV_ENABLE")
			(pinfunction "Pin_13")
			(pintype "passive")
			(uuid "75a7c385-f97c-4bb7-9795-1b772ec4bbfe")
		)
		(pad "14" thru_hole oval
			(at -2.54 -15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "/X_NO_LINK")
			(pinfunction "Pin_14")
			(pintype "passive")
			(uuid "9ca5c6a8-db77-4ea9-a19e-8321de8e0d62")
		)
		(pad "15" thru_hole oval
			(at 0 -17.780001 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "/X_OVERHEAT")
			(pinfunction "Pin_15")
			(pintype "passive")
			(uuid "709344a5-49e8-419e-9522-824502301360")
		)
		(pad "16" thru_hole oval
			(at -2.54 -17.78 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "/X_OVERLOAD")
			(pinfunction "Pin_16")
			(pintype "passive")
			(uuid "a8dd8dda-4afd-4f1d-bf6c-397416b6a96a")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x08_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "2e36a46c-860d-44ef-81f9-933d389557e9")
		(at 33.9 53.1 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C30"
			(at 0 -1.6 90)
			(layer "B.SilkS")
			(uuid "ffc62760-a862-4d8f-8c17-9e24f22ae638")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "0.1u"
			(at 0 -1.679999 90)
			(layer "B.Fab")
			(uuid "11dfad35-f018-48af-a191-80e81139ecf7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "91c82142-7476-4a85-b13b-2d3cd48955aa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "51f8d122-12cb-42f1-a570-47101cb723b1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "d82cba79-ef55-4f82-9aa3-366c9a966950")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/43780"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "790b5c51-c4ac-483d-a3bc-42177a25331b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/a6db7d78-1a8a-447c-806d-76fa5c068c05")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "25a5ddd2-f52a-4f8d-b4d0-c7ee6f28f2c2")
		)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4ac3b65e-e5c5-427f-a6cf-c4add3aebee7")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "e4a023a4-eadc-47f8-a554-38722c4ab615")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "65e9afcc-d60f-4c85-81db-f3972070a0c6")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "434f2145-29c1-4f92-9557-7b842d0bd9c8")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "964aa9f6-a44a-4984-a47a-75bd9ddd658e")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "9be8602c-4b02-4f55-bf85-1ea5434b7ae4")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "b0a8e729-0bbe-4294-b431-ba3da737e0d3")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "8d79760a-ae5d-4f62-bd91-7a03fbcee969")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "58419d19-1abc-4574-b379-239d58e1c68b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "9193e51e-eba5-46c7-98f6-cfaf364c4fd2")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 43 "Ua_MON")
			(pintype "passive")
			(uuid "b1e0dd91-dc31-4bf3-80fe-bb55792518d8")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "3ccda321-7653-4162-822d-c8868a6477bb")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "30b00c79-b23c-41cb-bcbb-a76351c0f643")
		(at 36.1 40.6 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at 0 2.649999 0)
			(layer "B.SilkS")
			(uuid "9d84f9d2-b456-4076-a7b7-3e2f201b0ae3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "100p"
			(at 0 -1.679999 0)
			(layer "B.Fab")
			(uuid "c88eb2e7-bb3f-4348-90e0-e14a8d0c63ec")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "4d76ef2a-8aad-44f7-916d-e53c2e2f379e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "8985eb28-f199-4e2d-946e-92fe7f742c2e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "3a3ab367-1ab7-439a-a3c1-c58dc82d0850")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "8a66b18f-cd42-40d9-a814-020a53aa3884")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/637c6c9a-abe7-49b5-a617-354adf1f1474")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f001b137-6e62-4ece-abbe-ee58fded8ff9")
		)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "88358162-f323-43e3-9b94-ade598fb01ff")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "8f9af985-a75a-4e70-8e7d-6f5d412f6acb")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "3ba9ef84-80cf-40cb-8c41-6a35332df545")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "ff4c0faa-dff0-4db2-8dbd-f1cfe9303d3d")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "9591b530-d541-44f1-b10f-cb3e0ebcde3a")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "4d967079-3a10-4ab9-a74f-65d1e5ddc751")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "54b48d6d-7c49-4c2d-bb0c-ee16d85b59e5")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f8e51690-74b9-448e-a610-09b44274de30")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "cde27e11-7383-4053-a794-82234dcd17f1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(uuid "ac981861-d22d-4af3-83c5-ba7e9d8d74cd")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 17 "Net-(D6B-+)")
			(pintype "passive")
			(uuid "c48006fd-46b2-4fff-b7ce-d294b12b2048")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "e618e2ca-dc2e-4fff-accc-7d72acc2ba5f")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "3d9f3b4b-273e-4a5b-b03b-98235978a012")
		(at 85.6 56 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at -0.1 -1.6 90)
			(layer "B.SilkS")
			(uuid "d84abe0b-2e7e-40be-b60a-fd3a0756fad8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "0.1u"
			(at 0 -1.679999 90)
			(layer "B.Fab")
			(uuid "df53f131-224d-4cce-b8f0-de029b92e868")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "a64b15aa-26b7-446a-80b4-53fe26d59593")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "d8ff7f31-3c8a-4289-af31-de51a4aea9c9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "04c7d5eb-0c71-42cb-b1cb-c1b31b69d721")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/43780"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "08053e2d-9f66-4146-9916-dee74b595fcb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/76fca6d4-328f-4b3f-8ed2-7212e0ab0120")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a766281e-1bf8-40f6-ba3a-42743aeea7ca")
		)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b68758ca-bde7-4201-9a98-4d78b550cec6")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "a00535d2-37de-46bf-abeb-bc0da54d5ba8")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "aa31368f-48b8-48f3-8117-8c755788f4cf")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "553d8c3b-e5dc-4b7d-a68f-80fcb2f8117e")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "5be95a5e-f615-48c6-8b51-1500fe9e7f29")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "132c4fc0-3854-460e-84cc-b4a7ced0706d")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "ffead588-0d9a-43cf-a98c-84d3f6594e8d")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "e204ad01-1d96-4f65-b5fe-90508415d343")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "0ef25bf9-a304-44d4-aa1c-f8b276d57fb1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "d6121ede-6cea-47a9-81d8-eca50cd1f51b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pintype "passive")
			(uuid "3464e759-f1af-4d60-862e-e71636e140e1")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "68119f48-0449-45d2-81ce-be4f2a161d3c")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(uuid "409a4af2-ca52-4e66-bd08-7229c6e53776")
		(at 106.6 44.1 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 1.65 90)
			(layer "B.SilkS")
			(uuid "4c7d1b69-d8a7-42c2-9de1-504c264f5665")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "10k"
			(at 0 -1.65 90)
			(layer "B.Fab")
			(uuid "a7724ffe-44ef-4a07-9a94-18947886ad08")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "d61cedc5-023a-4728-bd26-3109ace7de70")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "d0354af2-0356-444e-a9f8-b346ba3b0982")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "b37e4d15-2739-4725-9197-99bbb8e9ebbc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/7182783c-572b-48d9-a994-75f6244eb4d9")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.227064 0.735)
			(end -0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0b6b8194-8cc8-49ce-a8fd-ef4cd72f7510")
		)
		(fp_line
			(start 0.227064 -0.735)
			(end -0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "aada4544-fcc6-401f-beea-6386cfcb68d3")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "e1b4164e-e59c-4400-812d-fe5d7f224ac6")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "e0d935c0-896d-4ff6-9298-2d34c174dc10")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "5301a820-b5ff-4194-8a2e-09cc8d2acd65")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "e3bf4efc-1d45-405f-9053-77b12784e6e9")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "da9ad681-2a44-40cd-aabc-2795f588a199")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c434c2fc-387d-4277-83c5-a0a05ce05b5d")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "8841a8fa-d9b0-461a-8afe-05ee416d71dd")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "acb30964-5e9e-42ef-b5f2-ffb600d45511")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "03f93774-93b9-4151-9c0f-22db07ad3444")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 22 "TXEN")
			(pintype "passive")
			(uuid "187bb354-5b95-4e83-b474-9fcd8f08b202")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 4 "GND")
			(pintype "passive")
			(uuid "68eab1a4-3405-4ce5-87e4-d876d01676b5")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(uuid "43271314-832f-4027-952d-6c79a4639bbd")
		(at 55.7 47.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R19"
			(at 1 -1.6 0)
			(layer "B.SilkS")
			(uuid "a55155e1-11cf-4468-a896-9e7039320445")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "10k"
			(at 0 -1.65 0)
			(layer "B.Fab")
			(uuid "30ea832a-06be-45a4-9129-afef894d613f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "008b5b83-6bbf-4cad-8b2c-341667fada68")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "663b782c-c406-461f-8299-daed17bbfe81")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "315cf9bf-a4cb-4870-b428-2670e31a6f01")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/6856f579-c8f1-4122-847d-200a2e88597a")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.227064 -0.735)
			(end -0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "fe78127d-4945-469e-994a-0f731143918b")
		)
		(fp_line
			(start 0.227064 0.735)
			(end -0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9bdf607f-f2a2-43e5-bd52-99772452af97")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "38c07147-9bc6-4ade-aa92-eb3ef4fa8e64")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "acab8e9e-9aeb-496a-b710-3d7f9f845c62")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "0236ac98-0b01-41ae-bb3a-15db36ce1993")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "b4b03b7d-90fb-4ca5-ad66-e0be3ce1d6f1")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "26c068c6-adc7-40ac-90ae-39155f873647")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "def431e2-eeba-4a12-a486-d31296fca824")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "8c6ac971-927e-47bd-b5a2-cf2742c3a464")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "79bc0328-9942-40aa-9f12-6c565f990609")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(uuid "b60378cf-50ae-4469-8784-12fc40dba179")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 47 "HV_ENABLE")
			(pintype "passive")
			(uuid "3cf07a7a-401a-4e2b-a2e8-3e8bbd19e909")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 4 "GND")
			(pintype "passive")
			(uuid "b10d7353-1cae-4a6b-a76d-c2653c8e29d2")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(uuid "435e5482-0854-481b-91a6-c63e626c5eaa")
		(at 120.5 39.9)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 -1.6 0)
			(layer "B.SilkS")
			(uuid "f7bc3bd4-17de-4dcb-9db7-35b7cb772765")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "330"
			(at 0 -1.65 0)
			(layer "B.Fab")
			(uuid "10ce2447-b21c-496d-ac81-49e78ea57b2e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "3c6f5375-0c38-42f5-a987-f05e6e88a1c9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "d7d9b1f3-fbd7-4ce1-bbbb-71725409a81b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "ff850b4b-60d7-4660-b2ca-9efe2931628a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/5006503a-4cef-44fd-aadc-c27a01d791e2")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.227064 -0.735)
			(end -0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c01222b2-1fcf-4a60-b465-a2e53017669d")
		)
		(fp_line
			(start 0.227064 0.735)
			(end -0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "2f6dc3fa-834d-4a8a-9b52-4f714b2af414")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "29f3fbdf-8c1f-4af4-88cd-11db879c9910")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "430f2bc2-bc31-4406-9e4c-ac7768da42ab")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "e98143e2-1205-4892-9019-fa5a027faba1")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "23384eb8-7623-4df0-b1a7-892fe259f730")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "649b7c4a-8edd-4494-8aea-b22d5c7e6211")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "6c8e840b-205c-453a-b574-97aef172fb98")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "e39ac7ac-aa26-483b-a488-f76b15ed3c9b")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "b0a96ec1-67be-4bb5-8e4b-e2670bd9573a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(uuid "5289d5aa-d814-40d5-aac0-41ace77bca8c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 75 "Net-(HL3-K)")
			(pintype "passive")
			(uuid "7f994926-12cc-4226-90a2-d20ef227f517")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 4 "GND")
			(pintype "passive")
			(uuid "49c2d0bf-5e15-4c62-9477-12f721166319")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(uuid "462dec31-fd08-4a24-b525-07b1e03907cc")
		(at 75 51.7 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 -1.7 90)
			(layer "B.SilkS")
			(uuid "c964e90c-13a1-4fc7-b51c-59dbff90f57d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "680"
			(at 0 -1.65 90)
			(layer "B.Fab")
			(uuid "97b8243e-81fa-4099-bebd-2de77bca3ef8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "83d680f4-02c1-4f0e-aa20-d131d243ae53")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "a6949c41-588b-4012-8dc4-eb47555aee07")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "995d3bb7-08ba-4c91-b4cd-77138a2e3fa6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/e9a2694e-e043-4f72-b129-3c2bf7304ff4")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.227064 0.735)
			(end -0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ef7e1f61-170a-4663-9fbc-90eec05866c8")
		)
		(fp_line
			(start 0.227064 -0.735)
			(end -0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "15449ad8-1624-414d-8188-fde2a6de26e8")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "015c1af1-5904-4877-bbc7-d40b65a9cf9b")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "1113bbee-fe2f-4bd4-9995-94eb64a9cfc9")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "f6c075e1-ca5a-469a-9efd-7331adbee037")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "5d4c590c-d34f-4f7b-97dd-bf196088c617")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "3f4068f8-1449-46ad-81ef-fa7dcc6ccc6e")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "035a45ba-08f6-4e01-867c-f494ee08227a")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "40653cb8-174e-42fc-b66b-ae35ace0971a")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "2c462e0b-86a4-4f93-8a47-29589ae0d6b2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "3f9ebc73-cd85-4dc4-aa97-56e2e36a709d")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 76 "Net-(HL4-K)")
			(pintype "passive")
			(uuid "8617b357-639a-433b-8b54-114c8f2d5238")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 4 "GND")
			(pintype "passive")
			(uuid "6b7f6ab5-07db-4cc9-8e63-1a37085bb1a2")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "46ce41cc-5195-45a6-b75f-d5681b30a2be")
		(at 47.5 41.7)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 0.600001 -2.399997 0)
			(layer "B.SilkS")
			(uuid "f1a1cd6f-668c-4476-9977-f23b41cc205a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "100p"
			(at 0 -1.679999 0)
			(layer "B.Fab")
			(uuid "7cea99f5-f02e-4de8-af01-c72a069d643b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "e31cceb0-5454-4a44-b099-3fb88fed0e7d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "04c842e8-0145-48df-ba23-7e67e1dcbad3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "8db1ea2a-5393-4c20-9b68-c06367af4190")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "e686744e-61ba-4cdd-ae3d-7d4f813645ef")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/f55b1d74-33b0-46b6-874f-680421648dc6")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "5d2cf8b5-8af9-49ff-869f-a9c971cf76b9")
		)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "12a99c27-4520-498b-9a95-aff8f4382308")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "6dfd6440-f298-4f58-a4cd-8ccd1454683f")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "22a8a964-716f-43bc-854d-2887ac171b6f")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "532c95e4-0078-4a77-8b27-430a7ea9af88")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "9d06bf0c-de22-4058-8262-2e75047f64dc")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c666152b-679b-40cb-8499-5056e9f2f27f")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "312e9f97-8ff2-4153-8e4b-e11be4af29ce")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "16cf833f-2b46-4ad8-963e-b47cb6a0d0ee")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "2b2bc04a-76ff-45b7-adaa-e55dfddc608c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(uuid "f55ad49d-80c4-47a9-bb71-60661bafb850")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 16 "Net-(D6A-+)")
			(pintype "passive")
			(uuid "71e67ea7-ea45-4dac-823b-f31936c5c45e")
		)
		(pad "2" smd roundrect
			(at 0.949999 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "ec79f93e-df73-4180-b3ad-5fcabfdd20e4")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "483d1f40-a5c1-4fca-a708-394ebf14cc6e")
		(at 92.7 56.9 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 0 -1.700001 0)
			(layer "B.SilkS")
			(uuid "7d6c3f4b-2fcc-45a3-b15a-27d502d1b9b9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "0.1u"
			(at 0 -1.679999 0)
			(layer "B.Fab")
			(uuid "fe87083b-293a-45c9-8fe6-a668eacfbf49")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "7bce2730-961b-4e4b-83c6-7031d9f4a7f8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "0f5fe512-69cb-491d-bd00-0551ca10e28c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "f496f871-1e77-474e-b2ae-d4d353e13d6e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/43780"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "327e97b5-edd8-47de-932c-68676f6f8eae")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/125ab237-5e72-4e74-927f-3f6cb042e811")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "73cfeea8-d14c-4cf6-ab7d-330e4e06e977")
		)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "15df4c60-107b-4b78-ba39-4e43149f769a")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "ddc14d57-082a-426e-90f0-7a3efe4c7a50")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "5790e9f5-3c2c-46a8-aad4-36e29ca668e5")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "9071dfd3-eb42-4497-95bb-eb12324dcedd")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "c07155c2-67ab-467a-bf4f-3acc0f4e6072")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "6c88c317-66bc-4b61-a7ef-b5196ba51b5e")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "32954ca4-5899-4de4-898d-a3052556aaef")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "e4495832-5fee-4de8-82b3-01c8c2bb00ee")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "530bd3ee-463c-4f4f-b960-7bf4895f63cd")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(uuid "6b604b20-7b09-4a5c-8fd9-76d5208a8007")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pintype "passive")
			(uuid "c972b14e-73a7-4782-a022-0a988a4cff05")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "c0d646ab-adc0-4fab-9221-8732e31c6cc5")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "52d5ebf7-e445-4c52-b050-f91c9b91086e")
		(at 41.8 43.4)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C28"
			(at 0.049999 -1.7 0)
			(layer "B.SilkS")
			(uuid "d576c3cb-7a38-444b-b9dc-936034613fa2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "0.1u"
			(at 0 -1.679999 0)
			(layer "B.Fab")
			(uuid "08168295-03ba-4d3c-a68e-364051ff39dc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "c3d20783-86ea-404e-a6dc-77f0a5f52bca")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "d91c0f37-8c33-46e9-afcf-a1fab1e5475f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "88c470bd-4ebd-4652-8ab3-0ba5c22e2bd3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/43780"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "ba46d77f-e5a1-4c5e-8ea6-60fec00296de")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/dbd5d994-4a39-4ab3-aa91-c0289d248d79")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "418c5214-26ce-482f-8a58-4aac88980bd1")
		)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9525a4e5-3390-4a40-9c21-cb2ec4e0b4ef")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "1dd5a96e-20a4-4bb8-9b86-5d7c1b899181")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "cff6f64a-ecfa-40e1-91da-3d9acb97d0f9")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "57d56b57-08d9-43fb-a8bd-723f38f0ed5a")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "c5779a0d-7050-4c8a-8f8b-6fc14c232929")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "09e6a52d-968a-4d26-8459-b3decbdbd9ae")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "b1e97fe0-4c21-45a3-87c2-635cb928039f")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "1511f31a-066d-4f8b-afcc-e0e4165c5227")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "fc9b4a27-f0b9-4aa8-b6b5-cb1c74eb1ce1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(uuid "9fc961aa-5021-416d-97a0-64d10feb2e98")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 12 "+12VA")
			(pintype "passive")
			(uuid "33b3b435-ac32-40b5-b27c-20982fbc1e94")
		)
		(pad "2" smd roundrect
			(at 0.949999 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "5a3d76f8-152f-4c41-a647-a8f086b589ef")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Ecohim:Ecohim-logo_10x12mm"
		(layer "B.Cu")
		(uuid "5737a2dd-7446-4403-b165-3d137b20ed80")
		(at 76.9 42.5 180)
		(property "Reference" "G***"
			(at -0.3 -7.2 0)
			(layer "B.SilkS")
			(hide yes)
			(uuid "ec45358a-dff6-4fd8-ac01-23fdaac8f429")
			(effects
				(font
					(size 1.5 1.5)
					(thickness 0.3)
				)
				(justify mirror)
			)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
			(uuid "2ad33288-f5e3-4c2a-a577-0fb542475802")
			(effects
				(font
					(size 1.5 1.5)
					(thickness 0.3)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Ecohim:Ecohim-logo_10x12mm"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
			(uuid "14f55ce4-9f57-4241-8f95-73c6530f1d19")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
			(uuid "127cfcef-3442-407c-8de0-2bab66c313e2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
			(uuid "05f6d0cb-2dbd-4c6d-86bd-7d3343c30b87")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(fp_poly
			(pts
				(xy 1.480038 1.704832) (xy 1.651138 1.598408) (xy 1.791376 1.504383) (xy 2.025771 1.308802) (xy 2.224785 1.082627)
				(xy 2.352847 0.870868) (xy 2.38125 0.758005) (xy 2.308834 0.735784) (xy 2.119366 0.720069) (xy 1.865312 0.714375)
				(xy 1.349375 0.714375) (xy 1.349375 1.230313) (xy 1.355723 1.493086) (xy 1.372332 1.678918) (xy 1.394604 1.74625)
			)
			(stroke
				(width 0)
				(type solid)
			)
			(fill solid)
			(layer "B.SilkS")
			(uuid "04ed612e-6e3e-4ae6-9180-bb64b6ca5985")
		)
		(fp_poly
			(pts
				(xy -0.950323 -0.085154) (xy -0.657559 -0.100863) (xy -0.462728 -0.124061) (xy -0.396875 -0.150527)
				(xy -0.451806 -0.240918) (xy -0.591006 -0.388652) (xy -0.67745 -0.468027) (xy -0.911098 -0.636954)
				(xy -1.142735 -0.704884) (xy -1.292606 -0.711197) (xy -1.56365 -0.68051) (xy -1.806058 -0.60881)
				(xy -1.843474 -0.590645) (xy -2.035444 -0.443953) (xy -2.177463 -0.26169) (xy -2.2225 -0.12428)
				(xy -2.148353 -0.106601) (xy -1.946798 -0.092198) (xy -1.649171 -0.082613) (xy -1.309688 -0.079375)
			)
			(stroke
				(width 0)
				(type solid)
			)
			(fill solid)
			(layer "B.SilkS")
			(uuid "73ec39c0-73bd-406b-94da-0993d721b302")
		)
		(fp_poly
			(pts
				(xy -2.12752 -2.46838) (xy 0.000771 -4.643437) (xy 2.10011 -2.500312) (xy 4.19945 -0.357187) (xy 4.534283 -0.689475)
				(xy 4.869116 -1.021763) (xy 2.423989 -3.527131) (xy 1.914934 -4.048463) (xy 1.441236 -4.533074)
				(xy 1.014134 -4.969504) (xy 0.644867 -5.346293) (xy 0.344673 -5.651978) (xy 0.124792 -5.875101)
				(xy -0.003537 -6.0042) (xy -0.032924 -6.0325) (xy -0.088919 -5.977685) (xy -0.242739 -5.821903)
				(xy -0.481691 -5.578146) (xy -0.793078 -5.259404) (xy -1.164206 -4.87867) (xy -1.582379 -4.448936)
				(xy -1.952584 -4.067968) (xy -2.427649 -3.578169) (xy -2.889964 -3.10035) (xy -3.322086 -2.652622)
				(xy -3.706576 -2.253098) (xy -4.025993 -1.91989) (xy -4.262895 -1.671108) (xy -4.360513 -1.567393)
				(xy -4.860568 -1.031349) (xy -4.55819 -0.662336) (xy -4.255811 -0.293323)
			)
			(stroke
				(width 0)
				(type solid)
			)
			(fill solid)
			(layer "B.SilkS")
			(uuid "d82bf06a-acef-45ad-96c7-f8a2d1a6c02c")
		)
		(fp_poly
			(pts
				(xy 1.567704 4.345864) (xy 2.036713 3.864167) (xy 2.52687 3.360991) (xy 3.010404 2.864826) (xy 3.459543 2.404165)
				(xy 3.846517 2.007501) (xy 4.078576 1.769825) (xy 5.024803 0.801211) (xy 2.541171 -1.742519) (xy 2.026516 -2.268388)
				(xy 1.545446 -2.757551) (xy 1.109346 -3.198604) (xy 0.729599 -3.580145) (xy 0.417592 -3.89077) (xy 0.184708 -4.119076)
				(xy 0.042332 -4.253661) (xy 0.001584 -4.28625) (xy -0.063722 -4.231225) (xy -0.228278 -4.073751)
				(xy -0.480699 -3.825227) (xy -0.809602 -3.497053) (xy -1.203602 -3.100629) (xy -1.651315 -2.647354)
				(xy -2.141357 -2.148629) (xy -2.539142 -1.742068) (xy -2.851604 -1.422135) (xy -1.666875 -1.422135)
				(xy -1.643621 -1.633122) (xy -1.585472 -1.763477) (xy -1.567657 -1.776126) (xy -1.383047 -1.800117)
				(xy -1.106322 -1.774033) (xy -0.792471 -1.707479) (xy -0.496483 -1.610063) (xy -0.416931 -1.57509)
				(xy -0.053104 -1.331981) (xy 0.277253 -0.985658) (xy 0.52547 -0.59093) (xy 0.586012 -0.445662) (xy 0.637042 -0.307082)
				(xy 0.670573 -0.247403) (xy 0.690587 -0.283807) (xy 0.701069 -0.433478) (xy 0.706001 -0.713598)
				(xy 0.708108 -0.972343) (xy 0.714375 -1.825625) (xy 1.031875 -1.825625) (xy 1.349375 -1.825625)
				(xy 1.349375 -0.9525) (xy 1.349375 -0.079375) (xy 2.2225 -0.079375) (xy 2.616459 -0.072475) (xy 2.904756 -0.053004)
				(xy 3.067104 -0.022807) (xy 3.095625 0) (xy 3.017968 0.029809) (xy 2.791648 0.053101) (xy 2.426639 0.069348)
				(xy 1.932912 0.078022) (xy 1.597129 0.079375) (xy 0.098634 0.079375) (xy -0.004369 -0.169295) (xy -0.254312 -0.600277)
				(xy -0.589059 -0.905998) (xy -0.995418 -1.076908) (xy -1.305746 -1.11125) (xy -1.666875 -1.11125)
				(xy -1.666875 -1.422135) (xy -2.851604 -1.422135) (xy -4.144595 -0.098229) (xy -2.445082 -0.098229)
				(xy -2.391667 -0.226085) (xy -2.299939 -0.381646) (xy -2.035823 -0.674295) (xy -1.691725 -0.849654)
				(xy -1.301591 -0.900988) (xy -0.899366 -0.821558) (xy -0.663295 -0.706459) (xy -0.490076 -0.554839)
				(xy -0.321526 -0.338613) (xy -0.198061 -0.116922) (xy -0.15875 0.03184) (xy -0.233471 0.048647)
				(xy -0.43903 0.062844) (xy -0.74752 0.073279) (xy -1.131038 0.0788) (xy -1.309688 0.079375) (xy -1.783082 0.077795)
				(xy -2.115523 0.067529) (xy -2.324806 0.040293) (xy -2.428727 -0.012198) (xy -2.445082 -0.098229)
				(xy -4.144595 -0.098229) (xy -4.550616 0.3175) (xy -2.54 0.3175) (xy -2.461339 0.294208) (xy -2.228117 0.274787)
				(xy -1.844483 0.259355) (xy -1.314581 0.248029) (xy -0.642557 0.240925) (xy 0.167442 0.23816) (xy 0.277812 0.238125)
				(xy 1.104709 0.240341) (xy 1.794148 0.246911) (xy 2.341982 0.257718) (xy 2.744065 0.272644) (xy 2.996251 0.291575)
				(xy 3.094394 0.314391) (xy 3.095625 0.3175) (xy 3.016963 0.340793) (xy 2.783741 0.360214) (xy 2.400107 0.375646)
				(xy 1.870205 0.386972) (xy 1.198181 0.394076) (xy 0.388182 0.396841) (xy 0.277812 0.396875) (xy -0.549085 0.39466)
				(xy -1.238524 0.38809) (xy -1.786358 0.377283) (xy -2.188441 0.362357) (xy -2.440627 0.343426) (xy -2.53877 0.32061)
				(xy -2.54 0.3175) (xy -4.550616 0.3175) (xy -4.860702 0.635) (xy -2.460625 0.635) (xy -2.381978 0.611576)
				(xy -2.148852 0.59207) (xy -1.765477 0.576603) (xy -1.236078 0.565296) (xy -0.564883 0.558268) (xy 0.243882 0.555642)
				(xy 0.319012 0.555625) (xy 3.098649 0.555625) (xy 3.046186 0.773907) (xy 2.898229 1.195666) (xy 2.6572 1.574491)
				(xy 2.300633 1.940129) (xy 1.960475 2.211388) (xy 1.640336 2.478461) (xy 1.447595 2.724917) (xy 1.360342 2.984068)
				(xy 1.349375 3.14048) (xy 1.331186 3.265141) (xy 1.247006 3.320537) (xy 1.052414 3.333711) (xy 1.031875 3.33375)
				(xy 0.714375 3.33375) (xy 0.713599 2.043907) (xy 0.712824 0.754063) (xy 0.524736 1.150938) (xy 0.377565 1.431187)
				(xy 0.215037 1.65955) (xy 0.001507 1.87567) (xy -0.298671 2.119192) (xy -0.443055 2.227296) (xy -0.758974 2.494748)
				(xy -0.945774 2.746751) (xy -1.02525 3.017109) (xy -1.031875 3.14048) (xy -1.050064 3.265141) (xy -1.134244 3.320537)
				(xy -1.328836 3.333711) (xy -1.349375 3.33375) (xy -1.666875 3.33375) (xy -1.666875 2.971345) (xy -1.627815 2.611621)
				(xy -1.498114 2.302) (xy -1.258989 2.015274) (xy -0.891657 1.724232) (xy -0.733291 1.618861) (xy -0.47089 1.418906)
				(xy -0.239177 1.187711) (xy -0.071387 0.963588) (xy -0.000754 0.784849) (xy -0.000297 0.773907)
				(xy -0.075064 0.753506) (xy -0.28159 0.736118) (xy -0.592895 0.723048) (xy -0.981998 0.715602) (xy -1.230313 0.714375)
				(xy -1.72604 0.709399) (xy -2.104546 0.695028) (xy -2.352837 0.6721) (xy -2.45792 0.641455) (xy -2.460625 0.635)
				(xy -4.860702 0.635) (xy -5.023912 0.802113) (xy -4.860207 0.969792) (xy -2.329647 0.969792) (xy -2.320667 0.924448)
				(xy -2.249471 0.8961) (xy -2.092867 0.880758) (xy -1.827664 0.874432) (xy -1.43067 0.873133) (xy -1.352168 0.873125)
				(xy -0.967763 0.877769) (xy -0.648061 0.890477) (xy -0.422492 0.909413) (xy -0.320486 0.932742)
				(xy -0.3175 0.93765) (xy -0.369999 1.028252) (xy -0.501235 1.176498) (xy -0.555545 1.230236) (xy -0.845845 1.413706)
				(xy -1.196938 1.496859) (xy -1.565695 1.484495) (xy -1.908987 1.381414) (xy -2.183683 1.192416)
				(xy -2.299602 1.036123) (xy -2.329647 0.969792) (xy -4.860207 0.969792) (xy -4.078698 1.770275)
				(xy -3.756735 2.100097) (xy -3.351659 2.515127) (xy -2.891209 2.986937) (xy -2.403129 3.487102)
				(xy -1.915159 3.987195) (xy -1.565212 4.345864) (xy 0.00306 5.953288)
			)
			(stroke
				(width 0)
				(type solid)
			)
			(fill solid)
			(layer "B.SilkS")
			(uuid "60104f1a-515b-42ed-9888-d8d76e0cce37")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "B.Cu")
		(uuid "5d5c5cd0-255c-4969-8bcf-fb09e1f3395a")
		(at 55.7 50.662499 -90)
		(descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "D7"
			(at 0 2.4 90)
			(layer "B.SilkS")
			(uuid "5dfb5175-3c71-447a-983b-fc74586a936b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "74LVC1G17"
			(at 0 -2.4 90)
			(layer "B.Fab")
			(uuid "6a9ca594-8c3d-4b41-b135-88d12a35e7f6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "65d80df7-6079-4ac3-8fd9-d904676e534e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc1g17.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "87a71806-3b3b-4fe3-94e7-76ca3589fced")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Single Schmitt Buffer Gate, Low-Voltage CMOS"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "368ccc1c-2be0-462c-a03c-ff434bb975aa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product/sn74lvc1g17dbvr-umw"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "12f99f75-d444-4c59-9e5a-2a445fffe964")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "SOT?23* SOT?553* Texas?R-PDSO-G5?DCK* Texas?R-PDSO-N5?DRL* Texas?X2SON*0.8x0.8mm*P0.48mm*")
		(path "/fb857d4a-e1a5-424f-b313-8c2d7b7afd0c")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.8 1.56)
			(end 0 1.560001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "fcb0a90d-676e-4a27-8c93-c5c988eab022")
		)
		(fp_line
			(start 0.8 1.56)
			(end 0 1.560001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "59a7024f-0099-4325-bb9a-c0f354fa07d6")
		)
		(fp_line
			(start -0.8 -1.56)
			(end 0 -1.560001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "7879a2f5-0af7-4019-89b1-f13146eb5eaf")
		)
		(fp_line
			(start 0.8 -1.56)
			(end 0 -1.560001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a9b22e37-d102-4738-a4a6-5e90565e2921")
		)
		(fp_poly
			(pts
				(xy -1.3 1.51) (xy -1.54 1.84) (xy -1.06 1.84) (xy -1.3 1.51)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "B.SilkS")
			(uuid "444f5611-d7be-4255-895d-465fb280c942")
		)
		(fp_line
			(start -2.049999 1.7)
			(end 2.049999 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "1440818e-a687-479f-8df1-ee06e9d6f9c2")
		)
		(fp_line
			(start 2.049999 1.7)
			(end 2.049999 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "98365a06-22d4-4b92-ae75-d0f5c9ff00f0")
		)
		(fp_line
			(start -2.049999 -1.7)
			(end -2.049999 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "b3f92b25-e50b-40b5-a77f-f15ac6320f37")
		)
		(fp_line
			(start 2.049999 -1.7)
			(end -2.049999 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "ea824304-a679-4d03-ac1e-09b0223e057e")
		)
		(fp_line
			(start -0.4 1.45)
			(end -0.8 1.050001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "517cbe23-238b-4b36-a0a3-3fb523c74055")
		)
		(fp_line
			(start 0.8 1.45)
			(end -0.4 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "ed1a6e55-f1b5-40bc-86fc-052fd3d4326c")
		)
		(fp_line
			(start -0.8 1.050001)
			(end -0.8 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "734e70dd-93f4-488c-9888-f0e2cba0dd7d")
		)
		(fp_line
			(start -0.8 -1.45)
			(end 0.8 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "9db65f0b-6181-41f4-ae5b-ddc3792f3591")
		)
		(fp_line
			(start 0.8 -1.45)
			(end 0.8 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "33d3297f-64ed-4b70-b8a0-bed42df6fdab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "43942dc8-8ed1-4184-b923-55f3c23f3dbe")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.1375 0.949999 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 69 "unconnected-(D7-NC-Pad1)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "33988f29-9fd1-49a3-8410-64289790d349")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 47 "HV_ENABLE")
			(pintype "input")
			(uuid "12ca8386-bad0-4515-8c38-91d346f3f588")
		)
		(pad "3" smd roundrect
			(at -1.1375 -0.949999 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "67693f76-9223-4fb2-bb7f-ed0ea554fbde")
		)
		(pad "4" smd roundrect
			(at 1.1375 -0.949999 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 70 "X_HV_ENABLE")
			(pintype "output")
			(uuid "235d024b-a9bb-42da-b844-1e5c4409ea3a")
		)
		(pad "5" smd roundrect
			(at 1.1375 0.949999 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 6 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
			(uuid "1168e0dc-c8df-44b0-9993-2c7b7d313b3b")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "5dd74e79-6a31-4417-b6c1-ebbed74656a8")
		(at 89.5 40.5 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C26"
			(at 0 1.679999 90)
			(layer "B.SilkS")
			(uuid "865c3e86-e83a-438a-a41f-c8098a75ef02")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "100p"
			(at 0 -1.679999 90)
			(layer "B.Fab")
			(uuid "178706e4-71d7-47b0-a441-9dc5f02e4508")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "44bafe95-c149-455d-8956-d692b65cf5f5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "73d0b6d5-243c-4513-a804-5da7ad0a3f04")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "f5e9d1fe-43b6-4166-a230-4a06e9c424f4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "5182d233-20a7-44df-acbb-2c20c73e3b03")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/7e50fb04-d79c-43d3-b2c2-2d3630f84cb6")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c135440c-e35b-4223-b368-db31b4ce0514")
		)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "8c55d5e8-6bdf-4e84-bb2c-3dd81a8004f0")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "8c0abc88-1d6b-4505-8433-ea130b849e82")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "216e2491-a499-407e-bf9d-4759a475bf3b")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "4210342b-8de4-40ae-bebb-df5708189bc3")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "8361f262-b34a-488f-95d4-6368941e9e2f")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "d20813b9-9750-4ba9-8bb1-1f642eb416ff")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "55449267-687c-4a8a-84e9-3144e91a4226")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "4403057d-45d7-4f38-ae65-aee8ddbcc935")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "7311a0c9-2520-4faa-b029-fd50629d16a2")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "179e3dfe-afd9-40e2-991b-6fc9d52071e7")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 19 "HV_15V")
			(pintype "passive")
			(uuid "d5dab49f-8c7b-45aa-8b44-ccad1bbe0388")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "b8af466a-e13e-4230-afe4-b905a752d923")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(uuid "62f4495d-f6c0-46d5-8214-5d46f119c5e6")
		(at 120.5 44.9)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 -1.6 0)
			(layer "B.SilkS")
			(uuid "ac244ff7-e7ae-4abf-8388-6c00d21ba14b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "1k"
			(at 0 -1.65 0)
			(layer "B.Fab")
			(uuid "ca4ce8c5-2e56-43a3-afed-2030a73cc558")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "3af689e5-5c8b-47c7-97cb-9df1cbfe4799")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "b04f4d86-44be-4d3f-9971-3ac61b6a5e28")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "416fb397-301c-44c5-a291-b90a5703ec94")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/633cb51b-f0e2-4d94-a7f0-dd06da593eb5")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.227064 -0.735)
			(end -0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "811e6acd-8460-421b-9fdb-1f4c5b51509f")
		)
		(fp_line
			(start 0.227064 0.735)
			(end -0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6ea2d74b-29a8-4ab2-9cb2-8f3dfe5f3de9")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "b0479ead-e5eb-4f3b-bcc4-5cfcf3c45035")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "c6536c5d-530a-4260-8ae4-c949882bdb52")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "a539502f-8444-46a5-8e48-f003ab0900f6")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "7bc19f26-b484-4f89-a4cf-6161fd376e75")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "53f04c84-1bf6-41b4-87db-1b8eaf249996")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "bc06399d-d8fc-48a7-af2e-b4cae6120a66")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "533de615-f73e-4e99-a700-6cee8557ddae")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "248a0f5e-95c9-4d67-840a-7d3362cd0ac8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(uuid "2c028e22-8536-43ce-850e-73953257aabb")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 72 "Net-(HL1-K)")
			(pintype "passive")
			(uuid "3a938e9a-a923-47d9-9ddb-2b83cdc8a9f8")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 4 "GND")
			(pintype "passive")
			(uuid "20a91ce0-2fdb-4281-a8cd-fba85024499e")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(uuid "64eaa4fd-ceb8-4ee5-9841-0ffdbf357699")
		(at 87.5 40.5 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at -3.122651 0.48985 90)
			(layer "B.SilkS")
			(uuid "b7954f9a-6686-4cd3-bebb-ac2b7775eb8f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "15k"
			(at 0 -1.65 90)
			(layer "B.Fab")
			(uuid "c440f9ad-c649-4dfa-b42c-842130cd752c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "e3c1f349-585e-42be-a462-d980bf399e69")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "43d388b2-f9d1-4cad-9d93-74cb46fb28c4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "439ae392-c03d-4a2f-b158-f086e8c48e54")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/0e481519-fc35-435c-8774-2641d70ab406")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.227064 0.735)
			(end -0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c6dae0c1-0a5b-4e88-a51d-3f89ead72a77")
		)
		(fp_line
			(start 0.227064 -0.735)
			(end -0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "46e42dce-398c-4f4d-8f89-57fdc9731428")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "a099c81c-f67d-4a9a-972b-ffc52f4e3a9d")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "81058939-e3ae-4fa6-aa75-1c33c4b0fe99")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "77f56978-d7b9-4c12-82a3-d39910c2e435")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "40acacb3-f385-4986-adfa-10b335210275")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "d57b5010-babf-48ad-99f0-e6585f0cd12f")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "26470dab-a311-42e3-baed-7fa93d4def9b")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "1863cadc-91cf-4d30-8f2f-da0b39c2c3f9")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "9c562cf9-61ff-41d8-b696-0af827ee3eeb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "6f643850-6b42-4ad3-9c17-d671976e60dd")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 19 "HV_15V")
			(pintype "passive")
			(uuid "9503b106-9e73-4d54-8720-cb6e19a08ab6")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 4 "GND")
			(pintype "passive")
			(uuid "d400ae66-14cf-48c0-b878-69509bf04c83")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_1210_3225Metric"
		(layer "B.Cu")
		(uuid "68d1da9e-7b9c-49f1-a66b-1daa8b21d0c6")
		(at 67.4 41.4 180)
		(descr "Inductor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L1"
			(at 0 2.279999 360)
			(layer "B.SilkS")
			(uuid "8c1ab018-5a76-49ce-a7c0-f5e95b49473e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "4u7"
			(at 0 -2.279999 360)
			(layer "B.Fab")
			(uuid "d01ffa73-9830-4312-88a5-327bd965f30c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Inductor_SMD:L_1210_3225Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "ba594a1d-d6f0-46a6-bb0d-c888e43cbef1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "fa6d5a0d-a7ad-45f8-ab6f-022e87d94390")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "227eee40-f21e-402e-ad81-add9f24c6230")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product/lqh32mn4r7k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "3c5d3832-60d7-4b4d-bc62-f90d8003898f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Alternative" "LQH31MN4R7K"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "b2dc28c6-06ee-4bda-9148-4851d2b8794f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(path "/97cd8039-5d22-48f7-a985-67fd5b81767c")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.602064 1.36)
			(end -0.602064 1.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "8120ba7b-d3a9-4452-9673-b841fd37ac12")
		)
		(fp_line
			(start 0.602064 -1.36)
			(end -0.602064 -1.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "091ea863-8cb2-48da-bcf8-dadfaf1e278f")
		)
		(fp_line
			(start 2.28 1.58)
			(end -2.28 1.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "c0e46c88-154c-4b92-99ba-f9f271bb5510")
		)
		(fp_line
			(start 2.28 -1.58)
			(end 2.28 1.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "c46f6f96-5919-4f98-88c6-e7a2713a4434")
		)
		(fp_line
			(start -2.28 1.58)
			(end -2.28 -1.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "14a7e2d6-39f3-443c-81e0-5ecef2fcfd32")
		)
		(fp_line
			(start -2.28 -1.58)
			(end 2.28 -1.58)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "c380f60e-7551-4867-9f90-c17995dda8fd")
		)
		(fp_line
			(start 1.6 1.25)
			(end -1.6 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "601d55ed-c218-4906-afd8-b7c47c69774e")
		)
		(fp_line
			(start 1.6 -1.25)
			(end 1.6 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "b13e36db-b980-4c44-add3-61e22c17dee9")
		)
		(fp_line
			(start -1.6 1.25)
			(end -1.6 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "7520adf6-26c1-4a36-8284-225cf47ff71e")
		)
		(fp_line
			(start -1.6 -1.25)
			(end 1.6 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "1ef5dcea-77a0-475f-b37d-a1f47d9a118e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "B.Fab")
			(uuid "66738674-c6f1-4f03-8e1d-339d0170d546")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.399999 0 180)
			(size 1.25 2.65)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.2)
			(net 5 "+12V")
			(pintype "passive")
			(uuid "20d6b9a1-b987-48ff-b1f8-fecbadcd3292")
		)
		(pad "2" smd roundrect
			(at 1.399999 0 180)
			(size 1.25 2.65)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.2)
			(net 12 "+12VA")
			(pintype "passive")
			(uuid "af50bcd8-9c93-4667-a5ae-3810d6f7124b")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(uuid "92e6b973-5042-467e-8f63-dda0cec6087a")
		(at 47.5 43.7 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R20"
			(at -0.2 -1.600002 0)
			(layer "B.SilkS")
			(uuid "1e93fa28-cee6-4de2-88a8-27f749ef18bb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "10k"
			(at 0 -1.65 0)
			(layer "B.Fab")
			(uuid "e8c0bf2a-b8bd-49fe-98a9-212929b1a8e4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "9a5ec9e3-33b1-4b82-bdba-d8639b53b49e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "2e720fdd-44e7-4884-9285-9f604f0bc32e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "19355f51-3cb2-4a58-b8a3-c7cd498e335a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/0249c9da-9799-495e-8f66-57bd892d1da5")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.227064 0.735)
			(end -0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "43f36c8e-96da-49c9-b405-7cd11f999a1e")
		)
		(fp_line
			(start 0.227064 -0.735)
			(end -0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4ed7a3f6-8821-42fb-8d5d-2cd382b5cdde")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "c2cf6197-b76c-445f-978d-4bb03075916a")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "633b0496-b8b0-4666-90e0-7a81bb25e7d6")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "6c7c648c-639a-4074-ac5c-5cc5f37fa82c")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "4553910e-ebab-41d6-ae3d-9f82a2dcf8e3")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "e6f1b8d5-3246-4cf7-af14-fb696f8c8fde")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "4e2f8f24-f0a4-4333-a42d-02d051c6a164")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "311e6abe-fc1d-42a2-9129-23b8636290e7")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "27ef41ba-02e3-4306-9721-806d32d6b9d1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(uuid "630ed2f1-6280-49a8-9aa1-2589a56446a3")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 4 "GND")
			(pintype "passive")
			(uuid "dadf0644-5665-4d7e-ba38-dbeb40c4f386")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 68 "Net-(D6A--)")
			(pintype "passive")
			(uuid "8953bdc4-10af-44d1-b0b0-2a9a79bb44b0")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(uuid "93b21eda-edc7-40dc-8f6c-ab3a5d639c06")
		(at 67.1 50.8 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 2.600001 0 90)
			(layer "B.SilkS")
			(uuid "df464d4a-53d7-42b5-ba98-661156e2121f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "10k"
			(at 0 -1.65 90)
			(layer "B.Fab")
			(uuid "4a8240e2-f09f-47c6-b698-f3cf9bf05b4d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "27d138b0-33f2-4b50-96fd-318a4349240e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "4ed2998c-ba97-4ae6-a8ca-ee6c6ef8cd56")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "520c796f-b48d-4fe6-91e0-ea0db6e4d032")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/486633e9-d64b-421a-8b6c-cc68477f1c49")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.227064 0.735)
			(end -0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ad159d32-9036-4bf9-8111-853eca40ae5c")
		)
		(fp_line
			(start 0.227064 -0.735)
			(end -0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f75dc8ee-2090-4091-a36c-26de854eb0d3")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "31075c8b-dad4-4ee7-92b1-12b59b08a472")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "cc9cf2c1-bdc4-4eaf-9966-5698a18af229")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "b0ce4c72-24ce-4b4e-8f89-ec24fb678344")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "249afee1-5f94-41a4-9092-ff3ffda0fa78")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "80c4edc7-c472-48f3-8357-e3c13fd090f8")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "3aabed1d-7003-4c3d-b283-f671d0eed2ab")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "67222cba-cecb-48f5-8415-bb3a9920ee15")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "6e7149c1-ffb4-44de-ab17-08b68152af8e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "9b3dcd5a-8654-45e1-86f2-583f6a170a29")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 3 "+3V3")
			(pintype "passive")
			(uuid "c2910dfc-0c06-4d71-9331-450a25c60fdc")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 54 "CONN")
			(pintype "passive")
			(uuid "04b005d2-63e1-450f-b32d-79b4cd762572")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "B.Cu")
		(uuid "9bd325dc-8afe-4ad7-bdfc-28fc4b437575")
		(at 45.6 58.5 -90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "VD7"
			(at 3.8 -1.2 90)
			(layer "B.SilkS")
			(uuid "6ed4a2fb-9219-4b80-80f2-1a57ca3858a4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "MMSZ5234B"
			(at 0 -2.1 90)
			(layer "B.Fab")
			(uuid "d7fdfc5b-44dc-4668-bda6-b1299c0f9572")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "aa22f21a-4f61-40ad-9786-c297542dc896")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "ce8016c1-a2af-4f6f-a709-b6a2e3d79970")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "fb2bbf67-a57a-4cc3-b201-ada50b5d7557")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/8017539211"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "0eeaeaba-323b-4b58-999d-9ffa54248b6c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(path "/d4c692fc-629b-4019-8b27-7d50ebd6f40e")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 1.65 1)
			(end -2.36 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "43f08088-3942-45c9-b921-2b0aa315a2bd")
		)
		(fp_line
			(start -2.36 -1)
			(end -2.36 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a777f079-8069-4574-b483-d9080b842e46")
		)
		(fp_line
			(start 1.65 -1)
			(end -2.36 -1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "95b315c4-6095-4a2f-9095-21d280f212df")
		)
		(fp_line
			(start 2.35 1.15)
			(end -2.35 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "f30e307c-bbfb-46b2-afae-7fc6cf8383fc")
		)
		(fp_line
			(start -2.35 -1.15)
			(end -2.35 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "6e88fa0a-33c1-43e3-8896-f7934f1be4b8")
		)
		(fp_line
			(start -2.35 -1.15)
			(end 2.35 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "f7eb5cab-039b-4ff8-bee7-2271934a8721")
		)
		(fp_line
			(start 2.35 -1.15)
			(end 2.35 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "1c327ef2-309e-43bb-bac4-a5951ae0162e")
		)
		(fp_line
			(start -1.4 0.900001)
			(end -1.4 -0.900001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "805ca2e8-2519-4b63-adb8-ef3153ae91ca")
		)
		(fp_line
			(start 1.4 0.900001)
			(end -1.4 0.900001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "81f04c59-7af1-4dd8-ad1f-696c8423b5a6")
		)
		(fp_line
			(start -0.35 0.55)
			(end -0.349999 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "a22d438e-3267-4955-9c72-b76ad3115fcf")
		)
		(fp_line
			(start 0.25 0.4)
			(end -0.349999 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "505532e9-d921-4aa3-bcb1-d0d7bcb1bf1e")
		)
		(fp_line
			(start -0.349999 0)
			(end -0.75 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c1c05b81-3354-452f-ba04-a11be876e422")
		)
		(fp_line
			(start -0.349999 0)
			(end 0.25 -0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "e9548c32-7326-4400-9f85-84ae38fb574c")
		)
		(fp_line
			(start 0.75 0)
			(end 0.25 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "46a5af22-fc23-4f70-b201-6ea456918a2a")
		)
		(fp_line
			(start 0.25 -0.4)
			(end 0.25 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "bfd99202-6dc1-48c3-8590-aad7f55667c2")
		)
		(fp_line
			(start -0.35 -0.55)
			(end -0.349999 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c77cb1a5-d632-415f-9f3f-236f69e62b0e")
		)
		(fp_line
			(start -1.4 -0.900001)
			(end 1.4 -0.900001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "47ed2e75-3d14-41c7-9958-2a6be053d0d3")
		)
		(fp_line
			(start 1.4 -0.900001)
			(end 1.4 0.900001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "930ace1b-a01a-4fb7-97aa-9958fe4cdec3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.000001 90)
			(layer "B.Fab")
			(uuid "11187718-36df-4b66-8c80-8d3a43563906")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(D5B-+)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "c8243cbd-068c-4144-8c64-d515db1f2cea")
		)
		(pad "2" smd roundrect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "A")
			(pintype "passive")
			(uuid "1452465c-55a3-422a-8ea6-2ab16e58a9e7")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "B.Cu")
		(uuid "a4dd4072-30aa-467e-b755-934ca1bfe240")
		(at 135.2 54.1 -90)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "D1"
			(at 0 -4.3 90)
			(layer "B.SilkS")
			(uuid "9fa58235-082b-449f-a85d-612effb84ace")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "LM1117MP-5.0"
			(at 0 -4.500001 90)
			(layer "B.Fab")
			(uuid "0d24d669-c7ee-4d75-87a9-df33728f27b0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "de080181-2fd8-4c94-b143-72e22580eb31")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm1117.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "3468698c-a131-4b7e-a307-7365dcad066c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "bc0e233e-112f-4b70-aff8-507d5a8627a1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Alternative" "AMS1117-5.0"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "a805bb38-c694-44c5-beb1-c4a4c93970fd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product/ams1117-5.0-umw"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "18737b0a-53b4-4d89-9e35-59cc6cd09862")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "SOT?223*")
		(path "/d1b45d3a-23ce-4974-8c14-9d9ca2d49966")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 1.91 3.41)
			(end -1.85 3.410001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9247d831-dfd8-4764-b056-3ecfd7c418eb")
		)
		(fp_line
			(start 1.91 2.150001)
			(end 1.91 3.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4077a47a-4ede-4cf6-bfd5-b581e54bf194")
		)
		(fp_line
			(start 1.91 -2.150001)
			(end 1.91 -3.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "30d01a86-7bdf-46f9-bdc4-614a3f785884")
		)
		(fp_line
			(start 1.91 -3.41)
			(end -1.85 -3.410001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b136d238-3ee7-443a-94c9-e35c44b7cd94")
		)
		(fp_poly
			(pts
				(xy -3.13 3.31) (xy -3.37 3.64) (xy -2.89 3.64) (xy -3.13 3.31)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "B.SilkS")
			(uuid "84c2d626-a5e3-4a93-bd66-0bdcbbea8398")
		)
		(fp_line
			(start -4.4 3.6)
			(end 4.4 3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "7363402e-fb1d-4d92-a400-8f109ba47d3a")
		)
		(fp_line
			(start 4.4 3.6)
			(end 4.4 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "0b0c596f-d16e-4c45-8ccc-bf5c02d4b1b7")
		)
		(fp_line
			(start -4.4 -3.6)
			(end -4.4 3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "af3ab5a9-cd4c-44f4-b94b-d246e948c030")
		)
		(fp_line
			(start 4.4 -3.6)
			(end -4.4 -3.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "42f2d751-ac4a-4f43-bed4-431cafa867ea")
		)
		(fp_line
			(start -0.85 3.35)
			(end -1.85 2.349999)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "31afd342-5aa6-441a-ab15-af13c8252dae")
		)
		(fp_line
			(start 1.85 3.35)
			(end -0.85 3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "fba46fda-1345-4440-9e23-7eabadb6c779")
		)
		(fp_line
			(start -1.85 -3.35)
			(end -1.85 2.349999)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "bd5dbc41-e11f-4b96-849e-7ca06760b1c8")
		)
		(fp_line
			(start 1.85 -3.35)
			(end 1.85 3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "2ef955f6-8f05-4523-822f-7896c2cd95e1")
		)
		(fp_line
			(start 1.85 -3.35)
			(end -1.85 -3.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c0bf38e0-fe09-43d2-8642-6c53c5ba354e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "B.Fab")
			(uuid "3c4f68fa-baca-4873-b658-3b96a5143e78")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -3.15 2.3 270)
			(size 2 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "da33926d-5206-44e8-9bd7-9803a4824d21")
		)
		(pad "2" smd roundrect
			(at -3.149999 0 270)
			(size 2 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 6 "+5V")
			(pinfunction "VO")
			(pintype "power_out")
			(uuid "017c083c-6eff-4047-ba61-856238b1eab8")
		)
		(pad "2" smd roundrect
			(at 3.149999 0 270)
			(size 2 3.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 6 "+5V")
			(pinfunction "VO")
			(pintype "power_out")
			(uuid "7762688f-2d8b-4eaf-9a58-5d2cafd8e29f")
		)
		(pad "3" smd roundrect
			(at -3.15 -2.3 270)
			(size 2 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+12V")
			(pinfunction "VI")
			(pintype "power_in")
			(uuid "a51e4b27-2cd3-4203-94e6-485fdef0785d")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "a8f7103e-fe49-4ea4-9cfb-a228658e2be5")
		(at 92.7 53.8 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at -3.2 0 0)
			(layer "B.SilkS")
			(uuid "9312221e-4cbe-4aec-a99c-a618e5a1edcf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "0.1u"
			(at 0 -1.679999 0)
			(layer "B.Fab")
			(uuid "599713de-f7e7-4e2d-b29e-1d54699b2c85")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "ff0da3c6-bc65-4652-9f42-2a712dd9d21b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "a869bfe8-fbe5-460d-b258-7630ab8a386c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "e0cccecb-1268-4a13-abd2-10249664b933")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/43780"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "2d064a9f-84d9-42d5-84a0-c884257dc6a0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/35b901a2-45a7-484e-a25d-958ba4a410c9")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "2433a76c-58ad-4a44-bdc1-e4345143b6b3")
		)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "8d10a0ce-782b-419f-a6d4-c81543c6fe52")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "b441fcfd-9ab9-4811-8129-49bdc9b19cbb")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "ec3d5892-b23e-420c-a991-3c6c74594378")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "065bd2fd-e2cb-4e8b-b711-2144d2a7a511")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "aa0b9723-d214-486b-87d2-0df3aaa733e0")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "19fd2b2b-3052-44ae-b094-7c57fb54f4a6")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "46bc1e4b-10de-4858-909b-473d67f64c61")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "0ebd9275-958e-4ee4-b73c-c66244dfcc64")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "65f51a5c-4686-454b-9587-4f1667255671")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(uuid "488acbda-827c-4471-bb4d-3806cfafbc05")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+3.3VA")
			(pintype "passive")
			(uuid "6c0e0ccc-bfb5-4083-a655-d1f58e8fe588")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "215e8ef4-64a5-46db-a094-0a276265f03c")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "c0ce710b-f00d-4bac-ac71-b26809f5a2fa")
		(at 47.7 54.3 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C31"
			(at 0 1.679999 90)
			(layer "B.SilkS")
			(uuid "fa3e73f2-2a56-41e0-980d-69d96469f6ba")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "0.1u"
			(at 0 -1.679999 90)
			(layer "B.Fab")
			(uuid "bb937194-d6ed-44c5-bfc0-6d49097cedcd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "bf31f5d8-9ae2-4273-8c87-e68faa309e07")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "3ac82320-a80c-4f79-99de-0360077c2039")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "67173cb6-5a2d-4a7b-adde-c8a59000c206")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/43780"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "2b444542-fdd6-445a-abba-0a2601766734")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/4600278e-481d-4670-9de3-ce4232b2f91e")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "4bdfeeb8-ca0e-4409-8f82-49f3a7155596")
		)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0ecc5065-f49a-46b5-abe1-dac0d7a8dadb")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "bf5c3a2d-1c13-456b-a58b-53ec696da50a")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "4b1c2fd6-f370-4035-ae55-bcf190677fb1")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "7c262572-f04c-45af-a797-4943d3b3dc13")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "b4e11c2a-64a3-46be-8068-08bde2ae6f88")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "439fb092-dbf8-4965-9a76-6341e4895d9a")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "8cf5fea1-75de-42a0-ac69-8c74b5eb2f6f")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "1f67991b-ebb3-4ca3-bd7c-da608fc3e0e5")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "723acae0-3eb3-4e5f-bdc4-8b633851a0cd")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "8c94c1e3-a225-42f4-98c6-ab7680cfe18a")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 55 "Ia_MON")
			(pintype "passive")
			(uuid "bfc6a2dc-ede6-4c80-a3e1-9d09e94773dc")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "5a90641c-69c7-47f6-91f1-a8539e12c964")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "ce5d979d-7782-4df2-9004-b407a1f5b90c")
		(at 87.6 56 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 0 1.6 90)
			(layer "B.SilkS")
			(uuid "d902e943-6ab3-42e7-8364-554b7bd60ce4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "22u"
			(at 0 -1.679999 90)
			(layer "B.Fab")
			(uuid "b1893a8e-43d5-4505-93fa-fa04095f96cf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "286d89a6-6ecc-448f-92de-d98d6d92beb3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "d4c02936-cab3-4cf4-9d44-c3fcca1cc520")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "f60528bc-faf5-446c-abbb-4e7340efc5d6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "13f88c03-2549-451f-ab09-53edc26e044f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/18eb2b2a-2fd1-44ba-8b26-71be376ac905")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f037c2cd-92aa-4376-aa8f-904bc4ac59b4")
		)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c389edca-4ec0-4341-aa07-7fbb11588f14")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "05ef56fe-9ba8-436b-983d-06a4b58f4267")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "5c46340f-b5da-4f6d-970c-d6d0021b8a60")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "4379b463-d8bc-4e92-8b63-7e1a62ca69c3")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "a0fac81b-bf1a-4dc2-8473-e96a45a3ce52")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "07ba7edd-b334-4d47-a30a-b84467d3a8a0")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "299c7a1a-49c6-4ed3-87b9-8da1d8f3ca99")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "fcfa5ad2-47f9-4f7e-907b-bd29440f7bca")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c245563c-27ab-46bc-be97-c67735923647")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "c43b1b1f-c25c-42da-8c27-5db0e9b4b786")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pintype "passive")
			(uuid "071f8bef-bdf1-4b8e-ae4c-f07a25f44328")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "d92d6c06-48dc-4ca1-ba28-caa210183372")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "d0d59ce8-b022-4917-a4f7-5b4320b82754")
		(at 43.3 57.8 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 3.2 -0.1 90)
			(layer "B.SilkS")
			(uuid "79280681-d965-4aa0-b728-e14c3d621f1e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "100p"
			(at 0 -1.679999 90)
			(layer "B.Fab")
			(uuid "5b71a409-b232-4be2-a453-9a16e0caa2d8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "d7aed32e-f281-431e-a57e-e1f4c79add7f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "6e2ff744-190e-4d08-9b49-8418313340be")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "4dea125e-35ac-4a94-b19c-dc2cea959465")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "0dfb0b63-877c-4a1e-b5ad-c4866717a7c4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/eb46dfe5-7707-4708-94d1-91913d6ff460")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f5538cf1-0fd7-4b8a-9afc-193922161089")
		)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "fb97e62e-f503-4859-a884-e65985253d02")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "a9384aee-161d-4827-ae11-c5c6f57c6b03")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "da3e888a-672c-44d3-9fdf-88a07f0aa782")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "2eca77a3-5707-44a6-b4bd-76fb205d0b79")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "a4da6fd7-dd30-49fe-9c81-1202c3082932")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c44af677-f4b3-480a-a399-0a45f24e9679")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "02404b37-70fd-46e3-8693-f405538c4a12")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f06f7bf9-537e-4665-a4a2-aa70654edb51")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "1c37e0d7-be4b-4ee2-9bec-5034952268a0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "7fd79078-77ca-46ee-bd6f-e1731aaae9e2")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(D5B-+)")
			(pintype "passive")
			(uuid "faf1d7c6-3692-4a7e-abc4-dd670435f053")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "33a95cd9-a752-4f7b-98ff-4506364c9827")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fiducial:Fiducial_1mm_Mask3mm"
		(layer "B.Cu")
		(uuid "d12b8c95-d08a-48de-9a9c-757977bbb389")
		(at 32 60.5 180)
		(descr "Circular Fiducial, 1mm bare copper, 3mm soldermask opening (recommended)")
		(tags "fiducial")
		(property "Reference" "FID4"
			(at 0 2.54 0)
			(layer "B.SilkS")
			(hide yes)
			(uuid "6337eea8-3ad1-4c19-8e05-10cf1f721191")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "Fiducial"
			(at 0 -2.286 0)
			(layer "B.Fab")
			(uuid "37315141-47a6-46d0-9f39-e979b03e7054")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Fiducial:Fiducial_1mm_Mask3mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "d3b9cecf-c053-4652-9515-e5db1b438af1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "8637bec7-ad0d-486f-b105-1c1508902953")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Fiducial Marker"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "b50725e1-49c5-48b8-9c7e-8d142b57a1a8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Fiducial*")
		(path "/61cd446e-2b7b-40bb-b8e6-9882d5434938")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1.75 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "B.CrtYd")
			(uuid "b7c588b5-7d63-46b6-8003-5ba6eaa6cffd")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "B.Fab")
			(uuid "46533af5-1fc7-4f14-ae2e-cfd1b0d35a6b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(uuid "58fb7cca-c369-4280-ab37-74547f6d0a8b")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
				(justify mirror)
			)
		)
		(pad "" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(solder_mask_margin 1)
			(clearance 1)
			(uuid "da19fafc-f6a6-4b0a-8654-ac277bd234bd")
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(uuid "d6f54cfc-037e-44d6-b268-9f1910d3423d")
		(at 45.6 54.3 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R29"
			(at 0 1.65 90)
			(layer "B.SilkS")
			(uuid "eb85ac68-313d-4846-af6b-1d7b895f47c6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "1k"
			(at 0 -1.65 90)
			(layer "B.Fab")
			(uuid "9950e653-c4b4-4860-923b-182f438957fc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "8aad5a66-4148-487b-93aa-38ad222e7b09")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "7de05a61-92f4-4712-885b-4b185fdaf0e8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "6d442a39-5663-459c-943e-9b0b69a69233")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/4949e397-8f9a-40a9-8853-38f368f6bcb4")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.227064 0.735)
			(end -0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f8db0d18-b6ec-48e3-9ce8-6129c49c903d")
		)
		(fp_line
			(start 0.227064 -0.735)
			(end -0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "2bf9c90f-2a7c-405d-bb73-b33d6fff1293")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "c8d6c940-664e-4f22-8961-191f232dcf9c")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "7bd4667d-ab45-4d24-9754-3653acff0aa2")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "28f1ad58-97b6-4017-a69f-0bd69322d72d")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "27026eff-b811-48e7-95e3-c652c7704442")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "23dd85bf-6c07-4da8-9270-a19421db6fa2")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c4f0afbf-94f0-4f32-970b-91741662b839")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "ad03a651-16d7-4ad5-a08f-3257db53914f")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "eddb1bea-704c-494a-83cf-9f62a19b9b6d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "95bed7c8-0816-4618-b6ab-d5737877de51")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 55 "Ia_MON")
			(pintype "passive")
			(uuid "56cdf59e-9d7f-4589-9b64-18750eff00a8")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 4 "GND")
			(pintype "passive")
			(uuid "683b8944-e254-4a36-987a-5a65ab3cbf2c")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "df5d1b5f-9df3-436a-b1a5-86e10671334f")
		(at 109.7 51.6 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at -1.7 -1.7 90)
			(layer "B.SilkS")
			(uuid "c1f754fb-2c80-481e-8813-d5ceabbe0f76")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "0.1u"
			(at 0 -1.679999 90)
			(layer "B.Fab")
			(uuid "cbfd9e3f-6f5b-4bb7-9a9d-144f2e4e0e11")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "130e48f3-9cbc-4483-92bf-9173d8cb0bfc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "03802851-d029-4be1-8a57-8aec7d54ec4a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "def813c1-b4c2-48b7-96d0-f04dd2b717cd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/43780"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "b9322d99-c10c-469e-a714-86e6f944a91d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/42ce20c2-df3b-444d-ad3d-2d3a0737685d")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "978d759f-c14b-49c4-8e21-5197ba042361")
		)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "651260e3-7562-4aa9-8f4b-3ea7a548eac5")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "04ec45f5-25e9-4854-9e81-ad79ff64922d")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "03f3ba8a-f8b0-4e00-b5ba-0d56b80089a1")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "1e90ce14-0f35-4346-bafb-d21121b435a3")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "223ee635-95fb-4a9c-9728-7de1dc9c4d09")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "304e6120-f184-4adc-b6d9-5ddd5942a2b8")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "2e175fb6-1fb9-4f8d-b688-6c37ffef4a74")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "37fd52d7-8807-4dff-aa5f-6df3fe5ba1ad")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "47467440-b9d1-4cd8-86fc-19d711c42b39")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "e8b186dc-5837-4383-a7df-6398cf463f56")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pintype "passive")
			(uuid "0f133ed3-2336-408a-87c2-93d1e5b45bf7")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "878cd1b9-625e-49c2-bb6a-ede0ea363887")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "B.Cu")
		(uuid "e5fa8bda-84a5-44b4-b798-5a203ce32282")
		(at 92.3 40.5 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "VD8"
			(at -0.17735 -2.28985 90)
			(layer "B.SilkS")
			(uuid "e6e56215-115d-4c8e-937a-69ea1b9845b1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "BAT54S"
			(at 0 -2.4 90)
			(layer "B.Fab")
			(uuid "71fac435-0420-4c45-890c-6762d3b06031")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "cc0ec2a0-73c6-4638-9d0c-41cca3f0c586")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds11005.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "0183550f-b510-4844-a771-37dba3e710e8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "dual schottky barrier diode, in series"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "77da3756-24d3-4066-99bc-bb9d5cc910e1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product/bat54s-nxp"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "ac5cda12-911a-4186-96a8-873577fa85ed")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/eca95e4e-1368-4384-b555-e42999d94dbf")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.65 -1.56)
			(end 0 -1.560001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "e0a0b9b7-7c81-4f44-97b7-54d301e71677")
		)
		(fp_line
			(start -0.65 -1.56)
			(end 0 -1.560001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "1023f92b-5cbf-4a79-8246-e4ba1c00d276")
		)
		(fp_line
			(start 0.65 1.56)
			(end 0 1.560001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c9bb89e3-3ec3-4e96-8c43-ed3a48157170")
		)
		(fp_line
			(start -0.65 1.56)
			(end 0 1.560001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f38268dc-dd1b-4829-a51e-a0cb26f3237c")
		)
		(fp_poly
			(pts
				(xy -1.1625 1.51) (xy -1.4025 1.84) (xy -0.9225 1.839999) (xy -1.1625 1.51)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "B.SilkS")
			(uuid "7542dc71-c239-403a-82cf-8c32ac4060c0")
		)
		(fp_line
			(start 1.92 -1.700001)
			(end -1.92 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "ead237f5-7023-4d00-9ae3-76e457e91083")
		)
		(fp_line
			(start -1.92 -1.700001)
			(end -1.92 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "02a48d9d-7894-4f95-9482-eb57ab213285")
		)
		(fp_line
			(start 1.92 1.700001)
			(end 1.92 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "912890e2-4fb9-4be5-9f3a-3fb021d5a21c")
		)
		(fp_line
			(start -1.92 1.700001)
			(end 1.92 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "e3c215b2-852a-4487-be8a-5e72ccce062e")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f49d8ad8-dc9b-460b-8b73-36fc440e5198")
		)
		(fp_line
			(start -0.65 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "3bf802e8-adca-47b4-80a4-19ceef5a005b")
		)
		(fp_line
			(start -0.65 1.125001)
			(end -0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "d8fe14bb-2032-4f40-b201-666cee21da31")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.325 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "d77fd9c1-4815-45e2-8c1b-dec5bc96ab30")
		)
		(fp_line
			(start -0.325 1.45)
			(end -0.65 1.125001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "5291c2c9-15c3-4362-b58d-6e786e933df1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "32e278fd-eec0-4e3b-941a-2e5938a297c2")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "af851ddf-f682-42b6-837d-21a287063dcb")
		)
		(pad "2" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pintype "passive")
			(uuid "9fde7aa8-91c8-4dd8-a2f1-ec465c56e2ac")
		)
		(pad "3" smd roundrect
			(at 0.937501 0 90)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 19 "HV_15V")
			(pintype "passive")
			(uuid "762db974-2417-469e-962b-ed8eb73b4da0")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "e650f3b1-0c41-4514-a1a0-b4e5c1252033")
		(at 114.9 48.2 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 2.7 0 0)
			(layer "B.SilkS")
			(uuid "da632263-5f1f-4c9c-9193-052e817db522")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "0.1u"
			(at 0 -1.679999 0)
			(layer "B.Fab")
			(uuid "ad273814-802f-45c6-b43d-be3744824929")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "2bb0f88a-5375-40a0-b4b9-ae8914e0302b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "9d163fea-57fe-445b-84a7-ae7ebd8247db")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "635796fa-a1da-4c6b-b4bc-e194b664c694")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/43780"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "b2e5f04c-d472-464a-9521-42452dcfb592")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/9f27ee93-b734-481d-94d8-e73bd84c1433")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a8f33190-7437-4451-9275-3db28d17475b")
		)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "389d2c41-ee31-485c-9725-faf607e64075")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "45b0cf6e-f4f7-4b68-9f4a-e0c5b2bc3096")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "52c04694-9bac-4cff-91b6-7a02179bfbd3")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "69589ecf-8a2c-4064-8f4d-15e25d708cac")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "d6492e67-4663-488e-b48f-35da416b4ad1")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "40224c41-2852-43df-a660-ca00f837e74b")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f166e07c-90bf-4abd-a0d8-33b861a30db8")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "19decd39-db34-42a7-a3b9-131b7cb7f4d1")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "3ee243f1-82c6-4b27-b000-0f6f18c24c3e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(uuid "364488fc-f65a-4ffb-a707-2178ab36b568")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 6 "+5V")
			(pintype "passive")
			(uuid "8773f58c-db2c-49d9-97ce-2c840d2d2e1d")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "ebe9fc2a-0cf7-4a9e-8033-55242535e335")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(uuid "ef6872dc-1aac-449c-87d2-dc57d26edfa1")
		(at 122.8 60.1 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 0 -1.6 90)
			(layer "B.SilkS")
			(uuid "9156423d-cfea-4708-a059-6cbf5f02cda5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "10k"
			(at 0 -1.65 90)
			(layer "B.Fab")
			(uuid "321121e9-c4ff-42d0-94a1-3b4900706e3f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "0853f788-5e2c-4bd7-8dd8-3551bf7f3004")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "e3d3445f-82f3-46a4-9805-3e075d452806")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "38214bcb-0b89-45e0-bc48-e1701897e879")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/b9d3acaf-e329-4866-8023-38dccf61bf44")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.227064 0.735)
			(end -0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "68d03166-e417-49fd-806f-776855270e9c")
		)
		(fp_line
			(start 0.227064 -0.735)
			(end -0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "174a4527-8d78-4be8-a660-b5056d6f1364")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "94144b64-b1dc-4f4a-90bd-1db1e50288f6")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "78e00884-feaa-4255-93d1-7e59ac2f30a6")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "0ad4a530-4a9b-42d0-944d-a792ab2f7cc9")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "72ce5e73-efb3-4639-8855-5c29f428f80f")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "6e767422-bdb0-4726-a9c3-5aad5baec633")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f21948a6-f894-4140-83cf-a38cb7d572db")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "8942c956-a668-4814-8cf9-cce1c94815f0")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "583771aa-ecc0-44a1-b655-d35bbf233d3f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "2b5c8beb-294a-4746-b635-3572f0aac56f")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 3 "+3V3")
			(pintype "passive")
			(uuid "79f6a6df-8784-4a7b-862d-dcf63be486c1")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 38 "RESET")
			(pintype "passive")
			(uuid "507a509f-cb1a-4233-b43a-b5bf7663e29d")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(uuid "f63322c7-48dd-4824-974d-6eab97cd7f63")
		(at 36 53.1 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R28"
			(at 0.7 2.3 90)
			(layer "B.SilkS")
			(uuid "b987faec-9713-4a70-98d6-d9e4a10db4a8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "none"
			(at 0 -1.65 90)
			(layer "B.Fab")
			(uuid "f4950eb9-74e2-400b-acb9-cd45ab9b1f63")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "90cf8e28-c4ca-4857-b67f-ea388fb01452")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "86768d1f-e92d-4f3a-b3e6-395438fb7eba")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "48e59ccd-b206-4476-936f-c2a857535691")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/dcdcf1af-02c4-499c-a382-698b47672f46")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(fp_line
			(start 0.227064 0.735)
			(end -0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "23f4775c-150b-4b34-8857-7dd108043e95")
		)
		(fp_line
			(start 0.227064 -0.735)
			(end -0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "2bcc2666-451f-40f3-becc-2afda2af11a2")
		)
		(fp_line
			(start -1.68 0.95)
			(end -1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "67f12623-723c-415e-ab0b-d486ffd53553")
		)
		(fp_line
			(start 1.68 0.95)
			(end -1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "0bac70aa-0211-439b-ac3a-c84ad28cfbb2")
		)
		(fp_line
			(start -1.68 -0.95)
			(end 1.68 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "67542783-b5ee-44c0-bb8d-4d9ad7ac504d")
		)
		(fp_line
			(start 1.68 -0.95)
			(end 1.68 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "cba1e69d-b210-4626-a531-9e154667d800")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "98e941ee-27a0-4373-8b91-ebe64b15be21")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "31bfa59f-edfe-4495-932b-129e8f6020e8")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "dbfed403-ae9e-44d3-9103-7ac1e53bc293")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "53c3fb7e-7ef2-485f-a588-3df0cc660d45")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "021a0f86-0c07-4683-b3e2-68ccd678dfee")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 43 "Ua_MON")
			(pintype "passive")
			(uuid "4bd49730-3b9f-488d-9471-0f96956f4c56")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.243902)
			(net 4 "GND")
			(pintype "passive")
			(uuid "6fd6a824-c98b-4f5c-9dee-0f21ce8356ca")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(uuid "f727d452-2189-48ef-89bf-46069a26834f")
		(at 103.100001 54.4 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 0.2 -1.699999 90)
			(layer "B.SilkS")
			(uuid "d939f3dc-51cd-4398-beab-7555aadc422d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "22p"
			(at 0 -1.679999 90)
			(layer "B.Fab")
			(uuid "4d9a5728-2bb1-4c83-b0a5-b1febd104fc1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "c11472f4-fc13-44e8-b745-ac755a44882b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "aba14b48-c2a2-4931-a917-319931b305e5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "853e9261-2bee-4248-a650-64d3aff1b7af")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/7a5c9799-8fa7-4c9a-ade4-171cde868aa0")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 0.261253 0.735)
			(end -0.261253 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "70804cd7-ee01-46c3-8d1d-004e6a488a23")
		)
		(fp_line
			(start 0.261253 -0.735)
			(end -0.261253 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0c271c19-3a07-4fc1-88fa-c5c643eb4df4")
		)
		(fp_line
			(start -1.7 0.98)
			(end -1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "19f8c143-0697-4b16-876c-eef8d92b95ac")
		)
		(fp_line
			(start 1.7 0.98)
			(end -1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "71db4e90-df32-4476-b2d9-7b14afde92c9")
		)
		(fp_line
			(start -1.7 -0.98)
			(end 1.7 -0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "a9dd0374-3def-4f63-81dd-0736ca7f1898")
		)
		(fp_line
			(start 1.7 -0.98)
			(end 1.7 0.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "5abfd991-22e3-4e92-89c1-38242a39c103")
		)
		(fp_line
			(start -1 0.625)
			(end -1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "68711aa2-4019-46fd-8ec0-916d17496653")
		)
		(fp_line
			(start 1 0.625)
			(end -1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "34585adf-9f96-4d51-b37d-2953c1a2d950")
		)
		(fp_line
			(start -1 -0.625)
			(end 1 -0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "106eb327-adcf-4856-b85a-57e8d5430a37")
		)
		(fp_line
			(start 1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "a82d1abc-5132-4b1c-863f-76bac3a1bece")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "ce750aa1-11bc-4555-920f-a3a4c00f6e43")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.949999 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "a4a878d9-b793-40a9-9648-59b827fcf8a9")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(D4-PD0)")
			(pintype "passive")
			(uuid "bc6b9566-0534-40fd-8a59-01877ffc9323")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_1812_4532Metric_Pad1.30x3.40mm_HandSolder"
		(layer "B.Cu")
		(uuid "fc23dafa-52ee-4aae-b75e-d450a9a8cf53")
		(at 131.8 43.3 90)
		(descr "Fuse SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "fuse handsolder")
		(property "Reference" "F1"
			(at 0 2.65 90)
			(layer "B.SilkS")
			(uuid "3b511cb8-30b6-49b4-9aa4-93f09ff015b0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "MF-MSMF110"
			(at 0 -2.65 90)
			(layer "B.Fab")
			(uuid "1c1f3c54-4755-42f3-9445-3c8ed3cce91b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Fuse:Fuse_1812_4532Metric_Pad1.30x3.40mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "d9aed1d3-0f3e-451d-ad72-790f17da5544")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "08c9fc56-fc79-4487-bf63-977ab0794226")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "2a14c252-ba25-4707-8274-ab25a04e9f4a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Label" "1.1А"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "c0ca6677-6b27-4a0a-9e37-5abf301eabee")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product0/8022330802"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "07f1b4a1-9477-47c1-b629-9b5dbd97409a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "*Fuse*")
		(path "/b064b689-481d-4693-ab29-22ce565c503d")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start 1.386252 -1.71)
			(end -1.386252 -1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "107cc484-1759-41ba-8dda-85832c9d2444")
		)
		(fp_line
			(start 1.386252 1.71)
			(end -1.386252 1.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c150a91d-b2cf-47e2-ac5e-de451dcb9932")
		)
		(fp_line
			(start 3.12 -1.95)
			(end 3.12 1.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "0f622d98-db21-4ba7-a3b0-c1fd9703a91e")
		)
		(fp_line
			(start -3.12 -1.95)
			(end 3.12 -1.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "f10aa7ab-a940-40cc-b01c-5af7a5dc2296")
		)
		(fp_line
			(start 3.12 1.95)
			(end -3.12 1.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "720856fc-0908-4cc2-8d29-5fb89a83ad4e")
		)
		(fp_line
			(start -3.12 1.95)
			(end -3.12 -1.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "31af9a21-4f0e-4b6b-b02e-8f36af9e2865")
		)
		(fp_line
			(start 2.25 -1.6)
			(end 2.25 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "9d0372de-5a2b-4d1f-9abe-c3f6b839fc63")
		)
		(fp_line
			(start -2.25 -1.6)
			(end 2.25 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "37517dbc-6911-4311-8fa3-76e97ba20f33")
		)
		(fp_line
			(start 2.25 1.6)
			(end -2.25 1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "423f83d0-5d16-435b-8c2c-5eb37a133bc4")
		)
		(fp_line
			(start -2.25 1.6)
			(end -2.25 -1.6)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "8019c61c-0595-4b62-a03d-b5b7bf6da641")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "010a608c-f905-4668-886f-34116ecb8e80")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -2.225001 0 90)
			(size 1.3 3.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.192308)
			(net 71 "Net-(X2-Pin_1)")
			(pintype "passive")
			(uuid "5adc4fb2-a0bf-40c0-a866-56793d0dfd25")
		)
		(pad "2" smd roundrect
			(at 2.225001 0 90)
			(size 1.3 3.4)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.192308)
			(net 5 "+12V")
			(pintype "passive")
			(uuid "3edd472a-65f7-453c-b17e-5bbc74f1da3c")
		)
		(model "${ECOHIM_LIB}/Ecohim.3dmodels/fuse_smd1812.stp"
			(offset
				(xyz 0 0 1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "B.Cu")
		(uuid "fce347ca-bce5-4e9f-8258-cb5de05ba91b")
		(at 64.3 50.762499 -90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "VD14"
			(at 0 2.4 90)
			(layer "B.SilkS")
			(uuid "064e8d61-c753-4624-a1f9-5071c0b448ed")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "BAT54S"
			(at 0 -2.4 90)
			(layer "B.Fab")
			(uuid "937c8834-0299-48d7-9971-7ceba1e261f6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "0f5ec31c-fc26-493e-8568-38546c5910d8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ds11005.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "28ba4390-4a93-426a-997b-2c0990aab90a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "dual schottky barrier diode, in series"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "3a6d2ffe-1b85-4382-aa98-d2384e97e88d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Link" "https://www.chipdip.ru/product/bat54s-nxp"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "3dc81263-68cf-47e5-887b-404917190398")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/66e8a3c0-fe1e-4fac-965d-b0d228c1ad9d")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.65 1.56)
			(end 0 1.560001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "253cf9a5-1feb-4483-aad3-01a0c73933c8")
		)
		(fp_line
			(start 0.65 1.56)
			(end 0 1.560001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b2088ba5-1a41-46ae-a51d-1a901918fc6f")
		)
		(fp_line
			(start -0.65 -1.56)
			(end 0 -1.560001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "514f3ab3-6d91-4142-ac83-71ac73ccd96c")
		)
		(fp_line
			(start 0.65 -1.56)
			(end 0 -1.560001)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "c609a082-fc1a-4086-ac16-0a164827f1a5")
		)
		(fp_poly
			(pts
				(xy -1.1625 1.51) (xy -1.4025 1.84) (xy -0.9225 1.839999) (xy -1.1625 1.51)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "B.SilkS")
			(uuid "3e219a84-953f-4a26-8fc7-2eb4239ca997")
		)
		(fp_line
			(start -1.92 1.700001)
			(end 1.92 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "f78f0fdf-d234-4daf-80e4-0c710531c873")
		)
		(fp_line
			(start 1.92 1.700001)
			(end 1.92 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "31bc1367-a653-403b-a9f7-a98787344e8b")
		)
		(fp_line
			(start -1.92 -1.700001)
			(end -1.92 1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "dbfd4e30-b61f-408c-8b06-9519f1700805")
		)
		(fp_line
			(start 1.92 -1.700001)
			(end -1.92 -1.700001)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "3ffa43c9-19a2-491b-9ab3-0a8520c05ff5")
		)
		(fp_line
			(start -0.325 1.45)
			(end -0.65 1.125001)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "71d2aa38-b728-4fd4-9b92-7867dba3c385")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.325 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "c05d77f9-f21c-4b59-be6b-5904c8e20d4c")
		)
		(fp_line
			(start -0.65 1.125001)
			(end -0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "6b20a66a-a8f0-40c5-ac28-65b160629c0d")
		)
		(fp_line
			(start -0.65 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "883d7403-dc03-4ee7-8b32-bd1e1ab55954")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "fbe9b36f-d02e-4c08-944e-6e4fafd7ec5d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(uuid "05af93de-6eb1-45b1-b2c2-cabbab805d05")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
				(justify mirror)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 0.95 270)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "GND")
			(pintype "passive")
			(uuid "a0c3abae-a36e-41f9-a774-377b5e8b73fb")
		)
		(pad "2" smd roundrect
			(at -0.9375 -0.95 270)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pintype "passive")
			(uuid "cd200008-9220-4c1e-9bdf-29b2f8adeadc")
		)
		(pad "3" smd roundrect
			(at 0.937501 0 270)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 54 "CONN")
			(pintype "passive")
			(uuid "61034743-de5a-4b91-8d51-87ba4441454f")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fiducial:Fiducial_1mm_Mask3mm"
		(layer "B.Cu")
		(uuid "ff3b2a23-95e1-4a6d-9d66-7eccc2839cfb")
		(at 32 37.5 180)
		(descr "Circular Fiducial, 1mm bare copper, 3mm soldermask opening (recommended)")
		(tags "fiducial")
		(property "Reference" "FID3"
			(at 0 2.54 0)
			(layer "B.SilkS")
			(hide yes)
			(uuid "911d2f6a-bbae-4b5c-a33d-0fc0afa3e79b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "Fiducial"
			(at 0 -2.286 0)
			(layer "B.Fab")
			(uuid "b44255a2-77be-4c48-84a8-60da99df0d44")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Footprint" "Fiducial:Fiducial_1mm_Mask3mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "a6454ba4-58cf-43f0-8e98-9d59d17a258d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "d52125a0-e1f0-4482-8b9a-599dea8c1539")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Description" "Fiducial Marker"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
			(uuid "a428fe56-e739-4e51-9e72-30eb3c84b7dd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Fiducial*")
		(path "/34cc1ca6-560c-4409-8ec7-639c3dca87ad")
		(sheetname "Root")
		(sheetfile "RS485_BSV_V1R1.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1.75 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill none)
			(layer "B.CrtYd")
			(uuid "b0c1fd56-c73a-4e32-b686-d76194ede49a")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "B.Fab")
			(uuid "78a943eb-ef2f-442a-8297-fd5db3c33cea")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(uuid "f7fb8ef6-196b-412b-9140-931fb6cda953")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
				(justify mirror)
			)
		)
		(pad "" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(solder_mask_margin 1)
			(clearance 1)
			(uuid "65c61d48-736e-4f12-99fc-b38d1cd2f9fb")
		)
	)
	(gr_line
		(start 36.7 55.6)
		(end 36.1 54.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "B.SilkS")
		(uuid "178a3128-1137-4e37-a4a6-e849f1dc2306")
	)
	(gr_line
		(start 45.7 55.8)
		(end 45.1 56.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "B.SilkS")
		(uuid "366f4189-cf5b-41d9-a241-a7b69c74f75b")
	)
	(gr_line
		(start 36.1 54.6)
		(end 35.5 55.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "B.SilkS")
		(uuid "79c02244-0daa-44c7-9911-2b2b628b9b31")
	)
	(gr_line
		(start 35.5 55.6)
		(end 36.7 55.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "B.SilkS")
		(uuid "9f4cf647-5949-432d-8019-44a2944ab8d5")
	)
	(gr_line
		(start 45.1 56.8)
		(end 46.3 56.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "B.SilkS")
		(uuid "9f6dca37-642a-44f6-8127-cf56335bdf06")
	)
	(gr_line
		(start 46.3 56.8)
		(end 45.7 55.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "B.SilkS")
		(uuid "e67c1f1b-b2c3-441a-bb6b-ab86bc5d6c4b")
	)
	(gr_line
		(start 35.5 54.6)
		(end 36.7 54.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "B.SilkS")
		(uuid "ee338bff-cfb3-4c72-b351-2beab156066d")
	)
	(gr_line
		(start 45.1 55.8)
		(end 46.3 55.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "B.SilkS")
		(uuid "f88b1323-3068-4e25-bdef-88adb22ef6e0")
	)
	(gr_line
		(start 118.999999 43.1)
		(end 118.600001 43.7)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "03351a63-cfce-4d74-a28c-2e73cfab46a3")
	)
	(gr_line
		(start 38.7 47.550002)
		(end 39.699997 48.150001)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "05eab0f9-caa6-4749-8e1f-80fb2b9524e4")
	)
	(gr_line
		(start 74.4 51.9)
		(end 75.6 51.9)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "0b9265da-c14e-4d32-becb-3b193aa8f3fa")
	)
	(gr_line
		(start 43.999999 48.149998)
		(end 44.999997 47.549998)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "0bec2b22-7de5-49b1-b2f5-7404702075ce")
	)
	(gr_circle
		(center 126.29 53.375)
		(end 126.89 53.375)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "179a26e7-98ad-4760-8457-85c3f68fb377")
	)
	(gr_line
		(start 39.699997 46.950001)
		(end 38.7 47.550002)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3901eb0a-945a-408e-b61e-86f3dfedd189")
	)
	(gr_line
		(start 118.999999 44.3)
		(end 118.999999 43.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "431e5e1b-fa32-4f32-ab7e-84de339eb26f")
	)
	(gr_line
		(start 118.600001 43.7)
		(end 118.999999 44.3)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "4c292ffc-26d3-4558-9cd2-2ba4ba9b2a50")
	)
	(gr_line
		(start 75.6 51.9)
		(end 75 51.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "51b8c6aa-2ed4-491f-affb-c21b02b1977e")
	)
	(gr_line
		(start 44.999997 47.549998)
		(end 44 46.949997)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "58c94c04-caf7-4205-bb44-dc2b30036aef")
	)
	(gr_line
		(start 74.4 55.9)
		(end 75.6 55.9)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "703c0b79-8a7a-4432-9e71-db46a05090d1")
	)
	(gr_line
		(start 75.6 56.3)
		(end 75 55.9)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "71ef2f00-49d6-43ae-9a29-6bde6d5a3cce")
	)
	(gr_line
		(start 118.999999 39.8)
		(end 118.999999 38.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "785f5b2f-cfc4-423b-89a3-2aa22c32030f")
	)
	(gr_line
		(start 118.999999 38.6)
		(end 118.600001 39.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "7893aad8-f241-457b-a0da-d9a22991933b")
	)
	(gr_line
		(start 44 46.949997)
		(end 43.999999 48.149998)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "8f1c0595-786d-4641-a860-068ece0c9001")
	)
	(gr_line
		(start 118.600001 39.8)
		(end 118.600001 38.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a0dd269c-b879-416c-85a4-71f7c4712b11")
	)
	(gr_line
		(start 38.7 48.150001)
		(end 38.699999 46.950001)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a5902430-d1bb-4453-b318-85d1c672f4d1")
	)
	(gr_line
		(start 75 55.9)
		(end 74.4 56.3)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a8f111f9-c203-4eff-a2cf-47b3a539a87f")
	)
	(gr_line
		(start 118.600001 44.3)
		(end 118.600001 43.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "da777036-21f2-476c-8731-53408bf3e7b2")
	)
	(gr_line
		(start 44.999997 46.949998)
		(end 44.999997 48.149998)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e6047146-209f-408d-91ee-91c6549f58cd")
	)
	(gr_line
		(start 118.600001 39.2)
		(end 118.999999 39.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "ebde49ee-716b-4426-bb17-b79485450510")
	)
	(gr_line
		(start 75 51.5)
		(end 74.4 51.9)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f51aa1b8-1bd9-4ce9-822a-18c8f3149429")
	)
	(gr_line
		(start 74.4 51.5)
		(end 75.6 51.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f55e351e-db73-4dc0-bc84-c19f40d9b3ab")
	)
	(gr_line
		(start 39.699997 48.150001)
		(end 39.699997 46.950001)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f65e3860-3ac0-49cb-bdc7-4aab5a24b8c9")
	)
	(gr_line
		(start 74.4 56.3)
		(end 75.6 56.3)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f9803b65-23f6-4d1e-a0a9-01444a7626e8")
	)
	(gr_rect
		(start 30 35)
		(end 140 63)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "Edge.Cuts")
		(uuid "1c6ed06b-9b8b-42a4-bf05-af710007db34")
	)
	(gr_text "+"
		(at 63.699999 38.200001 90)
		(layer "B.SilkS")
		(uuid "339d0578-8883-4d3e-b9c5-a4a0f6861326")
		(effects
			(font
				(size 1 1)
				(thickness 0.2)
				(bold yes)
			)
			(justify mirror)
		)
	)
	(gr_text "+"
		(at 95.9 49.2 0)
		(layer "B.SilkS")
		(uuid "e05b41d2-721f-4212-96fa-1e28ffbf55b7")
		(effects
			(font
				(size 1 1)
				(thickness 0.2)
				(bold yes)
			)
			(justify mirror)
		)
	)
	(gr_text "ACT"
		(at 120.5 38.3 0)
		(layer "F.SilkS")
		(uuid "13a9bb46-a18c-4429-a009-06d7448b6bdb")
		(effects
			(font
				(size 1 1)
				(thickness 0.2)
				(bold yes)
			)
		)
	)
	(gr_text "24V"
		(at 76.9 56.1 90)
		(layer "F.SilkS")
		(uuid "1729ddfc-52e2-4296-afaa-69104438762f")
		(effects
			(font
				(size 1 1)
				(thickness 0.2)
				(bold yes)
			)
		)
	)
	(gr_text "RS485_BSV V1R2"
		(at 101.2 70.5 0)
		(layer "F.SilkS")
		(uuid "219c68f4-d096-495d-ac5a-2d1e2fa0359c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify top)
		)
	)
	(gr_text "UM"
		(at 39.2 50.4 0)
		(layer "F.SilkS")
		(uuid "23e13466-a34d-4898-8e1d-54dfb5a4500a")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.16)
				(bold yes)
			)
			(justify left bottom)
		)
	)
	(gr_text "PWR"
		(at 120.5 43.3 0)
		(layer "F.SilkS")
		(uuid "27eb1186-ee6e-4a84-8cc0-e7a88a4a009b")
		(effects
			(font
				(size 1 1)
				(thickness 0.2)
				(bold yes)
			)
		)
	)
	(gr_text "UC"
		(at 32.1 41.5 90)
		(layer "F.SilkS")
		(uuid "2ae2aa99-c79a-4342-8c2b-e8d29260fa3a")
		(effects
			(font
				(size 1 1)
				(thickness 0.2)
				(bold yes)
			)
			(justify left bottom)
		)
	)
	(gr_text "+"
		(at 120 49.2 0)
		(layer "F.SilkS")
		(uuid "2fea9d61-df99-4862-a82e-5069698adf9a")
		(effects
			(font
				(size 1 1)
				(thickness 0.2)
				(bold yes)
			)
		)
	)
	(gr_text "IM"
		(at 41.7 50.4 0)
		(layer "F.SilkS")
		(uuid "320b90e3-6000-4199-936b-b01f49e2119f")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.16)
				(bold yes)
			)
			(justify left bottom)
		)
	)
	(gr_text "IC"
		(at 50.800001 40.750001 90)
		(layer "F.SilkS")
		(uuid "35399502-2523-419e-aa01-905cd796d5c4")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.16)
				(bold yes)
			)
			(justify left bottom)
		)
	)
	(gr_text "XUM"
		(at 40.2 62.1 0)
		(layer "F.SilkS")
		(uuid "8dd94106-3489-4bd1-85b7-1bc9df098075")
		(effects
			(font
				(size 1 1)
				(thickness 0.2)
				(bold yes)
			)
			(justify right bottom)
		)
	)
	(gr_text "XUC"
		(at 33.6 46.7 90)
		(layer "F.SilkS")
		(uuid "95b0ab48-bacc-43ab-8fa6-c2633e8aea65")
		(effects
			(font
				(size 1 1)
				(thickness 0.2)
				(bold yes)
			)
			(justify left bottom)
		)
	)
	(gr_text "XIM"
		(at 41.5 62.1 0)
		(layer "F.SilkS")
		(uuid "a7a429b9-7b21-45e2-97b1-4bff401ebdfc")
		(effects
			(font
				(size 1 1)
				(thickness 0.2)
				(bold yes)
			)
			(justify left bottom)
		)
	)
	(gr_text "XIC"
		(at 52.399999 43.250001 90)
		(layer "F.SilkS")
		(uuid "b148bd0d-6f00-4117-84fb-053e8d271e32")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.16)
				(bold yes)
			)
			(justify right bottom)
		)
	)
	(gr_text "GND"
		(at 101.2 39.2 0)
		(layer "F.SilkS")
		(uuid "c8c52e06-0b84-4057-9c4f-81366b21b198")
		(effects
			(font
				(size 1 1)
				(thickness 0.2)
				(bold yes)
			)
			(justify bottom)
		)
	)
	(gr_text "Enable"
		(at 76.9 51.3 90)
		(layer "F.SilkS")
		(uuid "de463ce5-64b0-4dca-8cc9-c50eaf9b06d8")
		(effects
			(font
				(size 1 1)
				(thickness 0.2)
				(bold yes)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "Eco1.User")
		(uuid "21ba45e0-8e6d-432d-ac62-a76477ec4c44")
		(pts
			(xy 30 63) (xy 30 25)
		)
		(height -6.8)
		(orientation 1)
		(gr_text "38.0000 mm"
			(at 22.05 44 90)
			(layer "Eco1.User")
			(uuid "21ba45e0-8e6d-432d-ac62-a76477ec4c44")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type orthogonal)
		(layer "Eco1.User")
		(uuid "8fd87645-de63-41a4-9e9d-a9ce289ed41a")
		(pts
			(xy 30 63) (xy 34 29)
		)
		(height -3.1)
		(orientation 1)
		(gr_text "34.0000 mm"
			(at 25.75 46 90)
			(layer "Eco1.User")
			(uuid "8fd87645-de63-41a4-9e9d-a9ce289ed41a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type orthogonal)
		(layer "Eco1.User")
		(uuid "94374286-b290-4f54-b648-9db20320a62c")
		(pts
			(xy 30 25) (xy 100 25)
		)
		(height -6.8)
		(orientation 0)
		(gr_text "70.0000 mm"
			(at 65 17.05 0)
			(layer "Eco1.User")
			(uuid "94374286-b290-4f54-b648-9db20320a62c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type orthogonal)
		(layer "Eco1.User")
		(uuid "bf1874d7-2ec1-48c0-bccb-64b2de26067f")
		(pts
			(xy 34 29) (xy 96 29)
		)
		(height -7.6)
		(orientation 0)
		(gr_text "62.0000 mm"
			(at 65 20.25 0)
			(layer "Eco1.User")
			(uuid "bf1874d7-2ec1-48c0-bccb-64b2de26067f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(segment
		(start 101.1 55.050001)
		(end 99.650001 55.050001)
		(width 0.3)
		(layer "F.Cu")
		(net 1)
		(uuid "5f4f5670-9f3d-4eb8-83a3-abb330891a6d")
	)
	(segment
		(start 98.85 54.25)
		(end 95.375 54.25)
		(width 0.3)
		(layer "F.Cu")
		(net 1)
		(uuid "9476dd6c-aabc-405c-842f-eeb543f04762")
	)
	(segment
		(start 99.650001 55.050001)
		(end 98.85 54.25)
		(width 0.3)
		(layer "F.Cu")
		(net 1)
		(uuid "e7cc4d49-505b-4e2f-b6cf-91ed47fcd1a7")
	)
	(segment
		(start 103.100001 55.349999)
		(end 101.399998 55.349999)
		(width 0.3)
		(layer "B.Cu")
		(net 1)
		(uuid "1a59185a-d87c-4d19-b8a5-9288ad91a77e")
	)
	(segment
		(start 101.399998 55.349999)
		(end 101.1 55.050001)
		(width 0.3)
		(layer "B.Cu")
		(net 1)
		(uuid "62ed686d-cece-43c7-8fc1-cdc2768a2c29")
	)
	(segment
		(start 98.850001 53.749999)
		(end 101.1 51.5)
		(width 0.3)
		(layer "F.Cu")
		(net 2)
		(uuid "bc999e20-7ba7-4cad-95ac-5e3d512efac2")
	)
	(segment
		(start 101.1 51.5)
		(end 101.1 50.170001)
		(width 0.3)
		(layer "F.Cu")
		(net 2)
		(uuid "dda1fa27-e196-411e-9159-6e9a53c8430c")
	)
	(segment
		(start 95.375 53.749999)
		(end 98.850001 53.749999)
		(width 0.3)
		(layer "F.Cu")
		(net 2)
		(uuid "f65afe86-f018-4354-accb-88285cc3cd0d")
	)
	(segment
		(start 101.42 49.850001)
		(end 101.1 50.170001)
		(width 0.3)
		(layer "B.Cu")
		(net 2)
		(uuid "8d2f3863-d76e-464d-903b-24cc0b13e337")
	)
	(segment
		(start 103.1 49.850001)
		(end 101.42 49.850001)
		(width 0.3)
		(layer "B.Cu")
		(net 2)
		(uuid "c9c8d564-fab5-48f3-896f-3180d018dd31")
	)
	(segment
		(start 91.607649 50.792352)
		(end 91.300001 51.1)
		(width 0.5)
		(layer "B.Cu")
		(net 3)
		(uuid "67f58aa3-6f7c-41e9-8004-e3b1c0ff1330")
	)
	(segment
		(start 85.6 56.949999)
		(end 87.6 56.949999)
		(width 0.5)
		(layer "B.Cu")
		(net 3)
		(uuid "8f12b03e-c81a-4f75-8916-379b67788f02")
	)
	(segment
		(start 91.750001 48.4)
		(end 91.607649 48.542352)
		(width 0.5)
		(layer "B.Cu")
		(net 3)
		(uuid "90d44d12-a097-4a25-8d14-53eab50a99ac")
	)
	(segment
		(start 91.607649 48.542352)
		(end 91.607649 50.792352)
		(width 0.5)
		(layer "B.Cu")
		(net 3)
		(uuid "fb18c9b3-0f2b-49af-b23d-d2fc08d88c38")
	)
	(via
		(at 104.699999 52.6)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 4)
		(uuid "499f46dc-7ee4-4adc-b9c4-c8f6175bbe73")
	)
	(segment
		(start 36 54.0125)
		(end 33.937499 54.0125)
		(width 0.3)
		(layer "B.Cu")
		(net 4)
		(uuid "25a06e52-7c54-4806-b487-7a5ef979a0ec")
	)
	(segment
		(start 103.1 52.6)
		(end 104.699999 52.6)
		(width 0.3)
		(layer "B.Cu")
		(net 4)
		(uuid "4cab2c69-99d5-48d0-9e3a-25deb776ec7b")
	)
	(segment
		(start 103.100001 51.75)
		(end 103.1 51.749999)
		(width 0.3)
		(layer "B.Cu")
		(net 4)
		(uuid "5d909492-1bf1-418c-9a6e-9aa418f4508e")
	)
	(segment
		(start 33.937499 54.0125)
		(end 33.9 54.049999)
		(width 0.3)
		(layer "B.Cu")
		(net 4)
		(uuid "65008cac-16f0-4885-8e5f-bd405138c954")
	)
	(segment
		(start 103.100001 53.450001)
		(end 103.100001 51.75)
		(width 0.3)
		(layer "B.Cu")
		(net 4)
		(uuid "b2f13f1d-3269-49bd-857f-95c31f55f92d")
	)
	(segment
		(start 47.662501 55.2125)
		(end 47.7 55.249999)
		(width 0.3)
		(layer "B.Cu")
		(net 4)
		(uuid "cd356bf4-0e8d-4f90-a24b-ca4767f33e40")
	)
	(segment
		(start 45.6 55.2125)
		(end 47.662501 55.2125)
		(width 0.3)
		(layer "B.Cu")
		(net 4)
		(uuid "e49802e6-722c-43ba-b217-60cf4f71c313")
	)
	(segment
		(start 121.4375 44.9)
		(end 123.2 44.9)
		(width 0.3)
		(layer "F.Cu")
		(net 5)
		(uuid "731e5590-cb56-4957-b3ae-7f744ad126f5")
	)
	(via
		(at 123.2 44.9)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 5)
		(uuid "744124c6-8f1a-43e1-8302-f1281aeb81da")
	)
	(segment
		(start 68.799999 37.400001)
		(end 68.799999 41.4)
		(width 0.6)
		(layer "B.Cu")
		(net 5)
		(uuid "16fcae59-11ed-4b8f-81c5-8fb19597b458")
	)
	(segment
		(start 131.8 41.074999)
		(end 131.8 37.4)
		(width 0.6)
		(layer "B.Cu")
		(net 5)
		(uuid "531db41a-e5f0-4ed6-be3d-1a47df27e6ab")
	)
	(segment
		(start 132.462499 41.074999)
		(end 136.6 45.2125)
		(width 1.2)
		(layer "B.Cu")
		(net 5)
		(uuid "57d6589b-64f0-4978-97c6-73dd5a34f059")
	)
	(segment
		(start 131.8 41.074999)
		(end 132.462499 41.074999)
		(width 1.2)
		(layer "B.Cu")
		(net 5)
		(uuid "60b8316f-309f-420c-8c63-dda5a3389139")
	)
	(segment
		(start 130.6 36.2)
		(end 123.3 36.2)
		(width 0.6)
		(layer "B.Cu")
		(net 5)
		(uuid "756f6803-5987-40fa-8399-3d7e5ff6219d")
	)
	(segment
		(start 123.3 36.2)
		(end 70 36.2)
		(width 0.6)
		(layer "B.Cu")
		(net 5)
		(uuid "8a60dffa-0fb7-4a16-9553-533c837d8f3a")
	)
	(segment
		(start 137.5 48.3)
		(end 137.5 46.1125)
		(width 1.2)
		(layer "B.Cu")
		(net 5)
		(uuid "912fc0b2-856c-46c7-82eb-d2bef6451c5e")
	)
	(segment
		(start 136.149999 48.3)
		(end 137.5 48.3)
		(width 0.6)
		(layer "B.Cu")
		(net 5)
		(uuid "aea73cc6-3718-4932-becf-1035e0f96fe3")
	)
	(segment
		(start 123.2 36.3)
		(end 123.3 36.2)
		(width 0.3)
		(layer "B.Cu")
		(net 5)
		(uuid "b111357e-d3e6-4706-839b-c79b923a3c1e")
	)
	(segment
		(start 131.8 37.4)
		(end 130.6 36.2)
		(width 0.6)
		(layer "B.Cu")
		(net 5)
		(uuid "ca682048-34a1-4d7d-bafc-aa8535506bde")
	)
	(segment
		(start 137.5 46.1125)
		(end 136.6 45.2125)
		(width 1.2)
		(layer "B.Cu")
		(net 5)
		(uuid "cae3cf95-647c-41d1-9680-3e6112021567")
	)
	(segment
		(start 70 36.2)
		(end 68.799999 37.400001)
		(width 0.6)
		(layer "B.Cu")
		(net 5)
		(uuid "cb6bd8a5-b21c-43ab-bf08-16378efed40a")
	)
	(segment
		(start 137.5 50.95)
		(end 137.5 48.3)
		(width 1.2)
		(layer "B.Cu")
		(net 5)
		(uuid "e39a21f6-51e9-4d75-a2ed-6da6a7f5ecc5")
	)
	(segment
		(start 123.2 44.9)
		(end 123.2 36.3)
		(width 0.3)
		(layer "B.Cu")
		(net 5)
		(uuid "f01452ce-4e77-47ed-b446-f96162236452")
	)
	(segment
		(start 76.7 49.7)
		(end 75.1 48.1)
		(width 0.3)
		(layer "F.Cu")
		(net 7)
		(uuid "25b9cc09-1e84-48cf-94ab-948707d1b2b3")
	)
	(segment
		(start 69.9 49.9125)
		(end 70.9 49.9125)
		(width 0.3)
		(layer "F.Cu")
		(net 7)
		(uuid "2b7202a0-88b2-41d0-aa14-0f8aab3a8412")
	)
	(segment
		(start 84.025 53.749999)
		(end 78.549999 53.749999)
		(width 0.3)
		(layer "F.Cu")
		(net 7)
		(uuid "2be79bb5-7570-447e-83f5-a7259633c707")
	)
	(segment
		(start 71.862501 49.9125)
		(end 71.9 49.949999)
		(width 0.3)
		(layer "F.Cu")
		(net 7)
		(uuid "69341ec3-fc7d-43af-8a0d-4677a90b1a3f")
	)
	(segment
		(start 75.1 48.1)
		(end 70.9 48.1)
		(width 0.3)
		(layer "F.Cu")
		(net 7)
		(uuid "71001baf-166e-4473-b061-c4d6d1ba512c")
	)
	(segment
		(start 70.9 49.9125)
		(end 71.862501 49.9125)
		(width 0.3)
		(layer "F.Cu")
		(net 7)
		(uuid "7ef9b2c8-66ef-476a-96bd-c9655a79cc26")
	)
	(segment
		(start 76.7 51.9)
		(end 76.7 49.7)
		(width 0.3)
		(layer "F.Cu")
		(net 7)
		(uuid "aa29ba1b-1888-44a2-aa15-de5d67b8ab76")
	)
	(segment
		(start 78.549999 53.749999)
		(end 76.7 51.9)
		(width 0.3)
		(layer "F.Cu")
		(net 7)
		(uuid "c964c7e5-2aa7-4b75-b96f-3cc78ea19c68")
	)
	(segment
		(start 70.9 48.1)
		(end 70.9 49.9125)
		(width 0.3)
		(layer "F.Cu")
		(net 7)
		(uuid "f06d7edd-8252-49e4-a5e2-4971ca1b1add")
	)
	(segment
		(start 78.85 53.25)
		(end 77.2 51.6)
		(width 0.3)
		(layer "F.Cu")
		(net 8)
		(uuid "02d26a1e-7178-432d-8d6b-0362cbf19471")
	)
	(segment
		(start 67.5 44.6)
		(end 66.9 45.2)
		(width 0.3)
		(layer "F.Cu")
		(net 8)
		(uuid "37b8d61e-59bf-42d6-956c-d4cf266a3fa7")
	)
	(segment
		(start 66.9 48.1)
		(end 66.9 49.9125)
		(width 0.3)
		(layer "F.Cu")
		(net 8)
		(uuid "4d28b7e5-b3cc-459d-aa55-18efd5c7050d")
	)
	(segment
		(start 77.2 49.492893)
		(end 72.307107 44.6)
		(width 0.3)
		(layer "F.Cu")
		(net 8)
		(uuid "89724969-ba79-4d9f-b0d3-99ed3103c54f")
	)
	(segment
		(start 66.9 45.2)
		(end 66.9 48.1)
		(width 0.3)
		(layer "F.Cu")
		(net 8)
		(uuid "a809facb-fb4b-4968-b1e0-c4d390a132b2")
	)
	(segment
		(start 65.9 49.9125)
		(end 66.9 49.9125)
		(width 0.3)
		(layer "F.Cu")
		(net 8)
		(uuid "bf490c32-00ff-48ef-ae6b-ff6a49588945")
	)
	(segment
		(start 67.862501 49.9125)
		(end 67.9 49.949999)
		(width 0.3)
		(layer "F.Cu")
		(net 8)
		(uuid "c4e0f0ef-51b2-4a71-a9a5-291907fc11e4")
	)
	(segment
		(start 77.2 51.6)
		(end 77.2 49.492893)
		(width 0.3)
		(layer "F.Cu")
		(net 8)
		(uuid "cb153e64-dbe2-4642-ae81-d0e765a55792")
	)
	(segment
		(start 66.9 49.9125)
		(end 67.862501 49.9125)
		(width 0.3)
		(layer "F.Cu")
		(net 8)
		(uuid "d236f1fb-5163-4523-b7e5-86c8bae1a095")
	)
	(segment
		(start 72.307107 44.6)
		(end 67.5 44.6)
		(width 0.3)
		(layer "F.Cu")
		(net 8)
		(uuid "de8d6f5e-959b-4d61-bb85-89f85c79211d")
	)
	(segment
		(start 84.025 53.25)
		(end 78.85 53.25)
		(width 0.3)
		(layer "F.Cu")
		(net 8)
		(uuid "e7ccc187-3108-4eb5-a33c-d6d1a455711b")
	)
	(segment
		(start 61.9 49.9125)
		(end 62.9 49.9125)
		(width 0.3)
		(layer "F.Cu")
		(net 9)
		(uuid "15d82d17-0d6d-4c35-be2e-c4912c22e6a8")
	)
	(segment
		(start 72.514214 44.1)
		(end 63.7 44.1)
		(width 0.3)
		(layer "F.Cu")
		(net 9)
		(uuid "50977957-2e31-4652-85fd-4a93c7aaf3bb")
	)
	(segment
		(start 77.703553 51.396447)
		(end 77.703553 49.289339)
		(width 0.3)
		(layer "F.Cu")
		(net 9)
		(uuid "8c1ebcaa-0203-4294-a3e3-7e81118e6728")
	)
	(segment
		(start 77.703553 49.289339)
		(end 72.514214 44.1)
		(width 0.3)
		(layer "F.Cu")
		(net 9)
		(uuid "9183a79b-ab9b-45e4-8e04-2258754ec3ef")
	)
	(segment
		(start 62.9 44.9)
		(end 62.9 48.1)
		(width 0.3)
		(layer "F.Cu")
		(net 9)
		(uuid "9608cf98-f23b-4586-ae18-2fd72e3f68ed")
	)
	(segment
		(start 84.025 52.75)
		(end 79.057106 52.75)
		(width 0.3)
		(layer "F.Cu")
		(net 9)
		(uuid "a0412d11-2055-49b6-b532-fa966d7d433a")
	)
	(segment
		(start 63.7 44.1)
		(end 62.9 44.9)
		(width 0.3)
		(layer "F.Cu")
		(net 9)
		(uuid "a3554e9b-8f0f-4394-a470-f3d58133da3c")
	)
	(segment
		(start 62.9 48.1)
		(end 62.9 49.9125)
		(width 0.3)
		(layer "F.Cu")
		(net 9)
		(uuid "ae2d1751-e9a0-4cbc-9b64-cb88893dc8d4")
	)
	(segment
		(start 62.9 49.9125)
		(end 63.862501 49.9125)
		(width 0.3)
		(layer "F.Cu")
		(net 9)
		(uuid "b5fe100b-174a-4f3f-9809-478a98396a91")
	)
	(segment
		(start 79.057106 52.75)
		(end 77.703553 51.396447)
		(width 0.3)
		(layer "F.Cu")
		(net 9)
		(uuid "ed10994d-9a7c-4bc2-819e-bc10f40c41a0")
	)
	(segment
		(start 63.862501 49.9125)
		(end 63.9 49.949999)
		(width 0.3)
		(layer "F.Cu")
		(net 9)
		(uuid "ef35b30c-cb3b-4ee2-8171-ae9ab4b007f4")
	)
	(segment
		(start 78.810659 48.982233)
		(end 72.928426 43.1)
		(width 0.3)
		(layer "F.Cu")
		(net 10)
		(uuid "028c6ed2-20dc-48f4-836f-dd86d234b81d")
	)
	(segment
		(start 79.471318 51.75)
		(end 78.810659 51.089341)
		(width 0.3)
		(layer "F.Cu")
		(net 10)
		(uuid "06fca68b-9352-44e9-8b37-fd4fae227b2e")
	)
	(segment
		(start 54.9 49.9125)
		(end 55.862501 49.9125)
		(width 0.3)
		(layer "F.Cu")
		(net 10)
		(uuid "48b40dd2-13d1-442c-b44c-20f0f473799b")
	)
	(segment
		(start 78.810659 51.089341)
		(end 78.810659 48.982233)
		(width 0.3)
		(layer "F.Cu")
		(net 10)
		(uuid "5f470192-d6df-46b4-9cf3-f8d9fad1ba55")
	)
	(segment
		(start 53.9 49.9125)
		(end 54.9 49.9125)
		(width 0.3)
		(layer "F.Cu")
		(net 10)
		(uuid "5fbe7f90-5a7c-4b68-918d-e6e395d07a22")
	)
	(segment
		(start 84.025 51.75)
		(end 79.471318 51.75)
		(width 0.3)
		(layer "F.Cu")
		(net 10)
		(uuid "621dbb7c-aee6-4412-b5d1-3bc78340461c")
	)
	(segment
		(start 54.9 48.1)
		(end 54.9 49.9125)
		(width 0.3)
		(layer "F.Cu")
		(net 10)
		(uuid "892261e6-c274-44cf-9672-52ece393998f")
	)
	(segment
		(start 54.9 45)
		(end 54.9 48.1)
		(width 0.3)
		(layer "F.Cu")
		(net 10)
		(uuid "9eb0d268-1a96-4e4f-88bf-45b5089fecc1")
	)
	(segment
		(start 55.862501 49.9125)
		(end 55.9 49.949999)
		(width 0.3)
		(layer "F.Cu")
		(net 10)
		(uuid "c21241bd-9dc8-4fe1-a274-ed65f52bdb8e")
	)
	(segment
		(start 56.8 43.1)
		(end 54.9 45)
		(width 0.3)
		(layer "F.Cu")
		(net 10)
		(uuid "c39743ac-9442-4d3a-b8a4-628c748f1a81")
	)
	(segment
		(start 72.928426 43.1)
		(end 56.8 43.1)
		(width 0.3)
		(layer "F.Cu")
		(net 10)
		(uuid "d790c7e7-957b-4778-b1f4-886a76430cc0")
	)
	(segment
		(start 78.257106 49.135786)
		(end 72.72132 43.6)
		(width 0.3)
		(layer "F.Cu")
		(net 11)
		(uuid "1070a1dd-b4c0-426d-b529-297ff1bf0c76")
	)
	(segment
		(start 79.264212 52.25)
		(end 78.257106 51.242894)
		(width 0.3)
		(layer "F.Cu")
		(net 11)
		(uuid "31ecb16f-5175-4845-836f-88c6cb0d3093")
	)
	(segment
		(start 84.025 52.25)
		(end 79.264212 52.25)
		(width 0.3)
		(layer "F.Cu")
		(net 11)
		(uuid "367848af-bf28-4b0c-a5bc-22c4439c859d")
	)
	(segment
		(start 78.257106 51.242894)
		(end 78.257106 49.135786)
		(width 0.3)
		(layer "F.Cu")
		(net 11)
		(uuid "4dfab476-c314-44da-8b72-57bce7eded46")
	)
	(segment
		(start 72.72132 43.6)
		(end 60.3 43.6)
		(width 0.3)
		(layer "F.Cu")
		(net 11)
		(uuid "7875911f-c8b6-4e58-9b5e-026ec77d442c")
	)
	(segment
		(start 59.862501 49.9125)
		(end 59.9 49.949999)
		(width 0.3)
		(layer "F.Cu")
		(net 11)
		(uuid "80a13f1a-7089-4bd2-be92-48716a1a7c84")
	)
	(segment
		(start 57.9 49.9125)
		(end 58.9 49.9125)
		(width 0.3)
		(layer "F.Cu")
		(net 11)
		(uuid "8ee649ac-e34d-43d1-a607-5e65c0f0e612")
	)
	(segment
		(start 58.9 49.9125)
		(end 59.862501 49.9125)
		(width 0.3)
		(layer "F.Cu")
		(net 11)
		(uuid "8f208dea-1f53-40f9-a1bc-02026d522ccd")
	)
	(segment
		(start 60.3 43.6)
		(end 58.9 45)
		(width 0.3)
		(layer "F.Cu")
		(net 11)
		(uuid "b6f56e24-7b7b-43d6-a518-93c8a07ae459")
	)
	(segment
		(start 58.9 45)
		(end 58.9 48.1)
		(width 0.3)
		(layer "F.Cu")
		(net 11)
		(uuid "d69b3fa8-fee5-4c2c-9a49-6f5977ecd9d1")
	)
	(segment
		(start 58.9 48.1)
		(end 58.9 49.9125)
		(width 0.3)
		(layer "F.Cu")
		(net 11)
		(uuid "fb51366a-e754-401c-8106-00a8f3c51ffa")
	)
	(segment
		(start 39.325 45.305)
		(end 40.795 45.305)
		(width 0.6)
		(layer "F.Cu")
		(net 12)
		(uuid "3dd50b18-9ec7-4ca6-ae59-bd69f6c97ed7")
	)
	(segment
		(start 41.595 53.095)
		(end 40.8 52.3)
		(width 0.6)
		(layer "F.Cu")
		(net 12)
		(uuid "5ae4776e-a668-4850-8cc1-2e7c7bb60423")
	)
	(segment
		(start 40.795 45.305)
		(end 40.8 45.3)
		(width 0.6)
		(layer "F.Cu")
		(net 12)
		(uuid "92938496-c419-4c26-a49d-7e53371eddf6")
	)
	(segment
		(start 43.275 53.095)
		(end 41.595 53.095)
		(width 0.6)
		(layer "F.Cu")
		(net 12)
		(uuid "c004c7ac-5d22-4112-8191-5332ca80986f")
	)
	(via
		(at 40.8 45.3)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 12)
		(uuid "68745817-3797-4081-89fc-4c029f33da16")
	)
	(via
		(at 40.8 52.3)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 12)
		(uuid "9eca9e01-da9e-4cf8-b522-e338cc856316")
	)
	(segment
		(start 60.9 38.2875)
		(end 42.6125 38.2875)
		(width 0.6)
		(layer "B.Cu")
		(net 12)
		(uuid "018cd935-96bd-4e39-b148-586544e86671")
	)
	(segment
		(start 40.850001 43.4)
		(end 40.850001 43.850001)
		(width 0.6)
		(layer "B.Cu")
		(net 12)
		(uuid "25f5b955-f3c9-43d6-aadd-1a6cc77f87a1")
	)
	(segment
		(start 66.000001 41.4)
		(end 66.000001 38.900001)
		(width 0.6)
		(layer "B.Cu")
		(net 12)
		(uuid "355ac83c-e39f-402c-9b98-5385c5b814a4")
	)
	(segment
		(start 40.8 45.3)
		(end 40.8 52.3)
		(width 0.6)
		(layer "B.Cu")
		(net 12)
		(uuid "41c107f3-efdf-44c3-b538-11c7eeacf5f7")
	)
	(segment
		(start 66.000001 38.900001)
		(end 65.3875 38.2875)
		(width 0.6)
		(layer "B.Cu")
		(net 12)
		(uuid "495db8c0-3ad2-4ebb-a38d-730225a3699d")
	)
	(segment
		(start 42.6125 38.2875)
		(end 40.850001 40.049999)
		(width 0.6)
		(layer "B.Cu")
		(net 12)
		(uuid "4baf1aec-324f-4294-9bde-ea0348dd330d")
	)
	(segment
		(start 40.850001 40.049999)
		(end 40.850001 43.4)
		(width 0.6)
		(layer "B.Cu")
		(net 12)
		(uuid "655fab50-b1be-420c-af09-7ab3778c4655")
	)
	(segment
		(start 65.3875 38.2875)
		(end 60.9 38.2875)
		(width 0.6)
		(layer "B.Cu")
		(net 12)
		(uuid "745f4e53-01be-4765-bc32-a27c99674809")
	)
	(segment
		(start 40.8 43.900002)
		(end 40.8 45.3)
		(width 0.6)
		(layer "B.Cu")
		(net 12)
		(uuid "83600bd4-5d8b-4032-8505-1b410227a43c")
	)
	(segment
		(start 40.8 52.3)
		(end 40.8 53.550001)
		(width 0.6)
		(layer "B.Cu")
		(net 12)
		(uuid "8afb1fe5-6f9e-41cd-aebf-5f4ef2ceee49")
	)
	(segment
		(start 40.850001 43.850001)
		(end 40.8 43.900002)
		(width 0.6)
		(layer "B.Cu")
		(net 12)
		(uuid "d5934b03-8a8e-45a0-9985-db4939b35fc0")
	)
	(segment
		(start 93.817505 51.382494)
		(end 94.099999 51.1)
		(width 0.5)
		(layer "B.Cu")
		(net 13)
		(uuid "06b626de-f687-4418-8629-8c2fa4342ae0")
	)
	(segment
		(start 93.649999 53.8)
		(end 93.817505 53.632494)
		(width 0.5)
		(layer "B.Cu")
		(net 13)
		(uuid "dfdc3d07-7ffb-49db-aea6-b06413cef66e")
	)
	(segment
		(start 93.817505 53.632494)
		(end 93.817505 51.382494)
		(width 0.5)
		(layer "B.Cu")
		(net 13)
		(uuid "f1889b67-1750-4467-969a-c05ac2a219af")
	)
	(segment
		(start 36.0525 55.635)
		(end 36 55.6875)
		(width 0.3)
		(layer "F.Cu")
		(net 14)
		(uuid "cc50ed87-c3b0-4449-82d3-4c03728c6000")
	)
	(segment
		(start 38.325 55.635)
		(end 36.0525 55.635)
		(width 0.3)
		(layer "F.Cu")
		(net 14)
		(uuid "cf48861c-570e-464b-b444-776ebeec3919")
	)
	(via
		(at 36 55.7)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 14)
		(uuid "0e566a2b-c752-4daf-a440-c6324608ea91")
	)
	(segment
		(start 38.3 55.650001)
		(end 36.000001 55.650001)
		(width 0.3)
		(layer "B.Cu")
		(net 14)
		(uuid "42b496b1-06bd-4e0a-9c3a-9253c32efdbf")
	)
	(segment
		(start 36.000001 55.650001)
		(end 36 55.65)
		(width 0.3)
		(layer "B.Cu")
		(net 14)
		(uuid "66a9f4b6-e923-4194-8967-214b8fd4cfe5")
	)
	(segment
		(start 45.5825 56.905)
		(end 45.6 56.8875)
		(width 0.3)
		(layer "F.Cu")
		(net 15)
		(uuid "10e96161-bb0f-41dc-8357-d24d7d3c5ffa")
	)
	(segment
		(start 43.275 56.905)
		(end 45.5825 56.905)
		(width 0.3)
		(layer "F.Cu")
		(net 15)
		(uuid "9bfb5120-0199-4136-a222-72e7f1249658")
	)
	(via
		(at 45.6 56.9)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 15)
		(uuid "18392442-841f-4961-8f3d-c05ab4e10647")
	)
	(segment
		(start 43.3 56.850001)
		(end 45.599999 56.850001)
		(width 0.3)
		(layer "B.Cu")
		(net 15)
		(uuid "53caf235-48df-426b-8555-ccb77e4e13bc")
	)
	(segment
		(start 45.599999 56.850001)
		(end 45.6 56.85)
		(width 0.3)
		(layer "B.Cu")
		(net 15)
		(uuid "7f34cd81-6cea-4bb0-b397-a9afd34f9d45")
	)
	(segment
		(start 45.6 42.5)
		(end 45.6 42)
		(width 0.3)
		(layer "F.Cu")
		(net 16)
		(uuid "20bd32af-1b89-4fbb-b9da-93dd2bb31abd")
	)
	(segment
		(start 45.9 41.7)
		(end 46.4 41.7)
		(width 0.3)
		(layer "F.Cu")
		(net 16)
		(uuid "3ab9a51f-a71c-41b0-b81a-50b1169118c1")
	)
	(segment
		(start 45.335 42.765)
		(end 45.6 42.5)
		(width 0.3)
		(layer "F.Cu")
		(net 16)
		(uuid "715fa605-7b60-4ff0-9fea-0a053a47d175")
	)
	(segment
		(start 45.6 42)
		(end 45.9 41.7)
		(width 0.3)
		(layer "F.Cu")
		(net 16)
		(uuid "e25968da-362e-4e0f-a27e-91c92afd3aee")
	)
	(segment
		(start 44.275 42.765)
		(end 45.335 42.765)
		(width 0.3)
		(layer "F.Cu")
		(net 16)
		(uuid "f6e6158e-9157-4da6-bbad-fd70082e3dfd")
	)
	(via
		(at 46.4 41.7)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 16)
		(uuid "5f7fb48a-892b-4b3d-bd39-f86209793b69")
	)
	(segment
		(start 38 41.2)
		(end 38 40.9)
		(width 0.3)
		(layer "F.Cu")
		(net 17)
		(uuid "4d90404c-ca1b-491a-a159-40e3510e3754")
	)
	(segment
		(start 37.7 40.6)
		(end 37.0125 40.6)
		(width 0.3)
		(layer "F.Cu")
		(net 17)
		(uuid "8b087f08-9e61-4773-b080-e1d0b2ed11d4")
	)
	(segment
		(start 38 40.9)
		(end 37.7 40.6)
		(width 0.3)
		(layer "F.Cu")
		(net 17)
		(uuid "a14245d8-2bfe-4325-83fd-a12419c01e5f")
	)
	(segment
		(start 39.325 41.495)
		(end 38.295 41.495)
		(width 0.3)
		(layer "F.Cu")
		(net 17)
		(uuid "bc0478ca-8866-4d9c-bcaa-e97b9400a95a")
	)
	(segment
		(start 38.295 41.495)
		(end 38 41.2)
		(width 0.3)
		(layer "F.Cu")
		(net 17)
		(uuid "db067a88-b38a-47c9-9ff3-1f75725e21fb")
	)
	(via
		(at 37.0125 40.6)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 17)
		(uuid "e2259e3e-369a-492e-a61f-1c098456cbd9")
	)
	(segment
		(start 92.287502 39.550001)
		(end 92.3 39.562499)
		(width 0.3)
		(layer "F.Cu")
		(net 18)
		(uuid "03b8ee99-9b01-4d2d-900e-52d534b4af96")
	)
	(segment
		(start 85.5 39.5875)
		(end 87.5 39.5875)
		(width 0.3)
		(layer "F.Cu")
		(net 18)
		(uuid "04b5704e-7c12-4542-8d81-90ad91cfd6ab")
	)
	(segment
		(start 87.5 39.5875)
		(end 89.462501 39.5875)
		(width 0.3)
		(layer "F.Cu")
		(net 18)
		(uuid "6eec98ae-98b9-442e-b6f7-c919523351d9")
	)
	(segment
		(start 89.5 39.550001)
		(end 92.287502 39.550001)
		(width 0.3)
		(layer "F.Cu")
		(net 18)
		(uuid "7eacddf7-59e1-4ada-95a2-d87c36fdfb0d")
	)
	(segment
		(start 89.462501 39.5875)
		(end 89.5 39.550001)
		(width 0.3)
		(layer "F.Cu")
		(net 18)
		(uuid "9f1b2600-e121-459d-a9e7-cc715316eb3d")
	)
	(segment
		(start 89.462501 39.5875)
		(end 89.5 39.550001)
		(width 0.3)
		(layer "B.Cu")
		(net 19)
		(uuid "29f275da-54dc-40e8-b98e-d3520d6425e0")
	)
	(segment
		(start 87.5 39.5875)
		(end 89.462501 39.5875)
		(width 0.3)
		(layer "B.Cu")
		(net 19)
		(uuid "33b91acf-2854-4a91-952b-d1858b41dda7")
	)
	(segment
		(start 85.5 39.587499)
		(end 87.499999 39.587499)
		(width 0.3)
		(layer "B.Cu")
		(net 19)
		(uuid "3c7f8938-323e-49f2-99d8-82451510f632")
	)
	(segment
		(start 89.5 39.550001)
		(end 92.287502 39.550001)
		(width 0.3)
		(layer "B.Cu")
		(net 19)
		(uuid "3dd6068e-f668-4cb1-b84b-02e9a0f12a6f")
	)
	(segment
		(start 92.287502 39.550001)
		(end 92.3 39.562499)
		(width 0.3)
		(layer "B.Cu")
		(net 19)
		(uuid "53538a11-356c-426c-a890-c5b79e0ac7e9")
	)
	(segment
		(start 87.499999 39.587499)
		(end 87.5 39.5875)
		(width 0.3)
		(layer "B.Cu")
		(net 19)
		(uuid "d67bfa70-32b0-4685-b648-30e9f03cec30")
	)
	(segment
		(start 116.465 40.165)
		(end 114.275 40.165)
		(width 0.3)
		(layer "F.Cu")
		(net 20)
		(uuid "113ebd7c-07ba-4af2-9007-d71b82b72eda")
	)
	(segment
		(start 118.14 41.84)
		(end 116.465 40.165)
		(width 0.3)
		(layer "F.Cu")
		(net 20)
		(uuid "a9d2c3b2-4660-477e-8a27-30ab9e21cfde")
	)
	(segment
		(start 126.3 41.84)
		(end 118.14 41.84)
		(width 0.3)
		(layer "F.Cu")
		(net 20)
		(uuid "cd631e55-3cf8-40f5-9b39-c250ca651a50")
	)
	(segment
		(start 107.105 38.895)
		(end 105.9 40.1)
		(width 0.3)
		(layer "F.Cu")
		(net 21)
		(uuid "05713b4d-cdff-4923-bdba-c01bf4c44bef")
	)
	(segment
		(start 105.9 40.1)
		(end 105.9 59)
		(width 0.3)
		(layer "F.Cu")
		(net 21)
		(uuid "07f5f0b5-8d4c-42f3-be1d-82bef071416d")
	)
	(segment
		(start 105.9 59)
		(end 105.2 59.7)
		(width 0.3)
		(layer "F.Cu")
		(net 21)
		(uuid "11703d89-53f4-4766-bc72-5c608b7801d6")
	)
	(segment
		(start 90.949999 59.349999)
		(end 90.949999 58.175)
		(width 0.3)
		(layer "F.Cu")
		(net 21)
		(uuid "48986853-1a9a-47fb-8dac-661e45d2bcae")
	)
	(segment
		(start 109.325 38.895)
		(end 107.105 38.895)
		(width 0.3)
		(layer "F.Cu")
		(net 21)
		(uuid "55491ce9-b837-4f34-b318-d8e09700bf2d")
	)
	(segment
		(start 91.3 59.7)
		(end 90.949999 59.349999)
		(width 0.3)
		(layer "F.Cu")
		(net 21)
		(uuid "aeac3d22-821a-4951-a55c-a087cf6d2bbc")
	)
	(segment
		(start 105.2 59.7)
		(end 91.3 59.7)
		(width 0.3)
		(layer "F.Cu")
		(net 21)
		(uuid "b6826907-19a3-4987-8d06-57343f3dae4d")
	)
	(segment
		(start 89.6 59.7)
		(end 89.95 59.35)
		(width 0.3)
		(layer "F.Cu")
		(net 22)
		(uuid "176618ce-b267-4430-9963-7553f67df0d9")
	)
	(segment
		(start 109.325 40.165)
		(end 107.235 40.165)
		(width 0.3)
		(layer "F.Cu")
		(net 22)
		(uuid "3dc78736-1d05-4cd1-aad8-e26bc4e59a11")
	)
	(segment
		(start 89.95 59.35)
		(end 89.95 58.175)
		(width 0.3)
		(layer "F.Cu")
		(net 22)
		(uuid "451decbb-034c-40a4-be3a-7b22bef053b1")
	)
	(segment
		(start 106.635 41.435)
		(end 106.6 41.4)
		(width 0.3)
		(layer "F.Cu")
		(net 22)
		(uuid "587a2d0c-a714-4b31-9f58-24eae64334e7")
	)
	(segment
		(start 106.6 59.307107)
		(end 106.6 41.4)
		(width 0.3)
		(layer "F.Cu")
		(net 22)
		(uuid "74033364-487c-4a35-ac3f-6f7ea670458b")
	)
	(segment
		(start 91.25 60.5)
		(end 105.407107 60.5)
		(width 0.3)
		(layer "F.Cu")
		(net 22)
		(uuid "775edfc6-319b-4e70-bf8b-4903742ca899")
	)
	(segment
		(start 106.6 40.8)
		(end 106.6 41.4)
		(width 0.3)
		(layer "F.Cu")
		(net 22)
		(uuid "8cac4e41-d2bf-40f8-81c7-a8ae7bcc9388")
	)
	(segment
		(start 107.235 40.165)
		(end 106.6 40.8)
		(width 0.3)
		(layer "F.Cu")
		(net 22)
		(uuid "bc1691c9-ede2-436d-8a1f-b7700db20a5e")
	)
	(segment
		(start 109.325 41.435)
		(end 106.635 41.435)
		(width 0.3)
		(layer "F.Cu")
		(net 22)
		(uuid "bc3a6e6b-de44-4085-916c-aaff660ade56")
	)
	(segment
		(start 89.6 60.5)
		(end 89.6 59.7)
		(width 0.3)
		(layer "F.Cu")
		(net 22)
		(uuid "c963801b-8d0e-417f-b8f7-5407a3641878")
	)
	(segment
		(start 105.407107 60.5)
		(end 106.6 59.307107)
		(width 0.3)
		(layer "F.Cu")
		(net 22)
		(uuid "f0c915a9-bd2b-40e6-b4cd-f13ef47e3a26")
	)
	(via
		(at 106.65 41.435)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 22)
		(uuid "1d02b6de-1c21-4da5-89b9-f68319c4e60a")
	)
	(via
		(at 91.25 60.5)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 22)
		(uuid "d2a7e009-1a27-4c3c-be45-72317c45d930")
	)
	(via
		(at 89.6 60.5)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 22)
		(uuid "f1ca1af0-b740-462b-a99b-cba4efe623ef")
	)
	(segment
		(start 91.25 60.5)
		(end 89.6 60.5)
		(width 0.3)
		(layer "B.Cu")
		(net 22)
		(uuid "2e16fd2c-5ad5-45c2-a26c-2f6206186b8e")
	)
	(segment
		(start 106.6 43.1875)
		(end 106.6 41.485)
		(width 0.3)
		(layer "B.Cu")
		(net 22)
		(uuid "817a5cee-dd9f-4b23-97ee-c7d566264d40")
	)
	(segment
		(start 106.6 41.485)
		(end 106.65 41.435)
		(width 0.3)
		(layer "B.Cu")
		(net 22)
		(uuid "f70f522f-d80c-431c-8e29-5ac62ae3d3ed")
	)
	(segment
		(start 114.275 41.435)
		(end 116.235 41.435)
		(width 0.3)
		(layer "F.Cu")
		(net 23)
		(uuid "331ec86f-3283-457b-af38-e8b46133489d")
	)
	(segment
		(start 124.78 44.38)
		(end 126.3 44.38)
		(width 0.3)
		(layer "F.Cu")
		(net 23)
		(uuid "715c4978-3a2b-43aa-a8a5-7dcaa265dc6b")
	)
	(segment
		(start 123.5 43.1)
		(end 124.78 44.38)
		(width 0.3)
		(layer "F.Cu")
		(net 23)
		(uuid "751f8d98-05e2-4648-8982-8fd0ff81b171")
	)
	(segment
		(start 117.9 43.1)
		(end 123.5 43.1)
		(width 0.3)
		(layer "F.Cu")
		(net 23)
		(uuid "e389adbb-df68-42d0-b496-528e35a429ef")
	)
	(segment
		(start 116.235 41.435)
		(end 117.9 43.1)
		(width 0.3)
		(layer "F.Cu")
		(net 23)
		(uuid "fd2fce10-8823-4de3-8979-a64eec700788")
	)
	(segment
		(start 105.6 61.3)
		(end 90.8 61.3)
		(width 0.3)
		(layer "F.Cu")
		(net 24)
		(uuid "091ab243-a16a-4915-8d50-c1d97b874722")
	)
	(segment
		(start 90.45 60.95)
		(end 90.45 58.175)
		(width 0.3)
		(layer "F.Cu")
		(net 24)
		(uuid "09b4199b-405c-4ac6-bb60-dff1457a36f2")
	)
	(segment
		(start 109.325 42.705)
		(end 107.695 42.705)
		(width 0.3)
		(layer "F.Cu")
		(net 24)
		(uuid "123b710b-63c3-4de9-8d1c-2f30a5bf0657")
	)
	(segment
		(start 107.3 43.1)
		(end 107.3 59.6)
		(width 0.3)
		(layer "F.Cu")
		(net 24)
		(uuid "32d803ca-0977-44e9-b854-a3c9d235fdda")
	)
	(segment
		(start 107.3 59.6)
		(end 105.6 61.3)
		(width 0.3)
		(layer "F.Cu")
		(net 24)
		(uuid "7f78b2ba-2bd1-4e16-98ab-a5dbcf8b7ef1")
	)
	(segment
		(start 107.695 42.705)
		(end 107.3 43.1)
		(width 0.3)
		(layer "F.Cu")
		(net 24)
		(uuid "8c39af8f-a858-4c6c-86c9-308d61268ba9")
	)
	(segment
		(start 90.8 61.3)
		(end 90.45 60.95)
		(width 0.3)
		(layer "F.Cu")
		(net 24)
		(uuid "b46a64ff-df89-49f7-9a09-fdae3ba477b6")
	)
	(segment
		(start 123.185 57.315)
		(end 118.6 61.9)
		(width 0.3)
		(layer "F.Cu")
		(net 25)
		(uuid "135f0c86-311c-4b9d-b55b-c1c20ea28b3c")
	)
	(segment
		(start 89.4 61.9)
		(end 88.8 61.3)
		(width 0.3)
		(layer "F.Cu")
		(net 25)
		(uuid "181df3a0-f73e-45af-84ba-34bf8e5b0dc5")
	)
	(segment
		(start 88.8 61.3)
		(end 88.8 59.7)
		(width 0.3)
		(layer "F.Cu")
		(net 25)
		(uuid "2bf079af-7733-4233-94ad-970989f39361")
	)
	(segment
		(start 127.69 57.315)
		(end 123.185 57.315)
		(width 0.3)
		(layer "F.Cu")
		(net 25)
		(uuid "36d7ae56-9aa6-49c5-9d38-9b5fc3163102")
	)
	(segment
		(start 128.89 58.515)
		(end 127.69 57.315)
		(width 0.3)
		(layer "F.Cu")
		(net 25)
		(uuid "4d0b8f52-2456-4e8c-b75e-e6b61a7b82f3")
	)
	(segment
		(start 118.6 61.9)
		(end 89.4 61.9)
		(width 0.3)
		(layer "F.Cu")
		(net 25)
		(uuid "56c0292f-adc5-4d79-87e5-11ea49661957")
	)
	(segment
		(start 88.8 59.7)
		(end 88.95 59.55)
		(width 0.3)
		(layer "F.Cu")
		(net 25)
		(uuid "b120d2a3-e9b4-4657-b061-118bc9aeb02d")
	)
	(segment
		(start 88.95 59.55)
		(end 88.95 58.175)
		(width 0.3)
		(layer "F.Cu")
		(net 25)
		(uuid "ee8343c7-d6aa-4de3-840e-ea6664f1710a")
	)
	(segment
		(start 48.3125 39.750001)
		(end 48.3125 41.7)
		(width 0.3)
		(layer "F.Cu")
		(net 29)
		(uuid "1eb2c7fc-672f-41ac-bbbe-4fbe5f7df08b")
	)
	(segment
		(start 48.3125 41.7)
		(end 50.050001 41.7)
		(width 0.3)
		(layer "F.Cu")
		(net 29)
		(uuid "320ac5e5-5eca-4eb0-9a86-76e44a1a80bc")
	)
	(segment
		(start 50.050001 41.7)
		(end 50.2 41.550001)
		(width 0.3)
		(layer "F.Cu")
		(net 29)
		(uuid "ffd36994-7cbf-43bf-836e-67098d1a8abc")
	)
	(segment
		(start 85.4 59.6)
		(end 85.950001 59.049999)
		(width 0.3)
		(layer "F.Cu")
		(net 30)
		(uuid "086d56a0-75fc-4ddd-b840-47e4d8677477")
	)
	(segment
		(start 85.950001 59.049999)
		(end 85.950001 58.175)
		(width 0.3)
		(layer "F.Cu")
		(net 30)
		(uuid "26bdf8cb-e6cd-4bf9-9c8a-81e1a5632d28")
	)
	(segment
		(start 85.4 60.7)
		(end 85.4 59.6)
		(width 0.3)
		(layer "F.Cu")
		(net 30)
		(uuid "abb37201-f3a9-4ccd-89d2-9f68905db847")
	)
	(segment
		(start 87.1 62.4)
		(end 85.4 60.7)
		(width 0.3)
		(layer "F.Cu")
		(net 30)
		(uuid "c8f019b9-7106-4021-8c25-bfae6a6f4192")
	)
	(segment
		(start 126.35 58.515)
		(end 123.085 58.515)
		(width 0.3)
		(layer "F.Cu")
		(net 30)
		(uuid "cc29a902-3d51-407c-9f0f-a4429c44063d")
	)
	(segment
		(start 123.085 58.515)
		(end 119.2 62.4)
		(width 0.3)
		(layer "F.Cu")
		(net 30)
		(uuid "e009847f-7d6a-4bdf-bfbb-3bf883fbec19")
	)
	(segment
		(start 119.2 62.4)
		(end 87.1 62.4)
		(width 0.3)
		(layer "F.Cu")
		(net 30)
		(uuid "ea6c863c-5a1b-4b2e-aa1c-7bab501650fb")
	)
	(segment
		(start 86.95 58.175)
		(end 86.95 59.750001)
		(width 0.3)
		(layer "F.Cu")
		(net 36)
		(uuid "33462742-b33b-4fb1-a601-51223b0a6b4e")
	)
	(segment
		(start 86.95 59.750001)
		(end 86.6 60.100001)
		(width 0.3)
		(layer "F.Cu")
		(net 36)
		(uuid "a3fcd673-e114-44cd-85f0-f46b9f974d36")
	)
	(segment
		(start 96.95 53.25)
		(end 95.375 53.25)
		(width 0.3)
		(layer "F.Cu")
		(net 38)
		(uuid "6fb81fc9-59fc-4cfe-8dfd-877b833e4086")
	)
	(segment
		(start 97.4 52.8)
		(end 96.95 53.25)
		(width 0.3)
		(layer "F.Cu")
		(net 38)
		(uuid "d90a2f4d-d993-4621-8141-dfaf483c0fca")
	)
	(via
		(at 97.4 52.8)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 38)
		(uuid "f2982c87-3ceb-4555-8947-e1a9a5042d5a")
	)
	(segment
		(start 108.75 60.35)
		(end 98.55 60.35)
		(width 0.3)
		(layer "B.Cu")
		(net 38)
		(uuid "07bc0e25-41aa-41cc-bfd1-e787e680833f")
	)
	(segment
		(start 126.3075 61.0125)
		(end 126.35 61.055)
		(width 0.3)
		(layer "B.Cu")
		(net 38)
		(uuid "179e16b2-ba0e-409b-8e39-dae41b6da76b")
	)
	(segment
		(start 110.6 62.2)
		(end 108.75 60.35)
		(width 0.3)
		(layer "B.Cu")
		(net 38)
		(uuid "1847d50b-abcd-4f94-901e-8546e9a4a289")
	)
	(segment
		(start 121.4875 61.0125)
		(end 120.3 62.2)
		(width 0.3)
		(layer "B.Cu")
		(net 38)
		(uuid "3118b219-2846-4449-b96f-26b1a5c1333d")
	)
	(segment
		(start 97.5 59.3)
		(end 97.5 52.9)
		(width 0.3)
		(layer "B.Cu")
		(net 38)
		(uuid "4673348c-087c-464a-aa62-8fd603a646ac")
	)
	(segment
		(start 122.8 61.0125)
		(end 121.4875 61.0125)
		(width 0.3)
		(layer "B.Cu")
		(net 38)
		(uuid "49aab70b-3ee3-4f57-809b-c97c15a8cc48")
	)
	(segment
		(start 97.5 52.9)
		(end 97.4 52.8)
		(width 0.3)
		(layer "B.Cu")
		(net 38)
		(uuid "58d50e61-bb93-4116-bf25-0d59d0314930")
	)
	(segment
		(start 98.55 60.35)
		(end 97.5 59.3)
		(width 0.3)
		(layer "B.Cu")
		(net 38)
		(uuid "9931b9ae-ccad-4ac5-9a2f-8c7d8594371a")
	)
	(segment
		(start 122.8 61.0125)
		(end 126.3075 61.0125)
		(width 0.3)
		(layer "B.Cu")
		(net 38)
		(uuid "ca921f1f-83a0-4128-82df-13b066b1a174")
	)
	(segment
		(start 120.3 62.2)
		(end 110.6 62.2)
		(width 0.3)
		(layer "B.Cu")
		(net 38)
		(uuid "e1b4809f-7042-4544-b492-42f262c2a648")
	)
	(segment
		(start 126.35 55.975)
		(end 123.125 55.975)
		(width 0.3)
		(layer "F.Cu")
		(net 40)
		(uuid "7110c2b2-cd23-4f26-bbd8-3316deabee09")
	)
	(segment
		(start 81 55.3)
		(end 81.05 55.25)
		(width 0.3)
		(layer "F.Cu")
		(net 40)
		(uuid "acc6a6af-ff68-4f20-9ec2-b18ebef03e60")
	)
	(segment
		(start 118 61.1)
		(end 107.8 61.1)
		(width 0.3)
		(layer "F.Cu")
		(net 40)
		(uuid "bb0e9a81-600b-43f5-88f9-286df559a6b2")
	)
	(segment
		(start 81.05 55.25)
		(end 84.025 55.25)
		(width 0.3)
		(layer "F.Cu")
		(net 40)
		(uuid "d37c3510-a650-4047-9e49-547b104525cc")
	)
	(segment
		(start 123.125 55.975)
		(end 118 61.1)
		(width 0.3)
		(layer "F.Cu")
		(net 40)
		(uuid "f4c56764-c891-42e0-8d80-e95c62212a4e")
	)
	(via
		(at 107.8 61.1)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 40)
		(uuid "5d77fae7-1bdd-43cc-b664-2c95531c15ba")
	)
	(via
		(at 81 55.3)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 40)
		(uuid "a3ee1d3d-7961-45ea-a1b2-b87f61508af6")
	)
	(segment
		(start 85.7 61.5)
		(end 81.1 56.9)
		(width 0.3)
		(layer "B.Cu")
		(net 40)
		(uuid "217db4d5-867e-4d6d-8c5d-cecde0bb993d")
	)
	(segment
		(start 107.8 61.1)
		(end 107.4 61.5)
		(width 0.3)
		(layer "B.Cu")
		(net 40)
		(uuid "2637fa63-3097-4ab9-897a-134f89d38e47")
	)
	(segment
		(start 81.1 56.9)
		(end 81.1 55.4)
		(width 0.3)
		(layer "B.Cu")
		(net 40)
		(uuid "65c9ca60-132f-4740-bb1f-2b7015956c60")
	)
	(segment
		(start 107.4 61.5)
		(end 85.7 61.5)
		(width 0.3)
		(layer "B.Cu")
		(net 40)
		(uuid "7a5c84c9-8686-4b77-8620-7123febf9937")
	)
	(segment
		(start 81.1 55.4)
		(end 81 55.3)
		(width 0.3)
		(layer "B.Cu")
		(net 40)
		(uuid "bde8b450-d59d-4cbb-80d1-61076a844339")
	)
	(segment
		(start 84.025 49.75)
		(end 82.75 49.75)
		(width 0.3)
		(layer "F.Cu")
		(net 41)
		(uuid "1672eb56-b98c-44bc-8450-50ded6e3cf43")
	)
	(segment
		(start 82.75 49.75)
		(end 82 49)
		(width 0.3)
		(layer "F.Cu")
		(net 41)
		(uuid "6bc96ead-9185-41fb-8e56-81f41a9e4406")
	)
	(segment
		(start 35.974999 52.162499)
		(end 36 52.1875)
		(width 0.3)
		(layer "F.Cu")
		(net 43)
		(uuid "6201e939-9615-436b-a5b2-2796028875f4")
	)
	(segment
		(start 33.2 52.162499)
		(end 35.974999 52.162499)
		(width 0.3)
		(layer "F.Cu")
		(net 43)
		(uuid "f5b48751-0b54-4de5-8caa-d468987d7b36")
	)
	(via
		(at 36 52.2)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 43)
		(uuid "11198b14-9afb-464c-bc66-813ede494d0a")
	)
	(segment
		(start 37 51.2)
		(end 38.3 51.2)
		(width 0.3)
		(layer "B.Cu")
		(net 43)
		(uuid "5a3aeed7-63e6-45d0-b5ba-138fddbdf5ff")
	)
	(segment
		(start 36 52.2)
		(end 37 51.2)
		(width 0.3)
		(layer "B.Cu")
		(net 43)
		(uuid "5c94e395-3d28-4929-9088-41c457ca63fe")
	)
	(segment
		(start 33.949999 52.2)
		(end 33.9 52.150001)
		(width 0.3)
		(layer "B.Cu")
		(net 43)
		(uuid "8ea8301d-0daa-42bd-ac96-1a8000af98d8")
	)
	(segment
		(start 36 52.2)
		(end 33.949999 52.2)
		(width 0.3)
		(layer "B.Cu")
		(net 43)
		(uuid "96497789-bcb9-43ab-ad1c-5b81a6e36681")
	)
	(segment
		(start 87.45 59.749999)
		(end 87.800001 60.1)
		(width 0.3)
		(layer "F.Cu")
		(net 46)
		(uuid "8238b3e8-9deb-4521-b285-dc370d7db6f9")
	)
	(segment
		(start 87.45 58.175)
		(end 87.45 59.749999)
		(width 0.3)
		(layer "F.Cu")
		(net 46)
		(uuid "bec66d98-041a-4aaf-9bef-ef9f130f0d02")
	)
	(segment
		(start 73.135533 42.6)
		(end 55.8 42.6)
		(width 0.3)
		(layer "F.Cu")
		(net 47)
		(uuid "0f780f81-dd30-4603-900f-d4ccfd11c5b8")
	)
	(segment
		(start 79.310659 48.775126)
		(end 73.135533 42.6)
		(width 0.3)
		(layer "F.Cu")
		(net 47)
		(uuid "88441437-523e-4ff7-8ecb-0e3776bc3c02")
	)
	(segment
		(start 84.025 51.250001)
		(end 79.86066 51.250001)
		(width 0.3)
		(layer "F.Cu")
		(net 47)
		(uuid "9ad659e3-3ea5-41e7-ad70-bda33b5a4e89")
	)
	(segment
		(start 55.8 42.6)
		(end 54.8 43.6)
		(width 0.3)
		(layer "F.Cu")
		(net 47)
		(uuid "c42f5aff-9288-4ab2-b79a-5d7df734d26b")
	)
	(segment
		(start 79.310659 50.7)
		(end 79.310659 48.775126)
		(width 0.3)
		(layer "F.Cu")
		(net 47)
		(uuid "e157f274-debd-4a42-b00c-f137cd259fe3")
	)
	(segment
		(start 79.86066 51.250001)
		(end 79.310659 50.7)
		(width 0.3)
		(layer "F.Cu")
		(net 47)
		(uuid "e69b07a8-912f-4e57-80de-4f90f8d92e8b")
	)
	(via
		(at 54.8 43.6)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 47)
		(uuid "8046526b-0c2a-40e3-8c6c-a689147a64f6")
	)
	(segment
		(start 54.7875 47.8875)
		(end 54.7875 47.5)
		(width 0.3)
		(layer "B.Cu")
		(net 47)
		(uuid "59c98e30-5b22-43c4-a7d1-4930f1afbc21")
	)
	(segment
		(start 55.7 48.8)
		(end 54.7875 47.8875)
		(width 0.3)
		(layer "B.Cu")
		(net 47)
		(uuid "5dc4d9eb-8711-4cda-ba3f-434ca8347e1f")
	)
	(segment
		(start 54.8 43.6)
		(end 54.7875 43.6125)
		(width 0.3)
		(layer "B.Cu")
		(net 47)
		(uuid "7cb0c6db-ba93-462b-b484-1f04ad7ccfcc")
	)
	(segment
		(start 55.7 49.524999)
		(end 55.7 48.8)
		(width 0.3)
		(layer "B.Cu")
		(net 47)
		(uuid "b101adda-925e-47d4-9bd9-b663345049ff")
	)
	(segment
		(start 54.7875 43.6125)
		(end 54.7875 47.5)
		(width 0.3)
		(layer "B.Cu")
		(net 47)
		(uuid "d3c420c8-b43c-4ec0-9a88-c83e72a6b1a2")
	)
	(segment
		(start 35.1875 38.6)
		(end 35.1875 40.6)
		(width 0.3)
		(layer "F.Cu")
		(net 51)
		(uuid "02380516-5805-4f2a-90ba-bb0411d5cd1b")
	)
	(segment
		(start 33.649999 40.6)
		(end 33.4 40.350001)
		(width 0.3)
		(layer "F.Cu")
		(net 51)
		(uuid "9734b9f1-dcc2-4ab8-b55c-adbee88430bf")
	)
	(segment
		(start 35.1875 40.6)
		(end 33.649999 40.6)
		(width 0.3)
		(layer "F.Cu")
		(net 51)
		(uuid "e1d03130-b603-4a5a-a37b-bb1491c2a074")
	)
	(segment
		(start 84.025 48.750001)
		(end 84.025 48.625)
		(width 0.3)
		(layer "F.Cu")
		(net 53)
		(uuid "6c90eb82-4d8a-46b2-89ed-73b91ad94821")
	)
	(segment
		(start 84.025 48.625)
		(end 82 46.6)
		(width 0.3)
		(layer "F.Cu")
		(net 53)
		(uuid "d9bfea3a-942e-46fa-89df-72f5e911b236")
	)
	(segment
		(start 77.4 54.2)
		(end 77.45 54.25)
		(width 0.3)
		(layer "F.Cu")
		(net 54)
		(uuid "99b869ae-df88-414c-a63c-b9096b468f2b")
	)
	(segment
		(start 77.45 54.25)
		(end 84.025 54.25)
		(width 0.3)
		(layer "F.Cu")
		(net 54)
		(uuid "b17a583d-95b4-42dc-9bd3-b80f6fc70afe")
	)
	(via
		(at 77.4 54.2)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 54)
		(uuid "ebb7887a-0041-4af0-a0c3-ae77e212b5a8")
	)
	(segment
		(start 72.1 53.9)
		(end 69.9125 51.7125)
		(width 0.3)
		(layer "B.Cu")
		(net 54)
		(uuid "3ceedf69-cb1c-43ab-a295-353b92a556cb")
	)
	(segment
		(start 67.0875 51.7)
		(end 67.1 51.7125)
		(width 0.3)
		(layer "B.Cu")
		(net 54)
		(uuid "4a2b56a9-7676-4d6c-ad87-f662cff48062")
	)
	(segment
		(start 64.3 56.33)
		(end 64.255 56.375)
		(width 0.3)
		(layer "B.Cu")
		(net 54)
		(uuid "6e8e8532-671b-4cf5-b1a0-159541dce527")
	)
	(segment
		(start 77.1 53.9)
		(end 72.1 53.9)
		(width 0.3)
		(layer "B.Cu")
		(net 54)
		(uuid "8031a70f-2e4d-41f1-b3fa-2af9b036d1f8")
	)
	(segment
		(start 64.3 51.7)
		(end 64.3 56.33)
		(width 0.3)
		(layer "B.Cu")
		(net 54)
		(uuid "88391cbd-2e46-4fe8-a1ce-d85db91297f5")
	)
	(segment
		(start 69.9125 51.7125)
		(end 67.1 51.7125)
		(width 0.3)
		(layer "B.Cu")
		(net 54)
		(uuid "a82db604-de37-4343-a997-82602f11234b")
	)
	(segment
		(start 77.4 54.2)
		(end 77.1 53.9)
		(width 0.3)
		(layer "B.Cu")
		(net 54)
		(uuid "db1f5308-8d33-4a03-a4bc-ee53f587b6b0")
	)
	(segment
		(start 64.3 51.7)
		(end 67.0875 51.7)
		(width 0.3)
		(layer "B.Cu")
		(net 54)
		(uuid "ffd80810-f274-408b-8a7a-20f815dd252b")
	)
	(segment
		(start 45.6 53.4)
		(end 48.362499 53.4)
		(width 0.3)
		(layer "F.Cu")
		(net 55)
		(uuid "8cf1a823-6389-46e4-b2e6-765affa823b9")
	)
	(segment
		(start 48.362499 53.4)
		(end 48.4 53.362499)
		(width 0.3)
		(layer "F.Cu")
		(net 55)
		(uuid "d4238c4f-33ce-4d7e-a322-96ec1b7fc8a2")
	)
	(via
		(at 45.6 53.4)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 55)
		(uuid "321e85df-7cda-4be3-a0f9-4a6eaa625183")
	)
	(segment
		(start 44.8 51.2)
		(end 43.3 51.2)
		(width 0.3)
		(layer "B.Cu")
		(net 55)
		(uuid "3259befa-7870-4461-91d1-a66eb7e42d04")
	)
	(segment
		(start 45.6 53.4)
		(end 47.650001 53.4)
		(width 0.3)
		(layer "B.Cu")
		(net 55)
		(uuid "a4970690-3d1e-495c-ae3c-fe43e085f11a")
	)
	(segment
		(start 47.650001 53.4)
		(end 47.7 53.350001)
		(width 0.3)
		(layer "B.Cu")
		(net 55)
		(uuid "acc4fd88-4c17-4069-aed9-6d7021b658b4")
	)
	(segment
		(start 45.6 52)
		(end 44.8 51.2)
		(width 0.3)
		(layer "B.Cu")
		(net 55)
		(uuid "d1a1dd3f-d165-4eed-a79e-9efd17ff26b5")
	)
	(segment
		(start 45.6 53.3875)
		(end 45.6 52)
		(width 0.3)
		(layer "B.Cu")
		(net 55)
		(uuid "db34b4b8-3242-42d2-927b-2d6a5bab9909")
	)
	(segment
		(start 94.175 46.825)
		(end 94.5 46.5)
		(width 0.3)
		(layer "F.Cu")
		(net 56)
		(uuid "9ed69c82-0da8-420a-a9c2-e5bf6bacc47e")
	)
	(segment
		(start 93.449999 46.825)
		(end 94.175 46.825)
		(width 0.3)
		(layer "F.Cu")
		(net 56)
		(uuid "e9ef0556-e74d-401c-9cb6-2187e1254cd1")
	)
	(segment
		(start 121.4375 37.4375)
		(end 121.4375 39.9)
		(width 0.3)
		(layer "F.Cu")
		(net 59)
		(uuid "310343ee-56d6-424f-b86f-215d188f365e")
	)
	(segment
		(start 120.9 36.9)
		(end 121.4375 37.4375)
		(width 0.3)
		(layer "F.Cu")
		(net 59)
		(uuid "56722cec-c45d-4082-8b70-b5892c21e772")
	)
	(segment
		(start 96.25312 52.25)
		(end 96.8 51.70312)
		(width 0.3)
		(layer "F.Cu")
		(net 59)
		(uuid "6f32d628-1d6f-4197-bff3-04f33c7abf7e")
	)
	(segment
		(start 96.8 39)
		(end 98.9 36.9)
		(width 0.3)
		(layer "F.Cu")
		(net 59)
		(uuid "99c4ada2-ac22-400c-b010-929912e0392a")
	)
	(segment
		(start 96.8 51.70312)
		(end 96.8 39)
		(width 0.3)
		(layer "F.Cu")
		(net 59)
		(uuid "d5627a67-ee20-414f-a08a-a8c514404644")
	)
	(segment
		(start 98.9 36.9)
		(end 120.9 36.9)
		(width 0.3)
		(layer "F.Cu")
		(net 59)
		(uuid "d5f3f8e4-86ad-4e5d-8bbe-da883a1caedc")
	)
	(segment
		(start 95.375 52.25)
		(end 96.25312 52.25)
		(width 0.3)
		(layer "F.Cu")
		(net 59)
		(uuid "ed786865-930a-4220-8e75-eb1b79116775")
	)
	(segment
		(start 84.025 50.25)
		(end 82.05 50.25)
		(width 0.3)
		(layer "F.Cu")
		(net 60)
		(uuid "b65b65b5-d24d-4810-8dc0-b03d1f81ef4a")
	)
	(segment
		(start 82.05 50.25)
		(end 82 50.2)
		(width 0.3)
		(layer "F.Cu")
		(net 60)
		(uuid "f4ac56cf-8963-427c-b296-176614fa183a")
	)
	(segment
		(start 95.375 48.750001)
		(end 95.375 47.925)
		(width 0.3)
		(layer "F.Cu")
		(net 62)
		(uuid "067d2e12-daf3-4417-992c-f0fb25f27b47")
	)
	(segment
		(start 95.375 47.925)
		(end 95.7 47.6)
		(width 0.3)
		(layer "F.Cu")
		(net 62)
		(uuid "9eaf6a23-60fd-4027-8627-f2e195ec9d46")
	)
	(segment
		(start 83.05 49.25)
		(end 82.75 48.95)
		(width 0.3)
		(layer "F.Cu")
		(net 63)
		(uuid "0ceafc3a-5b18-4e41-8b9e-2ea7442b78de")
	)
	(segment
		(start 84.025 49.25)
		(end 83.05 49.25)
		(width 0.3)
		(layer "F.Cu")
		(net 63)
		(uuid "259f6990-240c-41f0-b557-8d54858a7d37")
	)
	(segment
		(start 82.75 48.55)
		(end 82 47.8)
		(width 0.3)
		(layer "F.Cu")
		(net 63)
		(uuid "2dc27525-7565-4ca9-a016-563a8fd80e69")
	)
	(segment
		(start 82.75 48.95)
		(end 82.75 48.55)
		(width 0.3)
		(layer "F.Cu")
		(net 63)
		(uuid "2dc63a7e-132a-43fb-bae2-6e00868b571e")
	)
	(segment
		(start 37.1 54.2)
		(end 37.265 54.365)
		(width 0.3)
		(layer "F.Cu")
		(net 65)
		(uuid "182e5de7-5c5c-464d-bb11-b55630da45ab")
	)
	(segment
		(start 38.325 53.095)
		(end 37.305 53.095)
		(width 0.3)
		(layer "F.Cu")
		(net 65)
		(uuid "49895a5d-88d2-43a9-a61a-90d733908089")
	)
	(segment
		(start 37.0875 54.0125)
		(end 37.1 54)
		(width 0.3)
		(layer "F.Cu")
		(net 65)
		(uuid "6b3d2ee7-6757-463d-b93e-72bfd63abf35")
	)
	(segment
		(start 37.265 54.365)
		(end 38.325 54.365)
		(width 0.3)
		(layer "F.Cu")
		(net 65)
		(uuid "703db16b-ce71-4d85-87be-0c4cb7c309c5")
	)
	(segment
		(start 37.1 54)
		(end 37.1 54.2)
		(width 0.3)
		(layer "F.Cu")
		(net 65)
		(uuid "afa29639-d3c6-45fd-a9a9-fe73fce81b8c")
	)
	(segment
		(start 37.1 53.3)
		(end 37.1 54)
		(width 0.3)
		(layer "F.Cu")
		(net 65)
		(uuid "b4b925ae-6199-4d37-9560-2a72f55204e6")
	)
	(segment
		(start 37.305 53.095)
		(end 37.1 53.3)
		(width 0.3)
		(layer "F.Cu")
		(net 65)
		(uuid "df5becce-5be1-4d6a-9f44-4a45265cea68")
	)
	(segment
		(start 36 54.0125)
		(end 37.0875 54.0125)
		(width 0.3)
		(layer "F.Cu")
		(net 65)
		(uuid "e94306d5-4db7-4d66-89e4-d2aa7325790a")
	)
	(segment
		(start 44.5 55.5)
		(end 44.365 55.635)
		(width 0.3)
		(layer "F.Cu")
		(net 66)
		(uuid "1b20b4ad-3404-40da-9855-9ae9abbfb931")
	)
	(segment
		(start 43.275 54.365)
		(end 44.265 54.365)
		(width 0.3)
		(layer "F.Cu")
		(net 66)
		(uuid "2a333e57-3bc9-43d3-b40e-cb1fd94713db")
	)
	(segment
		(start 44.5 54.6)
		(end 44.5 55.1)
		(width 0.3)
		(layer "F.Cu")
		(net 66)
		(uuid "3570a141-6505-44e8-9263-5a5dae0d2153")
	)
	(segment
		(start 44.365 55.635)
		(end 43.275 55.635)
		(width 0.3)
		(layer "F.Cu")
		(net 66)
		(uuid "5eb2d766-9724-488b-8784-0af198e9d21c")
	)
	(segment
		(start 44.265 54.365)
		(end 44.5 54.6)
		(width 0.3)
		(layer "F.Cu")
		(net 66)
		(uuid "7d38469a-cc5b-48f7-8f35-eed944f994be")
	)
	(segment
		(start 44.5 55.1)
		(end 44.6125 55.2125)
		(width 0.3)
		(layer "F.Cu")
		(net 66)
		(uuid "99731415-948a-4107-85df-f56b36ca3f0d")
	)
	(segment
		(start 44.6125 55.2125)
		(end 45.6 55.2125)
		(width 0.3)
		(layer "F.Cu")
		(net 66)
		(uuid "ef4db8fe-b503-4e1c-991b-36c30e9e5ca7")
	)
	(segment
		(start 44.5 55.1)
		(end 44.5 55.5)
		(width 0.3)
		(layer "F.Cu")
		(net 66)
		(uuid "fca403bc-0503-443c-8024-7cbb41e7107a")
	)
	(segment
		(start 39.325 42.765)
		(end 37.265 42.765)
		(width 0.3)
		(layer "F.Cu")
		(net 67)
		(uuid "9108ab64-543a-4356-8264-3ca629abf335")
	)
	(segment
		(start 37.265 42.765)
		(end 37 42.5)
		(width 0.3)
		(layer "F.Cu")
		(net 67)
		(uuid "d6bf65e1-3aa1-4d44-8243-358bbe861fe1")
	)
	(via
		(at 37 42.5)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 67)
		(uuid "69e0236c-2bc3-4190-8bb0-8b8372600c1e")
	)
	(segment
		(start 44.275 44.035)
		(end 44.41 43.9)
		(width 0.3)
		(layer "F.Cu")
		(net 68)
		(uuid "94fe0871-e4b5-41bf-80f6-30f50b0f16fc")
	)
	(segment
		(start 46.2875 43.9)
		(end 46.6 43.5875)
		(width 0.3)
		(layer "F.Cu")
		(net 68)
		(uuid "b2e1dd29-54d7-4428-8f90-34d28bff599e")
	)
	(segment
		(start 44.41 43.9)
		(end 46.2875 43.9)
		(width 0.3)
		(layer "F.Cu")
		(net 68)
		(uuid "ecad1fff-a2e7-4b35-9dfc-35281d2fbd38")
	)
	(via
		(at 46.6 43.5875)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 68)
		(uuid "c040b8c3-0c9c-4a39-8c17-df1087f6a3a2")
	)
	(segment
		(start 56.649999 51.799999)
		(end 56.649999 56.360001)
		(width 0.3)
		(layer "B.Cu")
		(net 70)
		(uuid "db841991-e729-4f44-a344-48bd90d1e690")
	)
	(segment
		(start 56.649999 56.360001)
		(end 56.635 56.375)
		(width 0.3)
		(layer "B.Cu")
		(net 70)
		(uuid "fdf9611c-87a7-4569-8c02-f65385a6a675")
	)
	(segment
		(start 127.98 46.92)
		(end 129.4 45.5)
		(width 1.2)
		(layer "B.Cu")
		(net 71)
		(uuid "2ee3c6fd-02b9-483e-823d-f118d85e993c")
	)
	(segment
		(start 131.774999 45.5)
		(end 131.8 45.525001)
		(width 1.2)
		(layer "B.Cu")
		(net 71)
		(uuid "5b66b518-ba3c-4573-a8a3-afbdb6a569ce")
	)
	(segment
		(start 129.4 45.5)
		(end 131.774999 45.5)
		(width 1.2)
		(layer "B.Cu")
		(net 71)
		(uuid "72ead983-ee58-49f1-8811-d99ba649128e")
	)
	(segment
		(start 126.3 46.92)
		(end 127.98 46.92)
		(width 1.2)
		(layer "B.Cu")
		(net 71)
		(uuid "eeee1dd5-bbb9-4ebc-9ada-028d4a334e8c")
	)
	(via
		(at 119.6 44.9)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 72)
		(uuid "76ff11e6-afff-4585-8fd3-19e52ff3a942")
	)
	(via
		(at 75 55.2)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 73)
		(uuid "0c36a9d3-b8d5-42f3-ad85-f93856423ee7")
	)
	(segment
		(start 73.075 56.375)
		(end 73.737501 57.037501)
		(width 0.3)
		(layer "F.Cu")
		(net 74)
		(uuid "5fbbf83e-0106-44f4-b408-9e5fd0024f54")
	)
	(segment
		(start 73.737501 57.037501)
		(end 75 57.037501)
		(width 0.3)
		(layer "F.Cu")
		(net 74)
		(uuid "7f518149-9fb2-4231-9f74-17dcd8333a21")
	)
	(segment
		(start 71.875 56.375)
		(end 73.075 56.375)
		(width 0.3)
		(layer "F.Cu")
		(net 74)
		(uuid "a76fb5de-fef4-4906-962c-80dbffe44d51")
	)
	(via
		(at 119.6 39.9)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 75)
		(uuid "34e5d202-578a-4c98-b5ba-44ffaf437207")
	)
	(via
		(at 75 50.8)
		(size 0.8)
		(drill 0.4)
		(layers "F.Cu" "B.Cu")
		(net 76)
		(uuid "1a061100-f07c-4b81-8c6b-7540d99636a4")
	)
	(segment
		(start 70.6 57.64)
		(end 71.875 58.915)
		(width 0.3)
		(layer "F.Cu")
		(net 77)
		(uuid "02d8a800-d660-4ff7-86a5-887c47917509")
	)
	(segment
		(start 70.6 54.5)
		(end 70.6 57.64)
		(width 0.3)
		(layer "F.Cu")
		(net 77)
		(uuid "106ee0a1-a4c0-4819-9b65-339549c07861")
	)
	(segment
		(start 71.9 53.2)
		(end 70.6 54.5)
		(width 0.3)
		(layer "F.Cu")
		(net 77)
		(uuid "9676e2e8-f967-4f3a-9391-d686a01911f2")
	)
	(segment
		(start 71.9 51.774999)
		(end 71.9 53.2)
		(width 0.3)
		(layer "F.Cu")
		(net 77)
		(uuid "a4362865-b2b9-438e-91c2-3b452bb9f59f")
	)
	(segment
		(start 67.9 51.774999)
		(end 67.9 52.7)
		(width 0.3)
		(layer "F.Cu")
		(net 78)
		(uuid "2dc70188-dba9-4147-a79e-8672ba366626")
	)
	(segment
		(start 67.9 52.7)
		(end 65.518022 55.081978)
		(width 0.3)
		(layer "F.Cu")
		(net 78)
		(uuid "87bbd6d2-72ac-4fa4-8f43-81e95a578f93")
	)
	(segment
		(start 65.518022 57.651978)
		(end 64.255 58.915)
		(width 0.3)
		(layer "F.Cu")
		(net 78)
		(uuid "883381da-933c-4581-98a0-52e0c5d4a86f")
	)
	(segment
		(start 65.518022 55.081978)
		(end 65.518022 57.651978)
		(width 0.3)
		(layer "F.Cu")
		(net 78)
		(uuid "bfb39fbb-a189-4df5-906e-810ffc84c424")
	)
	(segment
		(start 57.9 57.65)
		(end 56.635 58.915)
		(width 0.3)
		(layer "F.Cu")
		(net 79)
		(uuid "256c6533-da21-4318-8384-7bac4c994e99")
	)
	(segment
		(start 62.8 54.4)
		(end 58.5 54.4)
		(width 0.3)
		(layer "F.Cu")
		(net 79)
		(uuid "34eba394-18b9-49fe-96e1-6cd26dc8b720")
	)
	(segment
		(start 63.9 53.3)
		(end 62.8 54.4)
		(width 0.3)
		(layer "F.Cu")
		(net 79)
		(uuid "433b757d-ab3b-4df1-9261-d05f417dffcf")
	)
	(segment
		(start 57.9 55)
		(end 57.9 57.65)
		(width 0.3)
		(layer "F.Cu")
		(net 79)
		(uuid "62c4cd5d-e25e-4af8-9d11-2f418b8490e0")
	)
	(segment
		(start 63.9 51.774999)
		(end 63.9 53.3)
		(width 0.3)
		(layer "F.Cu")
		(net 79)
		(uuid "b128b007-8ffc-45c1-be14-a1f28218e270")
	)
	(segment
		(start 58.5 54.4)
		(end 57.9 55)
		(width 0.3)
		(layer "F.Cu")
		(net 79)
		(uuid "d306bf66-b7e1-4492-aefd-dbad579be90f")
	)
	(segment
		(start 52.715 58.915)
		(end 54.095 58.915)
		(width 0.3)
		(layer "F.Cu")
		(net 80)
		(uuid "321bf3f9-9ef3-47b0-9bc9-a36ae700cba3")
	)
	(segment
		(start 51.9 54.1)
		(end 51.9 58.1)
		(width 0.3)
		(layer "F.Cu")
		(net 80)
		(uuid "412e1934-4c5a-4c75-88d9-8dca7de639f4")
	)
	(segment
		(start 55.9 52.6)
		(end 55.2 53.3)
		(width 0.3)
		(layer "F.Cu")
		(net 80)
		(uuid "550807e2-cf8b-4e13-9018-16c043c5e3b8")
	)
	(segment
		(start 52.7 53.3)
		(end 51.9 54.1)
		(width 0.3)
		(layer "F.Cu")
		(net 80)
		(uuid "84102fcb-f7cd-405e-b376-53e65b8cc051")
	)
	(segment
		(start 51.9 58.1)
		(end 52.715 58.915)
		(width 0.3)
		(layer "F.Cu")
		(net 80)
		(uuid "88fdf51c-85d0-4cba-9874-c41b53d91316")
	)
	(segment
		(start 55.2 53.3)
		(end 52.7 53.3)
		(width 0.3)
		(layer "F.Cu")
		(net 80)
		(uuid "f752e2fb-b170-4c2a-8563-157bcfed6a64")
	)
	(segment
		(start 55.9 51.774999)
		(end 55.9 52.6)
		(width 0.3)
		(layer "F.Cu")
		(net 80)
		(uuid "fa492656-2ee1-4e95-ae2a-29efc36e9d8e")
	)
	(segment
		(start 59.9 51.774999)
		(end 59.9 53.2)
		(width 0.3)
		(layer "F.Cu")
		(net 81)
		(uuid "1a6e4ece-a06b-49ec-8981-d249c4e43c1c")
	)
	(segment
		(start 59.3 53.8)
		(end 54.7 53.8)
		(width 0.3)
		(layer "F.Cu")
		(net 81)
		(uuid "234a4f09-de82-4cea-ac8c-5a51254da489")
	)
	(segment
		(start 54.7 53.8)
		(end 54.094999 54.405001)
		(width 0.3)
		(layer "F.Cu")
		(net 81)
		(uuid "3c9b059d-f6cc-4144-8d65-78aabd8d5309")
	)
	(segment
		(start 59.9 53.2)
		(end 59.3 53.8)
		(width 0.3)
		(layer "F.Cu")
		(net 81)
		(uuid "9bf1b616-d4d2-436f-b978-111278438ab1")
	)
	(segment
		(start 54.094999 54.405001)
		(end 54.094999 56.375)
		(width 0.3)
		(layer "F.Cu")
		(net 81)
		(uuid "eba59855-b3b8-41fb-b900-2472e1b4b18b")
	)
	(segment
		(start 36 57.5125)
		(end 36 59.8)
		(width 0.3)
		(layer "F.Cu")
		(net 82)
		(uuid "1eee4377-ab24-4885-a378-bf8e3087fcb0")
	)
	(segment
		(start 36 59.8)
		(end 36.8 60.6)
		(width 0.3)
		(layer "F.Cu")
		(net 82)
		(uuid "f5d12419-2918-4e33-bc5a-879dee87af36")
	)
	(segment
		(start 36.8 60.6)
		(end 38.3 60.6)
		(width 0.3)
		(layer "F.Cu")
		(net 82)
		(uuid "fa3a854c-baa0-48c7-99aa-47522fa9cf3c")
	)
	(segment
		(start 45.6 58.7125)
		(end 45.6 59.8)
		(width 0.3)
		(layer "F.Cu")
		(net 83)
		(uuid "490d4fc6-202b-4afc-805b-0b2dd82a0f8f")
	)
	(segment
		(start 44.8 60.6)
		(end 43.3 60.6)
		(width 0.3)
		(layer "F.Cu")
		(net 83)
		(uuid "4f67b53a-75c8-4ddc-9974-1c42dfc0c59c")
	)
	(segment
		(start 45.6 59.8)
		(end 44.8 60.6)
		(width 0.3)
		(layer "F.Cu")
		(net 83)
		(uuid "6e62adb2-0bba-4bc2-a8ca-a9d5ee9a3c5d")
	)
	(segment
		(start 35.000001 42.4875)
		(end 33.037501 42.4875)
		(width 0.3)
		(layer "F.Cu")
		(net 84)
		(uuid "038ea77a-3374-4390-9757-343d8bfdac64")
	)
	(segment
		(start 33.037501 42.4875)
		(end 33 42.449999)
		(width 0.3)
		(layer "F.Cu")
		(net 84)
		(uuid "48d1fa47-49d1-4cd4-94ec-ef9f122e2805")
	)
	(segment
		(start 48.599999 43.5875)
		(end 50.537501 43.5875)
		(width 0.3)
		(layer "F.Cu")
		(net 85)
		(uuid "aab8ab9e-a48c-4fab-a570-67d204ad815e")
	)
	(segment
		(start 50.537501 43.5875)
		(end 50.6 43.649999)
		(width 0.3)
		(layer "F.Cu")
		(net 85)
		(uuid "c3e2c47e-84dc-4ce1-add6-d4b2c9260e94")
	)
	(segment
		(start 37 47.000001)
		(end 37.55 47.550001)
		(width 0.3)
		(layer "F.Cu")
		(net 87)
		(uuid "45aea153-7810-455c-99a2-2478c7030004")
	)
	(segment
		(start 37.2775 44.035)
		(end 37 44.3125)
		(width 0.3)
		(layer "F.Cu")
		(net 87)
		(uuid "78dc521f-a5ad-40e0-8714-f340e22f088b")
	)
	(segment
		(start 39.325 44.035)
		(end 37.2775 44.035)
		(width 0.3)
		(layer "F.Cu")
		(net 87)
		(uuid "a7f70850-bfe5-4bad-9d1b-8e661a2ba190")
	)
	(segment
		(start 37 44.3125)
		(end 37 47.000001)
		(width 0.3)
		(layer "F.Cu")
		(net 87)
		(uuid "c2793a56-0b44-4154-b1fe-9c0b17df9e88")
	)
	(segment
		(start 35.000001 44.3125)
		(end 37 44.3125)
		(width 0.3)
		(layer "F.Cu")
		(net 87)
		(uuid "d2fdd60d-3d70-4a3f-bdc0-edb29d175257")
	)
	(segment
		(start 46.4925 45.305)
		(end 46.6 45.4125)
		(width 0.3)
		(layer "F.Cu")
		(net 88)
		(uuid "1bc624c0-79a8-49bd-9a17-c3bda8fb567b")
	)
	(segment
		(start 44.275 45.305)
		(end 46.4925 45.305)
		(width 0.3)
		(layer "F.Cu")
		(net 88)
		(uuid "1c1f7610-7027-474c-aedd-c0a87da61d39")
	)
	(segment
		(start 46.6 45.4125)
		(end 46.6 47.050002)
		(width 0.3)
		(layer "F.Cu")
		(net 88)
		(uuid "25c59e84-7fe9-4934-addb-202868ad2828")
	)
	(segment
		(start 46.6 47.050002)
		(end 46.1 47.550002)
		(width 0.3)
		(layer "F.Cu")
		(net 88)
		(uuid "92633b74-be8d-4429-8f79-32b4229923a0")
	)
	(segment
		(start 46.6 45.4125)
		(end 48.599999 45.4125)
		(width 0.3)
		(layer "F.Cu")
		(net 88)
		(uuid "93513e56-ce26-4b2f-9cbf-300ef0d50017")
	)
	(zone
		(net 6)
		(net_name "+5V")
		(layer "F.Cu")
		(uuid "9a291b1d-fcfb-412f-b613-387c1fdac7ee")
		(name "5V")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads
			(clearance 0.3)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.4)
			(thermal_bridge_width 0.4)
		)
		(polygon
			(pts
				(xy 140.1 63.1) (xy 140.1 34.6) (xy 134.1 34.6) (xy 134.1 49.9) (xy 131 49.9) (xy 131 63.1)
			)
		)
		(filled_polygon
			(layer "F.Cu")
			(pts
				(xy 139.642539 35.320185) (xy 139.688294 35.372989) (xy 139.6995 35.4245) (xy 139.6995 62.5755)
				(xy 139.679815 62.642539) (xy 139.627011 62.688294) (xy 139.5755 62.6995) (xy 131.124 62.6995) (xy 131.056961 62.679815)
				(xy 131.011206 62.627011) (xy 131 62.5755) (xy 131 50.024) (xy 131.019685 49.956961) (xy 131.072489 49.911206)
				(xy 131.124 49.9) (xy 134.1 49.9) (xy 134.1 35.4245) (xy 134.119685 35.357461) (xy 134.172489 35.311706)
				(xy 134.224 35.3005) (xy 139.5755 35.3005)
			)
		)
	)
	(zone
		(net 6)
		(net_name "+5V")
		(layer "B.Cu")
		(uuid "7f21741f-b77b-4d2c-9be2-09066a22c985")
		(name "5V_f")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.3)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.3)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 140.2 63.2) (xy 140.2 52.4) (xy 136.5 52.4) (xy 136 51.9) (xy 136 49.9) (xy 134.4 49.9) (xy 134.4 51.9)
				(xy 133.9 52.4) (xy 131.8 52.4) (xy 131.3 51.9) (xy 131.3 49.9) (xy 124.6 49.9) (xy 124.6 53.4)
				(xy 130.1 53.4) (xy 131 54.3) (xy 131 63.2)
			)
		)
		(filled_polygon
			(layer "B.Cu")
			(pts
				(xy 131.243039 49.919685) (xy 131.288794 49.972489) (xy 131.3 50.024) (xy 131.3 51.9) (xy 131.8 52.4)
				(xy 133.9 52.4) (xy 134.4 51.9) (xy 134.4 50.024) (xy 134.419685 49.956961) (xy 134.472489 49.911206)
				(xy 134.524 49.9) (xy 135.876 49.9) (xy 135.943039 49.919685) (xy 135.988794 49.972489) (xy 136 50.024)
				(xy 136 51.9) (xy 136.5 52.4) (xy 139.5755 52.4) (xy 139.642539 52.419685) (xy 139.688294 52.472489)
				(xy 139.6995 52.524) (xy 139.6995 62.5755) (xy 139.679815 62.642539) (xy 139.627011 62.688294) (xy 139.5755 62.6995)
				(xy 131.124 62.6995) (xy 131.056961 62.679815) (xy 131.011206 62.627011) (xy 131 62.5755) (xy 131 54.3)
				(xy 130.1 53.4) (xy 124.724 53.4) (xy 124.656961 53.380315) (xy 124.611206 53.327511) (xy 124.6 53.276)
				(xy 124.6 50.024) (xy 124.619685 49.956961) (xy 124.672489 49.911206) (xy 124.724 49.9) (xy 131.176 49.9)
			)
		)
	)
	(group ""
		(uuid "2c4e65f1-793b-459f-b9e7-85773e1c5c71")
		(members "6e91051b-cd5b-47c6-ad77-e05b86662b30" "c8c52e06-0b84-4057-9c4f-81366b21b198")
	)
	(group ""
		(uuid "2fc43e0f-ed96-4800-842a-9689e4f699ce")
		(members "0626d90f-0897-4266-adea-1cfba5f06f11" "179a26e7-98ad-4760-8457-85c3f68fb377")
	)
	(group ""
		(uuid "38425e5e-5020-4b97-9c1a-91392efd29ba")
		(members "13a9bb46-a18c-4429-a009-06d7448b6bdb" "a1609a9c-7a58-44a8-9d03-4553fdd0b3e6")
	)
	(group ""
		(uuid "4fd1e9ac-cdee-4814-8da5-f69414f77d98")
		(members "0bec2b22-7de5-49b1-b2f5-7404702075ce" "58c94c04-caf7-4205-bb44-dc2b30036aef"
			"8f1c0595-786d-4641-a860-068ece0c9001" "e6047146-209f-408d-91ee-91c6549f58cd"
			"fa4c54d9-3fb1-4677-94f7-46a4bc6c8346"
		)
	)
	(group ""
		(uuid "9b11f2de-274a-41f1-b025-15ee80b6d2ff")
		(members "27eb1186-ee6e-4a84-8cc0-e7a88a4a009b" "848a0f0c-a0ea-4358-a5e1-8d2ba9cc6b5e")
	)
	(group ""
		(uuid "9cbc81b0-aec9-49c5-b763-6339a76c093e")
		(members "05eab0f9-caa6-4749-8e1f-80fb2b9524e4" "3901eb0a-945a-408e-b61e-86f3dfedd189"
			"5d806f2e-ea67-4dfc-a9e4-c25773a05cd7" "a5902430-d1bb-4453-b318-85d1c672f4d1"
			"f65e3860-3ac0-49cb-bdc7-4aab5a24b8c9"
		)
	)
	(group ""
		(uuid "aebcb72d-c168-41b2-8ca1-60ed7ef8468c")
		(members "2fea9d61-df99-4862-a82e-5069698adf9a" "f07619bd-a84b-41cc-a69d-8be87c48e561")
	)
	(group ""
		(uuid "3e7cd97b-0a32-41a2-8f48-b093e0383d8f")
		(members "0fb65ea6-819b-4930-a05b-84d5c95609f0" "339d0578-8883-4d3e-b9c5-a4a0f6861326")
	)
)
