(module EN11_Encoder (layer F.Cu) (tedit 5EF941E5)
  (fp_text reference SW1 (at 0 5.08) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Rotary_Encoder_Switch (at 0 -5.08) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 0 0) (end 3.75 0) (layer F.SilkS) (width 0.15))
  (pad A thru_hole circle (at -2.5 7.5) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
  (pad C thru_hole circle (at 0 7.5) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
  (pad B thru_hole circle (at 2.5 7.5) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
  (pad S1 thru_hole circle (at -2.5 -7) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
  (pad S2 thru_hole circle (at 2.5 -7) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
  (pad MP thru_hole oval (at -5.08 0) (size 2.5 4) (drill oval 2 3) (layers *.Cu *.Mask))
  (pad MP thru_hole oval (at 5.08 0 180) (size 2.5 4) (drill oval 2 3) (layers *.Cu *.Mask))
  (model ${KIPRJMOD}/Library/3D_Packages/en11-hsm1af15.STEP
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
