(footprint "SolderJumper-3_P1.3mm_Pad1.0x1.5mm" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5C756B4C)
  (descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
  (tags "solder jumper open")
  (attr exclude_from_pos_files exclude_from_bom)
  (fp_text reference "REF**" (at 0 -1.8) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c176c452-5030-47f2-9bd4-1a8ca85adbe0)
  )
  (fp_text value "SolderJumper-3_P1.3mm_Pad1.0x1.5mm" (at 0 2) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 25302f5a-cd4a-4236-b306-b0dd0c00a5e2)
  )
  (fp_line (start -1.6 1.5) (end -1 1.5) (layer "F.SilkS") (width 0.12) (tstamp 080a932c-c8e2-4559-876b-837f1841896a))
  (fp_line (start -1.3 1.2) (end -1.6 1.5) (layer "F.SilkS") (width 0.12) (tstamp 092ce409-030e-45a9-aaad-826bad9fe14d))
  (fp_line (start 2.05 -1) (end 2.05 1) (layer "F.SilkS") (width 0.12) (tstamp 14f87ee4-9f41-4f42-bdb0-583a76ef4873))
  (fp_line (start 2.05 1) (end -2.05 1) (layer "F.SilkS") (width 0.12) (tstamp 238470e8-8d31-474b-8e20-6cb943cda51d))
  (fp_line (start -2.05 -1) (end 2.05 -1) (layer "F.SilkS") (width 0.12) (tstamp 5ff0dd05-b6f9-4f9d-a3fa-342438c2b71c))
  (fp_line (start -1.3 1.2) (end -1 1.5) (layer "F.SilkS") (width 0.12) (tstamp 96b8cc3d-e7ec-40fa-b885-c43e4edf4e73))
  (fp_line (start -2.05 1) (end -2.05 -1) (layer "F.SilkS") (width 0.12) (tstamp e6c26cbf-86f4-4f68-b8ea-898609d5a5ea))
  (fp_line (start 2.3 1.25) (end -2.3 1.25) (layer "F.CrtYd") (width 0.05) (tstamp 6412f482-67b4-4b81-bf00-7eba1317cc9c))
  (fp_line (start -2.3 -1.25) (end 2.3 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp 94986137-ee8b-4f02-b061-1297ee9b6de4))
  (fp_line (start -2.3 -1.25) (end -2.3 1.25) (layer "F.CrtYd") (width 0.05) (tstamp c857e66e-819b-4837-9531-c8b02dd50299))
  (fp_line (start 2.3 1.25) (end 2.3 -1.25) (layer "F.CrtYd") (width 0.05) (tstamp fc87b1db-8b6e-449e-9787-b5e7ad4b6b71))
  (pad "1" smd rect (at -1.3 0) (size 1 1.5) (layers "F.Cu" "F.Mask") (tstamp f802df87-c293-4fc4-977c-48a123fd9bb9))
  (pad "2" smd rect (at 0 0) (size 1 1.5) (layers "F.Cu" "F.Mask") (tstamp c2dba507-2301-441e-8d42-1a95881ae48a))
  (pad "3" smd rect (at 1.3 0) (size 1 1.5) (layers "F.Cu" "F.Mask") (tstamp 5b08ad10-029b-45aa-b9a0-ab02f2dce368))
)
