EESchema-DOCLIB  Version 2.0
#
$CMP +3V3
D Power symbol creates a global label with name "+3V3"
K power-flag
$ENDCMP
#
$CMP 74LVC1G17
D Single Schmitt Buffer Gate, Low-Voltage CMOS
K Single Gate Buff Schmitt LVC CMOS
F http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf
$ENDCMP
#
$CMP AP2127K-3.3
D 300mA low dropout linear regulator, shutdown pin, 2.5V-6V input voltage, 3.3V fixed positive output, SOT-23-5 package
K linear regulator ldo fixed positive
F https://www.diodes.com/assets/Datasheets/AP2127.pdf
$ENDCMP
#
$CMP C
D Unpolarized capacitor
K cap capacitor
F ~
$ENDCMP
#
$CMP Conn_01x01
D Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x02
D Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x03
D Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_01x04
D Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Conn_02x05_Odd_Even
D Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)
K connector
F ~
$ENDCMP
#
$CMP Fuse
D Fuse
K fuse
F ~
$ENDCMP
#
$CMP GND
D Power symbol creates a global label with name "GND" , ground
K power-flag
$ENDCMP
#
$CMP IRLML6344TRPBF
D MOSFET N-CH 30V 5A SOT23
K IRLML6344TRPBFCT-ND HEXFET®
F https://www.infineon.com/dgdl/irlml6344pbf.pdf?fileId=5546d462533600a4015356689c44262c
$ENDCMP
#
$CMP LED
D Light emitting diode
K LED diode
F ~
$ENDCMP
#
$CMP MountingHole
D Mounting Hole without connection
K mounting hole
F ~
$ENDCMP
#
$CMP R
D Resistor
K R res resistor
F ~
$ENDCMP
#
$CMP Rotary_Encoder_Switch
D Rotary encoder, dual channel, incremental quadrate outputs, with switch
K rotary switch encoder switch push button
F ~
$ENDCMP
#
$CMP STM32F042F6Px
D ARM Cortex-M0 MCU, 32KB flash, 6KB RAM, 48MHz, 2-3.6V, 16 GPIO, TSSOP-20
K ARM Cortex-M0 STM32F0 STM32F0x2
F http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00105814.pdf
$ENDCMP
#
$CMP SW_SPST
D Single Pole Single Throw (SPST) switch
K switch lever
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x02
D Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP Screw_Terminal_01x08
D Generic screw terminal, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)
K screw terminal
F ~
$ENDCMP
#
$CMP SolderJumper_3_Bridged12
D 3-pole Solder Jumper, pins 1+2 closed/bridged
K Solder Jumper SPDT
F ~
$ENDCMP
#
$CMP USB_B_Micro
D USB Micro Type B connector
K connector USB micro
F ~
$ENDCMP
#
$CMP WS2812B
D RGB LED with integrated controller
K RGB LED NeoPixel addressable
F https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf
$ENDCMP
#
#End Doc Library
