(module SolderJumper-3_P1.3mm_Bridged12_Pad1.0x1.5mm (layer F.Cu) (tedit 5C756B4C)
  (descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
  (tags "solder jumper open")
  (attr virtual)
  (fp_text reference REF** (at 0 -1.8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SolderJumper-3_P1.3mm_Bridged12_Pad1.0x1.5mm (at 0 2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.3 1.2) (end -1 1.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.6 1.5) (end -1 1.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.3 1.2) (end -1.6 1.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.05 1) (end -2.05 -1) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.05 1) (end -2.05 1) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.05 -1) (end 2.05 1) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.05 -1) (end 2.05 -1) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.3 -1.25) (end 2.3 -1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.3 -1.25) (end -2.3 1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.3 1.25) (end 2.3 -1.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.3 1.25) (end -2.3 1.25) (layer F.CrtYd) (width 0.05))
  (fp_poly (pts (xy -0.9 -0.3) (xy -0.4 -0.3) (xy -0.4 0.3) (xy -0.9 0.3)) (layer F.Cu) (width 0))
  (pad 1 smd rect (at -1.3 0) (size 1 1.5) (layers F.Cu F.Mask))
  (pad 3 smd rect (at 1.3 0) (size 1 1.5) (layers F.Cu F.Mask))
  (pad 2 smd rect (at 0 0) (size 1 1.5) (layers F.Cu F.Mask))
)
