(footprint "USB-C_Female_6pin"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "USB type C Female 6pin connector")
	(property "Reference" "REF**"
		(at -5.1 -1.7 0)
		(layer "F.SilkS")
		(uuid "f65ce064-1632-4ff5-b110-958892142350")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify left)
		)
	)
	(property "Value" "USB-C_Female_6pin"
		(at 0 7.3 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "64f77c7c-84b8-471a-80b4-09ba8960b8cc")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 6.3 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6e5daad6-e254-40bc-9a66-fe021f9bd616")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 6.3 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7839dc84-1d9b-4a8c-9c76-9a68c3a68510")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "USB type C Female 6pin connector"
		(at 0 9 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "02f6b595-c7a8-47f9-8f67-c26b042e5dbc")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -5 -1)
		(end 5 6.4)
		(stroke
			(width 0.12)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "574b252c-3cab-4874-859f-9b15d3d03ec5")
	)
	(fp_rect
		(start -4.8 -0.8)
		(end 4.8 6.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "e2ad0a4d-a791-4f66-92ce-56540c0e3bc8")
	)
	(fp_line
		(start -4.4 -0.5)
		(end -4.4 6.1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "01246204-aae4-444e-80fa-431010b54b57")
	)
	(fp_line
		(start -4.4 -0.5)
		(end -2.8 -0.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "05a32fda-d01b-47c6-a269-4aed56000b76")
	)
	(fp_line
		(start -4.4 6.3)
		(end 4.4 6.3)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "14a9e598-07df-485a-b867-cb48cc99fd9f")
	)
	(fp_line
		(start -2.8 -0.5)
		(end -2.7 -0.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "2792b1d4-88a3-49b5-8ad5-f4e721021975")
	)
	(fp_line
		(start -2.7 -0.2)
		(end 2.7 -0.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "afcc1e6a-4fcf-4013-8aa2-d481ce30ba92")
	)
	(fp_line
		(start 2.7 -0.2)
		(end 2.8 -0.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "4d98c68d-d718-4f0e-bd78-8b3addd6140d")
	)
	(fp_line
		(start 2.8 -0.5)
		(end 4.4 -0.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "dee83144-9104-4f57-b9e0-67ccfd4c30ac")
	)
	(fp_line
		(start 4.4 6.1)
		(end 4.4 -0.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "df6edae7-7fe8-44d0-8999-a4d405ec927b")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.9 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "431c3472-e16c-4690-8725-2e61cfa896a8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "A5" smd rect
		(at -0.5 0)
		(size 0.7 1.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "14814590-beed-4bb1-a6c7-8f58d9074c92")
	)
	(pad "A9" smd rect
		(at 1.52 0)
		(size 0.8 1.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "02d08600-c765-4630-bd20-fbb96677a3b0")
	)
	(pad "A12" smd rect
		(at 2.75 0)
		(size 0.9 1.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "69217cbc-b406-40dd-9bc1-ffffc56812b9")
	)
	(pad "B5" smd rect
		(at 0.5 0)
		(size 0.7 1.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "7c3b035b-f08c-4eff-b6a6-fe01376bff53")
	)
	(pad "B9" smd rect
		(at -1.52 0)
		(size 0.8 1.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "4587f90a-5bdd-41cc-b35d-1cc9a3e60e1b")
	)
	(pad "B12" smd rect
		(at -2.75 0)
		(size 0.9 1.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "3fcadb4d-04e0-40a1-97df-6460a0f58ac5")
	)
	(pad "S1" thru_hole oval
		(at -4.32 0.1)
		(size 1.1 2)
		(drill oval 0.5 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
		(uuid "8a24ed32-2374-4301-b37d-aa759dcfbd6f")
	)
	(pad "S1" thru_hole oval
		(at -4.32 3.8)
		(size 1.1 2)
		(drill oval 0.5 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
		(uuid "cb5e4cef-82ea-4378-8e7e-652d4e1fd3f2")
	)
	(pad "S1" thru_hole oval
		(at 4.32 0.1)
		(size 1.1 2)
		(drill oval 0.5 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
		(uuid "6a9d362c-856a-4d17-918e-2a05ba137cd2")
	)
	(pad "S1" thru_hole oval
		(at 4.32 3.8)
		(size 1.1 2)
		(drill oval 0.5 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
		(uuid "06044b33-8aa2-4ba2-94ff-21dd82fbd873")
	)
	(model "${my_additions}/USB_C_female_6pin.step"
		(offset
			(xyz 0 -6.5 1.7)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
