(footprint "LDR_5mm_photoresistor" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "photoresistor LDR 5")
  (tags "photo resistor photoresistor")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -2.8) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 163d29fc-2305-4ce4-b225-b930968260e7)
  )
  (fp_text value "LDR_5mm_photoresistor" (at 0 2.9) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ee72294f-60d9-4bd2-be51-775f9f7af7f8)
  )
  (fp_text user "${REFERENCE}" (at 0 4.4) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7fbaaca6-de0e-462c-b673-5b1f5cf239cf)
  )
  (fp_line (start -1.4 -2.099999) (end 1.4 -2.099999)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 77b8d9c2-5999-4eaf-b611-19c5b893cb51))
  (fp_line (start -1.4 2.099999) (end 1.4 2.099999)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 907de4a8-f13b-4d50-afdb-db9beb2a53ec))
  (fp_arc (start -1.4 2.099999) (mid -2.523885 0) (end -1.4 -2.099999)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp a747397c-1772-409c-abb2-308d9b758876))
  (fp_arc (start 1.4 -2.099999) (mid 2.523885 0) (end 1.4 2.099999)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp e5e9058c-b4ca-4677-a9b2-00a7a3d1537b))
  (fp_line (start -1.4 -2.099999) (end 1.4 -2.099999)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp e9855c1c-2aa1-4cec-8851-aaf8a2f460b9))
  (fp_line (start -1.4 2.099999) (end 1.4 2.099999)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 75ccd5cc-ab11-4eca-a36d-ae349bdde6c1))
  (fp_arc (start -1.4 2.099999) (mid -2.523886 0) (end -1.4 -2.099999)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 39ab9aea-df36-49f3-87e6-df239e28ff85))
  (fp_arc (start 1.4 -2.099999) (mid 2.523886 0) (end 1.4 2.099999)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2ed6c0c4-6ebd-494f-988e-e1126b8319d6))
  (fp_line (start -1.4 -2.1) (end 1.4 -2.1)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp cac4f06b-ea3b-405f-9310-cf970a25614a))
  (fp_line (start -1.4 2.099998) (end 1.4 2.099998)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp 08f5acc1-1cd4-4f86-9f25-281bc8ad1cde))
  (fp_line (start -0.8 -1.6) (end -0.8 -1.2)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp 87a57112-1554-4890-9c70-5c486dd59b09))
  (fp_line (start -0.8 -0.8) (end -0.8 -0.4)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp cfed7e06-5b0a-47c8-98a5-d46fa4b40103))
  (fp_line (start -0.8 -0.8) (end 0.8 -0.8)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp 0aaff2ce-e050-4106-a75b-67f94b64ac40))
  (fp_line (start -0.8 0) (end -0.8 0.4)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp 2c45af7a-2ad9-4945-8f38-67e277621e47))
  (fp_line (start -0.8 0) (end 0.8 0)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp d5852248-f3e3-41ae-863e-a0e477305c4c))
  (fp_line (start -0.8 0.8) (end -0.8 1.2)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp db5226a1-1ff6-4ea6-aec2-73de23546d87))
  (fp_line (start -0.8 0.8) (end 0.8 0.8)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp f4b586b8-72b3-45b0-81b1-2abe07db60bc))
  (fp_line (start -0.8 1.6) (end 0.8 1.6)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp 4e4cd977-c73b-4311-82f0-b4c64ea245a2))
  (fp_line (start -0.8 2.1) (end -0.8 1.6)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp 048ac2e0-b246-4749-b49c-662ad1ec071c))
  (fp_line (start 0.8 -1.6) (end -0.8 -1.6)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp d5f0e719-7eb8-4834-a6f5-5416184bf4b0))
  (fp_line (start 0.8 -1.6) (end 0.8 -2.1)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp fa93a72f-d1ab-46ec-a676-54357b0531b9))
  (fp_line (start 0.8 -1.2) (end -0.8 -1.2)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp 74d23d58-1abf-42e1-9bbc-0fbae38255c2))
  (fp_line (start 0.8 -1.2) (end 0.8 -0.8)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp 77b83898-015f-467f-ae88-e7e34b2bfc14))
  (fp_line (start 0.8 -0.4) (end -0.8 -0.4)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp 9cfbc909-52ee-4d81-a0ff-83951831811a))
  (fp_line (start 0.8 -0.4) (end 0.8 0)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp b41ad121-799e-4c82-af53-1176d07a00cb))
  (fp_line (start 0.8 0.4) (end -0.8 0.4)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp 57728562-0da2-4a9f-93af-f71c406efca3))
  (fp_line (start 0.8 0.4) (end 0.8 0.8)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp d0581fc7-68ce-492f-a71d-fd939b6fd160))
  (fp_line (start 0.8 1.2) (end -0.8 1.2)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp 062268c0-31cf-4ae7-bc7c-e0c3a5781d09))
  (fp_line (start 0.8 1.2) (end 0.8 1.6)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp c86a0f48-ec5c-44d5-a510-498b95987389))
  (fp_arc (start -1.4 2.099998) (mid -2.523886 -0.000001) (end -1.4 -2.1)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp 87d53441-9134-4a48-86c5-aae9cc314191))
  (fp_arc (start 1.4 -2.1) (mid 2.523886 -0.000001) (end 1.4 2.099998)
    (stroke (width 0.12) (type default)) (layer "F.Fab") (tstamp f63fedf8-2a74-4418-ae0a-b258fbdf9e48))
  (pad "1" thru_hole circle (at -1.7 0) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask") (tstamp ad8a300b-f923-4014-9c78-2e47d9f360c3))
  (pad "2" thru_hole circle (at 1.7 0) (size 1.5 1.5) (drill 0.7) (layers "*.Cu" "*.Mask") (tstamp 723dffcd-b385-4037-8232-bd9460600a5e))
  (model "${my_additions}/LDR_5mm_photoresistor.step"
    (offset (xyz 0 0 5))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
