(module Connector_IDC_2x17_P1.27mm_Vertical_SMD (layer F.Cu) (tedit 604A909F)
  (descr "IDC Connector 02x17 SMD")
  (fp_text reference REF** (at 0 -14.732) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Connector_IDC_2x17_P1.27mm_Vertical_SMD (at 0 15.113) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.937 -1.27) (end -3.556 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.937 1.27) (end -3.937 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.556 1.27) (end -3.937 1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.556 -1.27) (end -3.556 1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.7 13.045) (end -1.7 10.668) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.7 13.045) (end 1.7 10.668) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.7 13.045) (end 1.7 13.045) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.7 -13.045) (end 1.7 -10.668) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.7 -13.045) (end -1.7 -10.668) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.7 -13.045) (end 1.7 -13.045) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.5 -13.895) (end 2.5 -13.895) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.5 13.895) (end -2.5 13.895) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.5 13.895) (end 2.5 10.668) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.5 13.895) (end -2.5 10.668) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.5 -13.895) (end -2.5 -10.668) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.5 -13.895) (end 2.5 -10.668) (layer F.SilkS) (width 0.12))
  (fp_poly (pts (xy -3.556 -10.16) (xy -4.191 -9.779) (xy -4.191 -10.541)) (layer F.SilkS) (width 0.1))
  (fp_poly (pts (xy -1.016 -10.795) (xy -1.397 -11.43) (xy -0.635 -11.43)) (layer F.SilkS) (width 0.1))
  (pad 1 smd rect (at -2 -10.16) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 2 -10.16) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -2 -8.89) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 2 -8.89) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -2 -7.62) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 2 -7.62) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -2 -6.35) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 2 -6.35) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -2 -5.08) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 2 -5.08) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -2 -3.81) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 2 -3.81) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at -2 -2.54) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 2 -2.54) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at -2 -1.27) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at 2 -1.27) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at -2 0) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at 2 0) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at -2 1.27) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at 2 1.27) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at -2 2.54) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at 2 2.54) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at -2 3.81) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at 2 3.81) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at -2 5.08) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd rect (at 2 5.08) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd rect (at -2 6.35) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 28 smd rect (at 2 6.35) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 29 smd rect (at -2 7.62) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 30 smd rect (at 2 7.62) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 31 smd rect (at -2 8.89) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 32 smd rect (at 2 8.89) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 33 smd rect (at -2 10.16) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (pad 34 smd rect (at 2 10.16) (size 2.6 0.74) (layers F.Cu F.Paste F.Mask))
  (model "$(my_additions)/IDC_Connector_SMD_01x17.step"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
