(footprint "AHT20_hand-soldering" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Humidity and Temperature Sensor")
  (tags "humidity, temperature, sensor")
  (attr smd)
  (fp_text reference "REF**" (at 0.1 -2.4 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fadb8cbd-0ecf-417d-bc89-d413bda90d34)
  )
  (fp_text value "AHT20_hand-soldering" (at 0.3 2.8 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a929f35a-e04e-4f3c-8b09-10072ce4d0fe)
  )
  (fp_text user "${REFERENCE}" (at 0.3 4.3 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f5bf28d8-8a80-4113-aaea-5439ea679532)
  )
  (fp_line (start -1.7 -1.7) (end 1.7 -1.7)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 2a508d59-a012-4b49-9982-8b4e470cb08f))
  (fp_line (start -1.7 -1.4) (end -1.7 -1.7)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp d8a6b749-cdf8-4ddf-99ee-1bafab1d78cd))
  (fp_line (start -1.7 1.4) (end -1.7 1.7)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 5313c788-7555-4500-b4af-5eb061699b29))
  (fp_line (start -1.7 1.7) (end 1.7 1.7)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp a5506b32-0d06-4ce4-a651-9d00be085eb4))
  (fp_line (start 1.7 -1.7) (end 1.7 -1.4)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp b166b77c-6654-4636-b016-ea117b168ab9))
  (fp_line (start 1.7 1.7) (end 1.7 1.4)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp b82a2e95-19ea-400c-a46d-77119c84e38e))
  (fp_poly
    (pts
      (xy -0.5 -0.9)
      (xy -0.5 -1.2)
      (xy -0.2 -1.2)
    )

    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp e71f9eb3-3ee9-4dbc-bfc2-22a0138736db))
  (fp_rect (start -1.6 -1.6) (end 1.6 1.6)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.CrtYd") (tstamp 2318bd8a-e011-4a11-b964-1f056ca1276f))
  (fp_rect (start -1.5 -1.5) (end 1.5 1.5)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 765f011f-143f-44db-9e7f-8ce32896acab))
  (fp_poly
    (pts
      (xy -0.5 -0.9)
      (xy -0.5 -1.2)
      (xy -0.2 -1.2)
    )

    (stroke (width 0.1) (type solid)) (fill solid) (layer "F.Fab") (tstamp 745867b6-5c89-4466-a63d-51696a61e774))
  (pad "1" smd rect (at -1.2 -1) (size 1.2 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 690fa992-4204-483e-a34e-f0a12c895ba0))
  (pad "2" smd rect (at -1.2 0) (size 1.2 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp d903c4fc-c469-4922-8a5f-e9074086a60a))
  (pad "3" smd rect (at -1.2 1) (size 1.2 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 66d19cf9-30de-4eac-8e53-63de96b41374))
  (pad "4" smd rect (at 1.2 1) (size 1.2 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp b7ddb2a6-9cec-4d77-82e5-fe333e1fc230))
  (pad "5" smd rect (at 1.2 0) (size 1.2 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 4ca26a4c-b1b6-47b2-8ba9-fd074433532a))
  (pad "6" smd rect (at 1.2 -1) (size 1.2 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 8a6b1c9c-d6ec-4e85-a0a2-ae7e56646108))
  (model "${my_additions}/AHT20_Sensor.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
