(footprint "L_CommonMode_7x8mm" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -8.5 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 071420d2-d181-4b72-9f68-df958125fb36)
  )
  (fp_text value "L_CommonMode_7x8mm" (at 0 9 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 23324487-c01c-434f-8145-2552a06c1ce4)
  )
  (fp_rect (start -1.5 -7.5) (end 1.5 7.5) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 24ffa79f-be1a-4bf6-bd71-6c290d55f1e0))
  (fp_rect (start -5.25 -6.25) (end 5.25 6.25) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 870ce796-704f-4954-9556-3799a4e301c2))
  (fp_rect (start -5.75 -8) (end 5.75 8) (layer "F.CrtYd") (width 0.12) (fill none) (tstamp 9ff542a4-c5f7-4814-a60c-6ba0d0ad7c19))
  (pad "1" thru_hole circle (at -3.5 -4) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask) (tstamp 9d41b3aa-c3f2-41a0-bce9-3779d8374794))
  (pad "2" thru_hole circle (at 3.5 -4) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask) (tstamp b88bb23e-aae2-47e7-aadb-f6b56b31f7dc))
  (pad "3" thru_hole circle (at -3.5 4) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask) (tstamp 384f8237-5e36-4233-913a-4bb2484931a8))
  (pad "4" thru_hole circle (at 3.5 4) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask) (tstamp a06e6b73-6b58-4456-bc0f-afc6f20f8a51))
  (model "${my_additions}/L_Commonmode_7x8mm.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
