(footprint "Buzzer-6636CY-HC6035" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Buzzer, Elektromagnetic Beeper, Summer,")
  (tags "buzzer, beeper, 6636CY, HC6035")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -4.3) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3fce2839-e576-4a7b-b2e7-e919865f9536)
  )
  (fp_text value "6636CY" (at 0 4.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 302ea18c-5cfd-4c9a-a42d-88d742855770)
  )
  (fp_text user "+" (at -1.5 -1.6) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9f6fd021-af6c-4053-ad1d-3e367deb9249)
  )
  (fp_text user "${REFERENCE}" (at 0 -4.3) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 80a0e8dd-e3b1-48d1-abcf-9c8e192f63a4)
  )
  (fp_text user "+" (at -1.5 -1.6) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp deaf7cc5-9d17-4cd0-a7d5-a53096c8590c)
  )
  (fp_circle (center 0 0) (end 3.6 0)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp be050cbe-13f5-4c09-9af9-b39d02590d28))
  (fp_circle (center 0 0) (end 3.4 0)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 698173be-7376-4703-97c1-ff7ab6a6f2d9))
  (fp_circle (center 0 0) (end 0.5 0)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 58d8d2cd-d57f-4653-8b16-8af048f5e69c))
  (fp_circle (center 0 0) (end 3.6 0)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 41a87d12-abdc-49d5-83d7-70f4a76e6240))
  (pad "1" thru_hole rect (at -1.6 0) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 5d967ec6-88bd-4210-b548-56976a879379))
  (pad "2" thru_hole circle (at 1.6 0) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask") (tstamp d6fb77c0-881f-4fb9-977a-c59417919be6))
  (model "${my_additions}/Buzzer-6636CY.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
