(footprint "TestPoint_THTPad_D1.5mm_Drill0.7mm_no_silk"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
	(tags "test point THT pad")
	(property "Reference" "REF**"
		(at 0 -1.648 0)
		(layer "F.SilkS")
		(uuid "8e3b35bb-4555-4b98-b228-8e15c28a300a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "TestPoint_THTPad_D1.5mm_Drill0.7mm_no_silk"
		(at 0 1.75 0)
		(layer "F.Fab")
		(uuid "8c0c2105-72ba-497b-b863-69823727ae67")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f66c147c-ecfa-48a9-ba64-2c9d9d3acde2")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8204a899-7b60-4ebe-a974-59705ac98aa9")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5f92940a-050b-4849-bff9-8f4f85794d93")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_circle
		(center 0 0)
		(end 0.8 0)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "a201c06a-732b-45b2-a5b8-3b9b053aee31")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -1.65 0)
		(layer "F.Fab")
		(uuid "258d936c-5468-40a7-bb8d-0b29d21bf981")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.5 1.5)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d4c59acd-c0ea-4830-8b44-6dc762ed1a14")
	)
)
