(footprint "SW_micro_TS-B003-Y"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Micro tactile angled button 3x6x3.5mm")
	(tags "micro, tactile, button")
	(property "Reference" "REF**"
		(at -12.6 -19.1 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "e92a3bcf-e357-4dfd-ba46-c950929f36ad")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "TS-B003-Y"
		(at -12.6 -17.6 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "a44c2629-292d-48bf-8c6a-35afbbc138b5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1b1cee75-4d5f-4b9e-a7db-cc1bb3e36b8f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Micro tactile angled button 3x6x3.5mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "32efc2b2-528e-463b-9921-eb47b25d32fe")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -3.5 -3.1)
		(end 3.5 0.9)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "83ab18a2-e1ec-436e-804f-7e624e3e1578")
	)
	(fp_text user "${REFERENCE}"
		(at -12.6 -16.1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "0572fe6c-a5b4-4d45-a8f3-fa2829b37b9e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" smd rect
		(at -3.8 -0.55)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "3f2bf5db-a4af-461b-b84d-67609be9f9b2")
	)
	(pad "" smd rect
		(at -3.45 -0.95)
		(size 1.5 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "ea8b3b2b-31cb-4c7c-8431-d877ceb898a0")
	)
	(pad "" np_thru_hole circle
		(at -1.15 0)
		(size 0.9 0.9)
		(drill 0.9)
		(layers "F&B.Cu" "*.Mask")
		(uuid "396ab127-63ef-455b-b081-a64396fa9b70")
	)
	(pad "" np_thru_hole circle
		(at 1.15 0)
		(size 0.9 0.9)
		(drill 0.9)
		(layers "F&B.Cu" "*.Mask")
		(uuid "c717789c-3bd0-4d45-bf73-48e6d0678e19")
	)
	(pad "" smd rect
		(at 3.45 -0.95)
		(size 1.5 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "a6a5d82a-f1b8-49b3-ba09-4279fccae7ad")
	)
	(pad "" smd rect
		(at 3.8 -0.55)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "9811b1b4-5f55-4b67-825d-9fbd8bad98ed")
	)
	(pad "1" smd rect
		(at -2.1 1.3)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "03ff5a55-12c8-4349-92ff-fba21eafe7bd")
	)
	(pad "2" smd rect
		(at 2.1 1.3)
		(size 1.2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "6e2edcb0-5f91-477a-bac7-78e845ae2e46")
	)
	(group ""
		(uuid "16961dbc-585c-4835-90d1-983c43949438")
		(members "3f2bf5db-a4af-461b-b84d-67609be9f9b2" "ea8b3b2b-31cb-4c7c-8431-d877ceb898a0")
	)
	(group ""
		(uuid "ce6833a8-045f-4dab-b2d4-98c4442ec7cf")
		(members "9811b1b4-5f55-4b67-825d-9fbd8bad98ed" "a6a5d82a-f1b8-49b3-ba09-4279fccae7ad")
	)
	(embedded_fonts no)
)
