(footprint "SIM800L-module" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "SIM800L GSM module")
  (tags "SIM800, GMS, module,")
  (attr through_hole)
  (fp_text reference "REF**" (at -12.6 -12.5) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 2b162358-e413-40aa-b0d2-bb19b2a8994d)
  )
  (fp_text value "SIM800L-module" (at 0 2.7) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c2a4987f-ef9b-4307-8cd0-937b4396e4a7)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 60c58827-6aae-46dc-a86c-3ccb1f2ea07a)
  )
  (fp_text user "SIM" (at 0 -15.7 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify bottom))
    (tstamp bbdc9a4c-7935-4f5c-9dd9-ac9e2a8e624f)
  )
  (fp_rect (start -12.6 -11.6) (end 12.6 11.6)
    (stroke (width 0.15) (type default)) (fill none) (layer "F.SilkS") (tstamp d3098dd8-37fa-46d5-96ab-ea0a62022f66))
  (fp_rect (start -12.5 -11.5) (end 12.5 11.5)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 7f444351-2cca-4a46-9264-1c163ac24cd0))
  (fp_line (start -4.1 -17.6) (end 3.9 -17.6)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 9fc57228-0d09-4efc-9bc4-f6d7fde8705c))
  (fp_line (start -4.1 -11.4) (end -4.1 -17.6)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp f90e06f0-3d90-4739-82dd-f6b2fc78034e))
  (fp_line (start -0.3 -12.9) (end 0 -11.9)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp d26c01c2-755f-44ec-b5ff-77f00b80d567))
  (fp_line (start 0 -12.9) (end 0 -15.2)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 75cc5d12-d490-4405-b36f-491c1de5d263))
  (fp_line (start 0 -11.9) (end 0.3 -12.9)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 0b839e70-4cdf-4764-936c-0269ca4aa5ec))
  (fp_line (start 0.3 -12.9) (end -0.3 -12.9)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 39554a2f-18fa-482f-8fa9-b3801c7538fc))
  (fp_line (start 3.9 -17.6) (end 3.9 -11.4)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 0576a317-3886-494a-acad-b1fe2d1aaec5))
  (fp_rect (start -12.4 -11.4) (end 12.4 11.4)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp ed76da88-12a6-4512-86ad-3587bd05f523))
  (fp_rect (start -8 -5.1) (end 8 10.2)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp cabcf77b-caa7-4a3b-a81a-a958465f56fd))
  (fp_arc (start 2.9 -11.4) (mid 0 -8.5) (end -2.9 -11.4)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 3f977e38-b756-45a3-884c-15f22cbe8d0b))
  (pad "2" thru_hole circle (at -11 -4.16 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 4de7d336-be68-4754-b34f-23ab10153335))
  (pad "3" thru_hole circle (at -11 -1.62 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 4dc137eb-5aa0-4538-9037-31253cf83aff))
  (pad "4" thru_hole circle (at -11 0.92 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 743ef3e3-2347-48d7-a1b8-388084fcabda))
  (pad "5" thru_hole circle (at -11 3.46 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 371f29a0-80cc-48ce-8120-4ce423fc1311))
  (pad "6" thru_hole circle (at -11 6 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask") (tstamp cb9fda53-0acd-4c4b-9048-79bc741b426e))
  (pad "7" thru_hole circle (at 11 8.5 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask") (tstamp de97df00-6462-4419-82f9-aebcd4ba2267))
  (pad "8" thru_hole circle (at 11 5.96 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 7adeaa13-1e79-4825-bc9b-37f97bcf67f5))
  (pad "9" thru_hole circle (at 11 3.42 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask") (tstamp f15ccc1b-8464-428e-bc6f-7ef07fe6b020))
  (pad "10" thru_hole circle (at 11 0.88 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 22e55f03-7122-4df2-a6b2-7092fea41094))
  (pad "11" thru_hole circle (at 11 -1.66 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask") (tstamp da23fc14-55e7-4c8e-9e4f-cfcfd2a8c1bd))
  (pad "12" thru_hole circle (at 11 -4.2 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask") (tstamp b3ff6056-06b5-44c1-9252-0d2a34323f25))
  (model "${my_additions}/SIM800L.step"
    (offset (xyz 0 0 2.5))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
