(footprint "LED_SK6812MINI-012" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.6) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp f3f599d1-b1e0-4872-a2e6-18eb18b9def7)
  )
  (fp_text value "LED_SK6812MINI-012" (at 0 2.7) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7f19e271-9ec3-4785-9348-fc554bcccc4c)
  )
  (fp_text user "${REFERENCE}" (at 0 4.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 0c507a7d-7abf-4cdc-9ff3-39f543339aa5)
  )
  (fp_line (start -1.9 -1.9) (end 1.9 -1.9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 45d2ad69-894c-4d25-a74f-2c1e68b10419))
  (fp_line (start -1.9 -1.4) (end -1.9 -1.9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 01d2affe-88d9-46b3-b0ed-55bc4cce82c7))
  (fp_line (start -1.9 1.4) (end -1.9 1.9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp e48db661-495d-467b-88b8-5ca01f44ce55))
  (fp_line (start -1.9 1.9) (end 1.4 1.9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 59bde027-32bb-44c2-b30f-b4c7ded2746c))
  (fp_line (start 1.4 1.9) (end 1.9 1.4)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 7b342723-0c7c-405a-b6d4-630f76822f26))
  (fp_line (start 1.9 -1.9) (end 1.9 -1.4)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp e57454b2-5920-4831-ba79-0519009a1bb7))
  (fp_rect (start -1.75 -1.75) (end 1.75 1.75)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.CrtYd") (tstamp eab8cd1b-791a-4e69-b94a-1e15f2bac2fe))
  (fp_line (start -1.9 -1.9) (end -1.9 1.9)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp fd548db6-c8c8-4996-ae38-32b9a2037a75))
  (fp_line (start -1.9 1.9) (end 1.4 1.9)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp de056733-273a-4969-9065-dec7665f0a28))
  (fp_line (start 1.4 1.9) (end 1.9 1.4)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 6ba8ed68-cd62-4eab-b67e-3a370de58057))
  (fp_line (start 1.9 -1.9) (end -1.9 -1.9)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 0b48cf4c-2f9c-4195-9f2d-e07a1e0c506f))
  (fp_line (start 1.9 1.4) (end 1.9 -1.9)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp a1a8ef90-6472-423e-96dd-db0c4509a5f0))
  (fp_circle (center 0 0) (end 1.6 0)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 0d627719-cf8d-4553-88f6-8ac148fd8b44))
  (pad "1" smd rect (at 1.5 0.85) (size 1.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp b53aba51-3f30-431d-afa8-4337b3913f05))
  (pad "2" smd rect (at 1.05 -0.7) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp cd18c868-4c8f-43a6-9a6e-41cd664275ea))
  (pad "3" smd rect (at -1.4 -0.65) (size 1.5 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 3b42f95c-da07-4f16-aca9-a3e3a830163a))
  (pad "4" smd rect (at -0.95 0.9) (size 2.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp e265a5dd-78ea-422a-9308-a36d14ebca82))
  (model "${my_additions}/SK6812MINI-012.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 180))
  )
)
