(footprint "USB-C_12(16)pin_legs"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "USB Type-C  female 12(16) pins. SMD with 4 through-hole legs")
	(tags "usb type-c")
	(property "Reference" "REF**"
		(at -5.8 -3.2 90)
		(layer "F.SilkS")
		(uuid "7e7ba1e7-21d3-4831-9b26-d73c892d6157")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "USB_type_C_smd_12p"
		(at -0.1 3.6 0)
		(layer "F.Fab")
		(uuid "44d2f8ff-835f-461d-8ef3-189117403fbe")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at -34.4 -27.6 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ea54f483-1540-44ef-9cfa-c18707c75ad1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at -34.4 -27.6 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4352b88c-71bf-4d12-8814-2c49db2627f2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -5 -5.5)
		(end -4 -5.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "9a61d4a5-f2ec-4392-8587-b8a9190affa3")
	)
	(fp_line
		(start -5 1.4)
		(end -5 -5.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "38bcc8c0-43e9-4ed1-8461-78e69a5c9f4d")
	)
	(fp_line
		(start 5 -5.5)
		(end 4 -5.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "52076a1e-91e6-47ac-b25b-99219c2e80af")
	)
	(fp_line
		(start 5 1.4)
		(end 5 -5.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "33fd911f-e4ed-4e8f-8e39-2f22ee880a0a")
	)
	(fp_line
		(start -4.4 1.8)
		(end 4.4 1.8)
		(stroke
			(width 0.1)
			(type dash)
		)
		(layer "Dwgs.User")
		(uuid "1ecc1ebc-1e61-43c2-957a-d8a5f81dc732")
	)
	(fp_rect
		(start -4.8 -5.3)
		(end 4.8 2.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "3c53a331-08ba-46d2-9e14-44f640faa8ef")
	)
	(fp_rect
		(start -4.47 -4.75)
		(end 4.47 2.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "ad8a9757-6b41-4434-b47e-e656eb442b47")
	)
	(fp_text user "PCB Edge"
		(at 0 1.5 0)
		(unlocked yes)
		(layer "Dwgs.User")
		(uuid "e06eda43-2787-4471-a5dc-b97b0175767c")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.1)
				(bold yes)
			)
			(justify bottom)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 -2.4 0)
		(layer "F.Fab")
		(uuid "84755afc-ca88-4bad-adf2-1deb6fec8e35")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at -2.89 -3.68)
		(size 0.65 0.65)
		(drill 0.65)
		(layers "F&B.Cu" "*.Mask")
		(uuid "a1ef6779-ad19-467f-8e35-4232f945f9f8")
	)
	(pad "" np_thru_hole circle
		(at 2.89 -3.68)
		(size 0.65 0.65)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(uuid "c79e9435-6c1c-4e4c-9f1b-84243287c627")
	)
	(pad "A1" smd rect
		(at -3.2 -5.045)
		(size 0.6 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "3f96c1d1-0571-4353-a915-a7c0d7be5040")
	)
	(pad "A4" smd rect
		(at -2.4 -5.045)
		(size 0.6 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "7fa84788-bbc6-4562-8e73-a9247f296526")
	)
	(pad "A5" smd rect
		(at -1.75 -5.045)
		(size 0.25 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "7f885070-d512-4623-9ed1-9e2bc88c3cf9")
	)
	(pad "A6" smd rect
		(at -0.25 -5.045)
		(size 0.25 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "6c467e7f-6ae9-4c9c-8293-0ce9bc535526")
	)
	(pad "A7" smd rect
		(at 0.75 -5.045)
		(size 0.25 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "68947e92-0137-4c3d-8df7-cffbe3e0ae60")
	)
	(pad "A8" smd rect
		(at 1.75 -5.045)
		(size 0.25 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "96f920c0-01bc-4c87-9856-b6327cc35217")
	)
	(pad "A9" smd rect
		(at 2.4 -5.045)
		(size 0.6 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "91330bdf-cdba-499a-8115-6cd6ba6ba822")
	)
	(pad "A12" smd rect
		(at 3.2 -5.045)
		(size 0.6 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "dc48ec50-8dc7-4536-b1e4-5e3af05d33e6")
	)
	(pad "B1" smd rect
		(at 3.2 -5.045)
		(size 0.6 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "1d3361aa-2faa-4af5-ad91-9b541f207eac")
	)
	(pad "B4" smd rect
		(at 2.4 -5.045)
		(size 0.6 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "98d50175-d409-49cb-9650-606e913f9bff")
	)
	(pad "B5" smd rect
		(at 1.25 -5.045)
		(size 0.25 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "d9a9f716-b237-45de-92c3-0741a5c45d27")
	)
	(pad "B6" smd rect
		(at 0.25 -5.045)
		(size 0.25 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "c993af3e-54d5-4ee3-9ca5-83454ce10897")
	)
	(pad "B7" smd rect
		(at -0.75 -5.045)
		(size 0.25 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "94aaa72b-8ccb-48bc-b471-ff74599d388b")
	)
	(pad "B8" smd rect
		(at -1.25 -5.045)
		(size 0.25 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "54eaa484-345d-4a74-a847-bee14619af35")
	)
	(pad "B9" smd rect
		(at -2.4 -5.045)
		(size 0.6 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "f797f565-fb3e-4789-938c-c83095cd7668")
	)
	(pad "B12" smd rect
		(at -3.2 -5.045)
		(size 0.6 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "e94d7b31-6239-4a8f-99d5-cd952d095649")
	)
	(pad "S1" thru_hole oval
		(at -4.32 -4.18)
		(size 1 2.1)
		(drill oval 0.6 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6493fdd3-13da-46ea-9b73-641b0437d92c")
	)
	(pad "S1" thru_hole oval
		(at -4.32 0)
		(size 1 1.6)
		(drill oval 0.6 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5107fb4e-a69f-4991-83d9-e1702ff5556d")
	)
	(pad "S1" thru_hole oval
		(at 4.32 -4.18)
		(size 1 2.1)
		(drill oval 0.6 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9cd47795-6191-4aef-9d0c-80905814e183")
	)
	(pad "S1" thru_hole oval
		(at 4.32 0)
		(size 1 1.6)
		(drill oval 0.6 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "81806171-de01-44bc-a546-48db4ae8489b")
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "USB_type_C_smd_12p_v2.step")
			(type model)
			(data |KLUv/aBC6g0AvIUCqtf3dCjg8Gg6+A8c3WxmzlME2C8O/HQpIUJf1CRlkiklJYTB+WE5hhmoDgYc
[encoded data, 152442 characters]
				3D9LVHPBDXv6fN6SaQaGFnzoFDLqI4/VNw==|
			)
			(checksum "66A30F62DCA3818BEFF0A00E1561BB38")
		)
	)
	(model "kicad-embed://USB_type_C_smd_12p_v2.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
