(footprint "FPC_Connector_1.0K-DX-14PWB" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "HDGC FPC Connector 1.0K-DX-14PWB")
  (tags "fpc, connector, flat cable")
  (attr smd)
  (fp_text reference "REF**" (at 7.1 -0.7) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp e7bf642b-2c82-4784-b19f-0da80a266795)
  )
  (fp_text value "1.0K-ES-14PWB" (at 0 3.4) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c93d9188-b485-4f38-bd8d-e361be43063a)
  )
  (fp_text user "${REFERENCE}" (at 0 1.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 940584f8-2632-4448-8ecc-84c1b7771847)
  )
  (fp_line (start -9.95 0) (end -9.95 0.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp c37b34f7-74be-4ced-8044-2fec3fab1d2c))
  (fp_line (start -9.95 4.5) (end 9.95 4.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp c5daafde-52b4-4e6c-92d9-60cccb8521e5))
  (fp_line (start -9.95 5.3) (end -9.95 3.3)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 271a8fdc-11a3-4ebb-bc2a-e6b453c28035))
  (fp_line (start -9.95 5.3) (end 9.95 5.3)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 92da0955-3ae5-4704-b116-ba0c3c7d8f6a))
  (fp_line (start -7 0) (end -9.95 0)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp c6f59a22-1b1f-434e-866c-5f508a33b693))
  (fp_line (start 9.95 0) (end 7 0)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp f15f25f9-dc41-4cee-a546-1e7d0d4e94e7))
  (fp_line (start 9.95 0) (end 9.95 0.5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 6a6a5da4-d4ff-4388-b123-874566e87507))
  (fp_line (start 9.95 5.3) (end 9.95 3.3)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp c75449c1-63f0-465b-9945-7a0c642c2e38))
  (fp_poly
    (pts
      (xy -6.5 -1.8)
      (xy -6.7 -2.1)
      (xy -6.3 -2.1)
    )

    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 201abed3-b7d7-4862-8313-5d7aed3697ba))
  (fp_line (start -9.9 0) (end -7 0)
    (stroke (width 0.12) (type default)) (layer "F.CrtYd") (tstamp 44fa0da9-a920-4908-9b9b-336254e8b935))
  (fp_line (start -9.9 5.2) (end -9.9 0)
    (stroke (width 0.12) (type default)) (layer "F.CrtYd") (tstamp b366d63a-8106-4ebf-98f7-191c2a071b18))
  (fp_line (start -7 -1.2) (end 7 -1.2)
    (stroke (width 0.12) (type default)) (layer "F.CrtYd") (tstamp 35aa8369-a77c-4e15-b27c-75675555f5c1))
  (fp_line (start -7 0) (end -7 -1.2)
    (stroke (width 0.12) (type default)) (layer "F.CrtYd") (tstamp d2641ec0-0219-4635-9814-e1b3eadb131b))
  (fp_line (start 7 -1.2) (end 7 0)
    (stroke (width 0.12) (type default)) (layer "F.CrtYd") (tstamp d8f3f8e7-f87a-4178-8a52-a458190460d8))
  (fp_line (start 7 0) (end 9.9 0)
    (stroke (width 0.12) (type default)) (layer "F.CrtYd") (tstamp 327e577a-ba1c-4489-a540-b042efe173bf))
  (fp_line (start 9.9 0) (end 9.9 5.2)
    (stroke (width 0.12) (type default)) (layer "F.CrtYd") (tstamp ab56514f-192a-41b2-854b-905d095993ab))
  (fp_line (start 9.9 5.2) (end -9.9 5.2)
    (stroke (width 0.12) (type default)) (layer "F.CrtYd") (tstamp 457e9ff2-93ce-428c-a61d-23eae0f1b5e4))
  (fp_line (start -9.8 4.5) (end 9.8 4.5)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 8374212b-e32e-4a0c-9787-8d4b3fc0fab1))
  (fp_line (start -6.5 0.4) (end -6.5 0.1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 419172e2-25af-4d38-9d92-a4136b631bfd))
  (fp_line (start -5.5 0.4) (end -5.5 0.1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp e9d1beee-c9cb-4120-96a6-1ebd6b5cbe08))
  (fp_line (start -4.5 0.4) (end -4.5 0.1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 08d30677-54d9-4ecb-b2ba-76ef4c5ec70a))
  (fp_line (start -3.5 0.4) (end -3.5 0.1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 86c254c6-5e41-411d-9c27-08c4a3383cac))
  (fp_line (start -2.5 0.4) (end -2.5 0.1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 3a484595-7f4f-4f03-b2f7-839c2ad54299))
  (fp_line (start -1.5 0.4) (end -1.5 0.1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 613c00a6-7d20-43a6-8060-35585d0c30c6))
  (fp_line (start -0.5 0.4) (end -0.5 0.1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp d6c88c8c-fa63-4ae3-a97c-ca349ffe7927))
  (fp_line (start 0.5 0.4) (end 0.5 0.1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 40a20ece-f173-4635-aa1b-4e2a9609b65a))
  (fp_line (start 1.5 0.4) (end 1.5 0.1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 04ea5475-46c5-4f23-b45e-7d2fe0a552d8))
  (fp_line (start 2.5 0.4) (end 2.5 0.1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 5e2564e3-631f-482c-b649-bf83a49d9a85))
  (fp_line (start 3.5 0.4) (end 3.5 0.1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp cd37e256-36f0-4ce4-ae7c-8fef69c0c161))
  (fp_line (start 4.5 0.4) (end 4.5 0.1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp de6c909e-420b-44bd-930c-1e323cad1801))
  (fp_line (start 5.5 0.4) (end 5.5 0.1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 78f1399e-385c-446b-b696-3a137f5c5b1b))
  (fp_line (start 6.5 0.4) (end 6.5 0.1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 82e3a8ea-f0b7-415c-8165-437e82e3ee7d))
  (fp_rect (start -9.8 5.2) (end 9.8 0.4)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp cda4bc98-c8e2-43b7-b189-34581373d526))
  (pad "1" smd rect (at -6.5 -0.7) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp baf463e1-a7ec-46af-a928-638602ab9eb3))
  (pad "2" smd rect (at -5.5 -0.7) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 2fa6261c-0a55-418e-8748-b904ee7c2ee3))
  (pad "3" smd rect (at -4.5 -0.7) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 8c7d530d-de2f-42e7-a2c6-462a8f3f57b0))
  (pad "4" smd rect (at -3.5 -0.7) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 15dfc6eb-647b-4bab-be1f-15784ddced94))
  (pad "5" smd rect (at -2.5 -0.7) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 997254f3-9907-42f8-9ac5-cafb0ebb7bac))
  (pad "6" smd rect (at -1.5 -0.7) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 57ac7c76-668f-4e3b-83b6-63cf5246c036))
  (pad "7" smd rect (at -0.5 -0.7) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 3b474447-0733-49bf-a231-f0307be3145f))
  (pad "8" smd rect (at 0.5 -0.7) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp c7c82633-2911-41f1-bd1e-15e7de2fcfb1))
  (pad "9" smd rect (at 1.5 -0.7) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 7bc0e6d5-bb4d-4e27-8045-225d5e0f40e5))
  (pad "10" smd rect (at 2.5 -0.7) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 9ef7bd81-eeba-48ee-bdd7-42d5bb913444))
  (pad "11" smd rect (at 3.5 -0.7) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 9f7273ee-783e-469b-b5b9-03d9daf62b69))
  (pad "12" smd rect (at 4.5 -0.7) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 30ff1ce3-b50c-4ab8-9f69-2c41a62ab6b9))
  (pad "13" smd rect (at 5.5 -0.7) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 0e00ae85-6090-4ba0-8d69-f01497577aba))
  (pad "14" smd rect (at 6.5 -0.7) (size 0.4 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 29537b48-52fa-4b71-b521-93119ded382c))
  (pad "MP" smd rect (at -9.25 1.9) (size 2.5 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 27811b89-de78-4e68-acbf-f61c1fd42478))
  (pad "MP" smd rect (at 9.25 1.9) (size 2.5 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 181ff1a6-d7dc-4f65-b825-9d21ca11dbc7))
  (model "${my_additions}/1.0K-DX-14PWB.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
