(footprint "Fuse_1808_0451_Holder_HandSolder" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5F68FEF1)
  (descr "Fuse SMD 1808 https://aliexpress.ru/item/10000001106516.html?sku_id=12000024121607749&spm=a2g2w.productlist.search_results.17.7f124aa6lKLWXf")
  (tags "fuse handsolder")
  (attr smd)
  (fp_text reference "REF**" (at 0.2 -3.5) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 08e3cc40-a961-4547-8b96-57a6010139e2)
  )
  (fp_text value "Fuse_1808_0451_Holder_HandSolder" (at 0.1 3.6) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 8a71d230-fd0c-44f1-bc06-9a46f771681a)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 31a043f3-95df-4daf-aeab-2f9597299aa5)
  )
  (fp_line (start -5 2.5) (end -5 2.1) (layer "F.SilkS") (width 0.12) (tstamp 3674c9a8-6aee-4969-870b-4ca385424e32))
  (fp_line (start -5 2.5) (end 5 2.5) (layer "F.SilkS") (width 0.12) (tstamp 3d9794af-c6ad-42a9-a0e6-6f38ac8fc454))
  (fp_line (start 5 2.5) (end 5 2.1) (layer "F.SilkS") (width 0.12) (tstamp 73d356fe-5aa3-42d9-9072-3c84da46af07))
  (fp_line (start -5 -2.5) (end -5 -2.1) (layer "F.SilkS") (width 0.12) (tstamp 92ed25c5-f60e-41c4-bab9-154553222289))
  (fp_line (start 5 -2.5) (end 5 -2.1) (layer "F.SilkS") (width 0.12) (tstamp 95477d2e-dc30-4f92-9020-ae21e7752032))
  (fp_line (start -5 -2.5) (end 5 -2.5) (layer "F.SilkS") (width 0.12) (tstamp a0c9ffab-3db3-4171-ab74-2e36537ccba1))
  (fp_rect (start -5.2 -2.6) (end 5.2 2.6) (layer "F.CrtYd") (width 0.12) (fill none) (tstamp 2ea4ac5b-264a-4a57-aea6-a1f01b36cacc))
  (fp_line (start 2.25 -1.6) (end 2.25 1.6) (layer "F.Fab") (width 0.1) (tstamp 90870a81-1bd0-4eb5-b3d8-0884615f8eca))
  (fp_line (start -2.25 1.6) (end -2.25 -1.6) (layer "F.Fab") (width 0.1) (tstamp dab29ee6-2cb5-4d81-b74a-11beb3bd3a09))
  (pad "1" smd roundrect (at -3.61 0) (size 5.08 3.81) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.08) (tstamp 83a0d48f-ba11-4401-8828-0e7504307ded))
  (pad "2" smd roundrect (at 3.61 0) (size 5.08 3.81) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.08) (tstamp 387f3196-a575-4511-83e7-110ec20cfe69))
  (model "${my_additions}/SMD-fuse-holder-for-1808-fuse_with_fuse.step"
    (offset (xyz 0 0 0.2))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
