(footprint "BNC-KE_22.5mm_long" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5A1DBFC1)
  (descr "BNC female PCB mount 4 pin straight chassis connector http://www.te.com/usa-en/product-1-1478204-0.html")
  (tags "BNC female PCB mount 4 pin straight chassis connector ")
  (attr through_hole)
  (fp_text reference "REF**" (at -0.25 -6.25) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3a6ff247-253c-46be-bf30-139c658c06f9)
  )
  (fp_text value "BNC-KE_22.5mm_long" (at 0 6.5) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bb0e2cba-5c99-48d6-8e5e-97a69e16a3cd)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a21a3d9c-6c11-4f52-8401-f5259b1d58ca)
  )
  (fp_arc (start -2.5 -4.9) (mid 0 -5.500909) (end 2.5 -4.9) (layer "F.SilkS") (width 0.12) (tstamp 0e0eb948-47b3-4c42-bddc-0d0de9019f71))
  (fp_arc (start -4.9 2.5) (mid -5.500909 0) (end -4.9 -2.5) (layer "F.SilkS") (width 0.12) (tstamp 2c912a0b-2f09-4208-85ae-00c0baa3721d))
  (fp_arc (start 2.5 4.9) (mid 0 5.500909) (end -2.5 4.9) (layer "F.SilkS") (width 0.12) (tstamp 7233b03f-1ef1-47c4-b6ae-f7b38a25f1d9))
  (fp_arc (start 4.9 -2.5) (mid 5.500909 0) (end 4.9 2.5) (layer "F.SilkS") (width 0.12) (tstamp d2558a92-acf9-4fea-bbb6-ee3755eb23e7))
  (fp_line (start -5.5 5.5) (end -5.5 -5.5) (layer "F.CrtYd") (width 0.05) (tstamp 2c72c170-89db-4819-9dcb-1e73e2e1e548))
  (fp_line (start 5.5 -5.5) (end 5.5 5.5) (layer "F.CrtYd") (width 0.05) (tstamp 6967a5f4-0742-47e4-987c-aeccd5fab0f1))
  (fp_line (start -5.5 -5.5) (end 5.5 -5.5) (layer "F.CrtYd") (width 0.05) (tstamp 8db283cc-f882-4a57-96da-3f857f09b0cc))
  (fp_line (start 5.5 5.5) (end -5.5 5.5) (layer "F.CrtYd") (width 0.05) (tstamp c282a32f-bbb1-4e82-bdc8-53df2ddff881))
  (fp_circle (center 0 0) (end 5.5 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp b9aa5c04-7a16-4b74-a6ab-066a7d1d9496))
  (pad "1" thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.2) (layers *.Cu *.Mask) (tstamp f0f7bfb4-2033-4ee5-a1c9-e4e5b846ec80))
  (pad "2" thru_hole circle (at -3.25 -3.25) (size 3.4 3.4) (drill 1.6) (layers *.Cu *.Mask) (tstamp 553b2698-79f2-4522-9029-f003906cce61))
  (pad "2" thru_hole circle (at 3.25 3.25) (size 3.4 3.4) (drill 1.6) (layers *.Cu *.Mask) (tstamp 5d1bd656-097b-4603-a789-891bc267ca20))
  (pad "2" thru_hole circle (at 3.25 -3.25) (size 3.4 3.4) (drill 1.6) (layers *.Cu *.Mask) (tstamp d2cba9ae-5d2e-4ce8-8282-96fe847d4171))
  (pad "2" thru_hole circle (at -3.25 3.25) (size 3.4 3.4) (drill 1.6) (layers *.Cu *.Mask) (tstamp f21f9418-7d42-4668-9843-8d8fac878198))
  (model "${my_additions}/BNC-KE_jack.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
