(footprint "DG128-5.08-03P-14-1000(H)" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Degson screw terminal block DG128-5.08-03P")
  (tags "terminal block, screw terminal, connector")
  (attr through_hole)
  (fp_text reference "REF**" (at -7.747 -5.715) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 10d56af5-466e-4115-9bd7-a16fe3b6c8c9)
  )
  (fp_text value "DG128-5.08-03P-14-1000(H)" (at 0.254 6.755) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp febb6743-33b8-4308-8005-405b0820f39f)
  )
  (fp_text user "${REFERENCE}" (at 0.254 8.255) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c30dc36b-b157-450d-806a-3aef1f9fe950)
  )
  (fp_rect (start -7.62 -5) (end 7.62 5.2)
    (stroke (width 0.15) (type default)) (fill none) (layer "F.SilkS") (tstamp 229c1126-64ae-4451-ade0-c3120a86c713))
  (fp_rect (start -7.62 -5) (end 7.62 5.2)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 7dba1d57-3f4f-49d3-a5b0-ad8e5e8681b9))
  (fp_line (start -6.35 2.032) (end -3.81 2.032)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp fcb81f0d-6c2d-48cd-b718-600a18edd13e))
  (fp_line (start -6.35 4.953) (end -6.35 2.032)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 8dc43a77-68a3-4deb-a4d7-bef02de3a828))
  (fp_line (start -3.81 2.032) (end -3.81 4.953)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 58a3d69f-dfd2-4707-98f3-39d8f602e14e))
  (fp_line (start -1.27 2.032) (end 1.27 2.032)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp bc69efe4-fc2b-4138-94d6-9aa93bb16fda))
  (fp_line (start -1.27 4.953) (end -1.27 2.032)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 1d26f19b-b1e8-4e54-b082-6c2b79a4b209))
  (fp_line (start 1.27 2.032) (end 1.27 4.953)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp c4e34363-3bde-41f9-a24b-2698506db41e))
  (fp_line (start 3.81 2.032) (end 6.35 2.032)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 9727472c-b1be-4168-bb76-92b6d08377b6))
  (fp_line (start 3.81 4.953) (end 3.81 2.032)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 2fdf4e64-d352-481b-be01-54613d8dad3a))
  (fp_line (start 6.35 2.032) (end 6.35 4.953)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 5521e0e9-1e99-46f8-9f28-cb5b9368b50e))
  (fp_rect (start -7.366 -4.699) (end 7.366 4.953)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 2703f9cc-06a9-4a47-988f-257745861531))
  (pad "1" thru_hole oval (at -5.08 0) (size 2.6 3.8) (drill 1.4) (layers "*.Cu" "*.Mask") (tstamp d0334a59-e536-4a2f-8d3a-b98e72401932))
  (pad "2" thru_hole oval (at 0 0) (size 2.6 3.8) (drill 1.4) (layers "*.Cu" "*.Mask") (tstamp c41023f7-1589-491f-b0cc-2024db498f94))
  (pad "3" thru_hole oval (at 5.08 0) (size 2.6 3.8) (drill 1.4) (layers "*.Cu" "*.Mask") (tstamp 830b8371-674c-41a9-a003-6058ad68d379))
  (model "${my_additions}/DG128-5.08-03P-14-1000A(H).step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
