(footprint "TO-220-3_Horizontal_TabUp_BigHole" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
  (tags "TO-220-3 Horizontal RM 2.54mm")
  (attr through_hole)
  (fp_text reference "REF**" (at 2.54 20.58) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3e74c4ac-d8e4-442e-b651-ed8f42c18567)
  )
  (fp_text value "TO-220-3_Horizontal_TabUp_BigHole" (at 2.54 -2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bfb72d85-0609-436b-a8e4-f25a44c2d30b)
  )
  (fp_text user "${REFERENCE}" (at 2.54 20.58) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 84eb3829-960c-4fdc-99aa-4ee55d684206)
  )
  (fp_line (start -2.58 3.69) (end -2.58 13.18)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1c6e4ed9-987a-4064-9b0a-d8afcfbf16d8))
  (fp_line (start -2.58 3.69) (end 7.66 3.69)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a7e58aa7-6b8d-4285-9a45-ef112365eb87))
  (fp_line (start -2.58 13.18) (end 7.66 13.18)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5d28ee72-2aae-401f-bb92-1f75c0145a85))
  (fp_line (start -2.58 13.42) (end -2.58 14.62)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c67dd297-ba34-4289-92f0-30c4894ce7c5))
  (fp_line (start -2.58 15.82) (end -2.58 17.02)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9ebec0ba-5d01-47b8-a75f-a2ea30d65d18))
  (fp_line (start -2.58 18.22) (end -2.58 19.42)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 06cd93b2-41e1-4e77-a414-ac0983b63891))
  (fp_line (start -2.58 19.58) (end -1.38 19.58)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp da474bbd-a08a-4bff-bc15-acab7c59e984))
  (fp_line (start -0.181 19.58) (end 1.02 19.58)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d579c66c-0d56-4bae-88e6-d1d9222979e7))
  (fp_line (start 0 1.15) (end 0 3.69)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5c03bfa7-5f04-4a5d-82f1-8609cd3836c1))
  (fp_line (start 2.54 1.15) (end 2.54 3.69)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0afdd74f-de2f-494e-ab68-44b6e89beecd))
  (fp_line (start 4.62 19.58) (end 5.82 19.58)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4f4c4974-255f-4f4d-8d31-140801aa7ff7))
  (fp_line (start 5.08 1.15) (end 5.08 3.69)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a4486e7f-4062-41fa-a6d0-b724d7c4dea0))
  (fp_line (start 7.02 19.58) (end 7.66 19.58)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b9ec9391-3a6f-4a79-823e-b46624d1837e))
  (fp_line (start 7.66 3.69) (end 7.66 13.18)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 532a8f20-42dd-48b1-a79f-69db43aee85a))
  (fp_line (start 7.66 13.42) (end 7.66 14.62)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8d3efc05-7368-40a3-986f-ba75bda70f85))
  (fp_line (start 7.66 15.82) (end 7.66 17.02)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d1909c51-5d6c-4c76-8a26-fff0c51200a7))
  (fp_line (start 7.66 18.22) (end 7.66 19.42)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 49c2df0b-c98f-4594-aa31-2a502ed5fa16))
  (fp_line (start -2.71 -1.25) (end -2.71 19.71)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dd5a8caa-4a25-470c-beb5-606b0663e60b))
  (fp_line (start -2.71 19.71) (end 7.79 19.71)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 901e70ed-2885-4bef-a830-98287c75a952))
  (fp_line (start 7.79 -1.25) (end -2.71 -1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d9e1ba9b-c1f7-4040-989b-54f74d10ad14))
  (fp_line (start 7.79 19.71) (end 7.79 -1.25)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ad7f117d-9ba0-4c06-b93e-bfb5d5d8fa19))
  (fp_line (start -2.46 3.81) (end -2.46 13.06)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2e19ad08-9633-4444-8357-6747b499af29))
  (fp_line (start -2.46 13.06) (end -2.46 19.46)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 937d8b9c-ce24-4a54-b5ec-563202d36147))
  (fp_line (start -2.46 13.06) (end 7.54 13.06)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a23e131d-7443-4eda-8f16-13ac2dfb12c8))
  (fp_line (start -2.46 19.46) (end 7.54 19.46)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9dfd0362-c8d3-4a12-ac3c-3b6bf1353bb2))
  (fp_line (start 0 3.81) (end 0 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a5731f85-b313-40c9-9474-eaa3614b9057))
  (fp_line (start 2.54 3.81) (end 2.54 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bdbd70ba-96a5-4c96-8969-a9c7000a2271))
  (fp_line (start 5.08 3.81) (end 5.08 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f8b15e66-30ba-47f1-9f86-20dace263729))
  (fp_line (start 7.54 3.81) (end -2.46 3.81)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6f97d451-ef9a-4444-90b2-8307fe2974d5))
  (fp_line (start 7.54 13.06) (end -2.46 13.06)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f77f1488-41f3-4055-8805-3f9edf7aa092))
  (fp_line (start 7.54 13.06) (end 7.54 3.81)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4875dd58-47b3-403a-84cd-c641d5d3cdaf))
  (fp_line (start 7.54 19.46) (end 7.54 13.06)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1e921ca4-d316-4855-838d-ec62f16a427a))
  (fp_circle (center 2.54 16.66) (end 4.39 16.66)
    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp f0a37f73-70c7-4e25-adaa-b0161b7d68ed))
  (pad "" np_thru_hole oval (at 2.54 16.66) (size 6 6) (drill 6) (layers "F&B.Cu" "*.Mask") (tstamp 388034ca-8b76-48c2-9f60-4140367c75c2))
  (pad "1" thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp 3df413da-64eb-4ec6-8a0d-403967777249))
  (pad "2" thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp 27701952-d3b2-4a2e-883e-02062b0b688e))
  (pad "3" thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask") (tstamp eca9fd38-9363-4a69-a047-6b34b28525ed))
  (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabUp.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
