(footprint "ESP-01_proper"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Wi-Fi Module, https://docs.ai-thinker.com/_media/esp8266/esp8266_series_modules_user_manual_en.pdf")
	(tags "Wi-Fi Module")
	(property "Reference" "REF**"
		(at 3.8 -10.2 0)
		(layer "F.SilkS")
		(uuid "d8effc85-5684-4466-8535-a99f82591335")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "ESP-01_proper"
		(at 3.7 -19 0)
		(layer "F.Fab")
		(uuid "6ffd1dab-5bab-4aa1-96a9-4ab576ada2b3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "2e63a0bf-3b8c-4d73-9a0a-9e901a403478")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "757c17aa-3ded-4ed5-876f-63f43c1be221")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "1c658b4b-0150-4ed8-8493-ad84e7cfc671")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_rect
		(start -3.61 -20.77)
		(end 11.01 4.15)
		(stroke
			(width 0.12)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "a0af32bf-69e2-41bf-9381-c72df5627f57")
	)
	(fp_rect
		(start -1.3 -1.3)
		(end 9.02 3.84)
		(stroke
			(width 0.12)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "623187d2-2f8c-4776-abac-c60cd51a932c")
	)
	(fp_poly
		(pts
			(xy -0.480921 -2.449755) (xy 0.519079 -2.449755) (xy 0.019079 -1.449755)
		)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "aebc66f5-f481-466d-a00d-f3acd30f2fe2")
	)
	(fp_rect
		(start -3.75 -20.91)
		(end 11.15 4.29)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "327597de-7052-49e0-8c10-8573a6444a80")
	)
	(fp_line
		(start -3.5 -0.96)
		(end -3.5 0.87)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "5d4fe3d7-3be4-4b37-94b3-d71cd05d55fe")
	)
	(fp_line
		(start -1.56 0.03)
		(end -3.5 -0.96)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "3a343de0-3a81-4549-b63d-00a0550be98f")
	)
	(fp_line
		(start -1.56 0.03)
		(end -3.5 0.87)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "b46dae9f-3633-4c93-b23e-62d2fbf93b7a")
	)
	(fp_rect
		(start -3.5 -20.66)
		(end 10.9 4.04)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "cb5e3626-80eb-4434-9838-786c086abb42")
	)
	(fp_text user "${REFERENCE}"
		(at 3.7 -11.8 0)
		(layer "F.Fab")
		(uuid "a2c9e3fb-eee8-454a-a997-836484989193")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1470588235)
		(uuid "5852532e-84b3-44b9-bc38-11e16151ee3f")
	)
	(pad "2" thru_hole circle
		(at 0 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "909402fa-089b-4f6b-8cbc-915b46d40474")
	)
	(pad "3" thru_hole circle
		(at 2.54 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f8ba2933-fe7f-48fb-8bc1-4f6fd6f8eb1d")
	)
	(pad "4" thru_hole circle
		(at 2.54 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5cb99055-8d4a-4873-beb3-42ba3680623c")
	)
	(pad "5" thru_hole circle
		(at 5.08 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "fdfff63f-7cd4-4078-afd6-2f667fef81f1")
	)
	(pad "6" thru_hole circle
		(at 5.08 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e76ed5b2-0159-44ba-8701-e97082e5805d")
	)
	(pad "7" thru_hole circle
		(at 7.62 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "bf6c95f2-5042-4005-bf68-9098e207f1ed")
	)
	(pad "8" thru_hole circle
		(at 7.62 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1e9cae4a-3d4d-48c7-bdaa-7fd14a701858")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "*.Cu")
		(uuid "9e0b8615-afdf-416b-90a8-5814408a416e")
		(name "No Copper")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -3.475 -20.625) (xy 10.85 -20.6) (xy 10.825 -13.975) (xy -3.5 -14)
			)
		)
	)
	(model "${my_additions}/ESP-01S_PBD-8.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
