(footprint "Mini_Blade_Fuse_Holder" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Mini blade fuse holder")
  (tags "fuse, holder, mini, automotive, auto")
  (attr through_hole)
  (fp_text reference "REF**" (at -7.7 -3.6) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 17b3d72d-aa02-4ade-925d-2e0ef0b78959)
  )
  (fp_text value "Mini_Blade_Fuse_Holder" (at 0 2.7 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 67d63c0b-fa7b-4a64-a1c6-e1f175a626bc)
  )
  (fp_text user "${REFERENCE}" (at 0 -0.6 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 92e4ef00-add5-4014-831a-95b5a0882188)
  )
  (fp_rect (start -7.5 -2.85) (end 7.5 2.15)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp 8681f8ed-0b19-4962-866d-dcdb1e3638f9))
  (fp_rect (start -7.4 -2.75) (end 7.4 2.05)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp e299f74a-cc04-4804-a766-9e45b2b4142c))
  (fp_rect (start -7.3 -2.65) (end 7.3 1.95)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp fc004ba5-8051-4050-83b7-48fe39f0d72d))
  (pad "1" thru_hole oval (at -5.85 0) (size 1.7 3.4) (drill oval 0.5 2.2) (layers "*.Cu" "*.Mask") (tstamp f085ede4-adbf-4633-8c02-7729c33eaf29))
  (pad "1" thru_hole oval (at -2.15 0) (size 1.7 3.4) (drill oval 0.5 2.2) (layers "*.Cu" "*.Mask") (tstamp e0b7a3b3-7c2c-45f9-a4fe-57a6e07d3b31))
  (pad "2" thru_hole oval (at 2.15 0) (size 1.7 3.4) (drill oval 0.5 2.2) (layers "*.Cu" "*.Mask") (tstamp 49be6fd9-6aac-4baf-8d0d-0469796c59c0))
  (pad "2" thru_hole oval (at 5.85 0) (size 1.7 3.4) (drill oval 0.5 2.2) (layers "*.Cu" "*.Mask") (tstamp b431d4a4-f2af-446d-a417-8fa050c87306))
  (model "${my_additions}/Mini_Blade_Fuse_Holder.step"
    (offset (xyz 0 -2 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
