(footprint "KLS5-CR2032-01" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "KLS5-CR2032-01, BH-642, CH224-2032. CR2032 battery cell holder")
  (tags "battery, holder, cr2032")
  (attr through_hole)
  (fp_text reference "REF**" (at 10.5 -4.8) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 7a06462d-0b42-4640-8b7b-dde240ed33bd)
  )
  (fp_text value "KLS5-CR2032-01" (at 0 3.3) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 0a741ecf-60e8-4f00-ae34-c4408124b997)
  )
  (fp_text user "+" (at 10.7 3.4 unlocked) (layer "F.SilkS")
      (effects (font (size 2 2) (thickness 0.25) bold) (justify left bottom))
    (tstamp 0b68a9a5-0f90-4157-b063-5b832d9fba5b)
  )
  (fp_text user "+" (at 9 0.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.25) bold) (justify left bottom))
    (tstamp 50d5a671-ff43-4052-908f-bc94ad4bcc93)
  )
  (fp_text user "${REFERENCE}" (at 0 -1.6) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a9b827e4-3664-4f8d-af52-35e48c22f99e)
  )
  (fp_line (start 10.499999 -3.9) (end 13.4 -3.9)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 81080e87-c287-4162-b92f-5cd53eaeb114))
  (fp_line (start 13.4 -3.9) (end 13.4 3.9)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp dab1a89e-ba66-4d30-8d24-226faf259c1a))
  (fp_line (start 13.4 3.9) (end 10.499999 3.9)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 9c092500-109c-490f-aeac-ee6bf61efa86))
  (fp_arc (start 10.499999 3.9) (mid -11.20089 0) (end 10.499999 -3.9)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 970c8a9b-1f3c-4b82-a05b-120804cd9ac9))
  (fp_line (start 10.4 -3.8) (end 13.3 -3.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp f2763410-6c46-47be-8a19-493f30ecb2ab))
  (fp_line (start 13.3 -3.8) (end 13.3 3.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp c131a590-b684-4631-b9e4-03de89034ca2))
  (fp_line (start 13.3 3.8) (end 10.4 3.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp ed51486a-ee4c-4b0b-882f-aed76932f904))
  (fp_arc (start 10.4 3.8) (mid -11.072488 0) (end 10.4 -3.8)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 078b3f14-1f61-4dfd-b421-a3735145b7bb))
  (fp_line (start 13.25 -3.75) (end 10.4 -3.75)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp d09faec6-34ba-4484-821a-4c00bc0ed635))
  (fp_line (start 13.25 -3.75) (end 13.25 3.75)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 42c7957a-4dff-4e43-9f54-72686861bbed))
  (fp_line (start 13.25 3.75) (end 10.4 3.75)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 993157ba-3e92-4d59-8775-ba45658f3579))
  (fp_circle (center 0 0) (end 11.05 0)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp f42ebe5d-535d-44e3-aad8-aef766bdecb2))
  (pad "1" thru_hole circle (at 12 0) (size 2.5 2.5) (drill 1.3) (layers "*.Cu" "*.Mask") (tstamp 58eacb1a-65e7-4009-a01d-8b86d02caf1b))
  (pad "2" thru_hole circle (at -8 0) (size 2.5 2.5) (drill 1.3) (layers "*.Cu" "*.Mask") (tstamp 7e503268-ae11-4a7d-97c4-96243cc0b555))
  (model "${my_additions}/KLS5-CR2032-01.stp"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 180))
  )
)
