(footprint "18650_double_holder_SMT" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Double 18650 battery holder")
  (tags "battery, holder, 18650")
  (attr smd)
  (fp_text reference "REF**" (at -38.9 -21.1) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp b3b6ef52-0361-4aba-9c98-cc83c1aae260)
  )
  (fp_text value "18650_double_holder_SMT" (at 0 1.9) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 015ecf8d-0d41-4942-b05c-9052745518d5)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ff4e5074-6d09-49dd-bda3-7c2f199d22e2)
  )
  (fp_line (start -38.6 -20.1) (end -38.6 -13)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 36f6d6f6-c0b7-49f7-be85-bb12f738965b))
  (fp_line (start -38.6 -6.1) (end -38.6 6.1)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 6a4eb3ad-1ecd-44d0-8913-9be28acfc17a))
  (fp_line (start -38.6 20.1) (end -38.6 13)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 83ed7f61-7930-40ae-8b4e-865bb62beffb))
  (fp_line (start 38.6 -20.1) (end -38.6 -20.1)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp c6918153-7cc6-4879-a604-f9c92e9a7013))
  (fp_line (start 38.6 -13) (end 38.6 -20.1)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp b52f50a4-df3f-483b-a9ec-e4252ec0e2ad))
  (fp_line (start 38.6 6.1) (end 38.6 -6.1)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp c6f0fb4b-e51e-473a-b401-1a77bb4b2c56))
  (fp_line (start 38.6 20.1) (end -38.6 20.1)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp a519c515-e45d-4c55-933d-4826083be1a3))
  (fp_line (start 38.6 20.1) (end 38.6 13)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 7f4ca586-5df8-4b8c-a9b0-99221ccdcb1f))
  (fp_rect (start -38.5 -20) (end 38.5 20)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.CrtYd") (tstamp 25ebb8a1-b118-48c8-8857-885998df7fae))
  (fp_line (start -38.4 -5.7) (end 38.4 -5.7)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 8cdccb6c-54d1-4424-abe4-ccfb9901c532))
  (fp_line (start -38.4 13.4) (end 38.4 13.4)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp cb7ecc0a-986a-4d1f-8488-bf836a36ae5c))
  (fp_line (start 38.4 -13.4) (end -38.4 -13.4)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 3223cc2f-483b-4aee-b7ae-2b11e1c253bc))
  (fp_line (start 38.4 5.7) (end -38.4 5.7)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp aa2f2e2e-30a7-42c0-9658-3963291bbcd2))
  (fp_rect (start -38.4 -19.9) (end 38.4 19.9)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp aebd283c-9645-407c-ab2d-2b9d2acce569))
  (pad "" np_thru_hole circle (at -27.6 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp 6b8c6349-9ec7-4baa-b6de-f5035c7db794))
  (pad "" np_thru_hole circle (at 27.6 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp 6b7988b1-4699-4e8f-aa14-f64a0c3008e3))
  (pad "" np_thru_hole circle (at 35.82 17.505) (size 2.4 2.4) (drill 2.4) (layers "F&B.Cu" "*.Mask") (tstamp cc4ddadb-d7a2-4e2e-915b-c2d36ec9b020))
  (pad "1" smd rect (at 39.83 9.555) (size 8.34 6.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp e10e4f01-cb1e-4994-9db3-a484753f1bb8))
  (pad "2" smd rect (at -39.83 9.555) (size 8.34 6.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 106a7d8b-fb69-42d3-b720-18a3af58c83b))
  (pad "3" smd rect (at -39.83 -9.555) (size 8.34 6.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp d039db73-dae7-46ad-93c0-1cbf049fb1fc))
  (pad "4" smd rect (at 39.83 -9.555) (size 8.34 6.35) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp b97c3835-f508-4e8f-85c1-bc50a540bcd5))
  (model "${my_additions}/18650_double_holder_SMT.STEP"
    (offset (xyz 0 0 7.4))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
