(footprint "NRF24L01_SMD_Breakout"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -3.175 -1.905 90)
		(layer "F.SilkS")
		(uuid "a7785c7d-17e6-4bd8-8b22-3a4f028535d4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "NRF24L01_SMD_Breakout"
		(at 4.445 -19.05 0)
		(layer "F.Fab")
		(uuid "de0ba54f-2cdf-4fb0-a32e-edee07fba029")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at -18.415 32.425 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e9e10c10-8d5b-4e95-8e27-4c06d80ee013")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at -18.415 32.425 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4c6ba108-b1cd-4ac2-8723-040166c8de3d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at -18.415 32.425 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "cb47fd5a-7f6e-4461-b489-625b96544a00")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.905 0)
		(end -1.905 -10.795)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "742356ca-c2f0-428f-b810-fc12fdba68e3")
	)
	(fp_line
		(start -0.835 0)
		(end -1.905 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3478fc46-cfe7-4f9a-9be5-03f7fbda2ca9")
	)
	(fp_line
		(start 9.725 0)
		(end 10.795 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "88ea4b79-5fc4-4181-a28d-dab0b9271df9")
	)
	(fp_line
		(start 10.795 0)
		(end 10.795 -10.795)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "943bf883-21ad-47de-baac-c26df2e04b9e")
	)
	(fp_rect
		(start -1.6 -18)
		(end 10.4 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "2d545c18-a573-4636-9c27-11f712afb152")
	)
	(fp_line
		(start -1.6 -11.5)
		(end 10.4 -11.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "66103c1e-be0f-4690-a562-0bb76b54bfc9")
	)
	(fp_line
		(start -0.635 -17.145)
		(end 0.635 -17.145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "aa1073cb-11bf-40ce-84b5-f8624e966208")
	)
	(fp_line
		(start -0.635 -12.065)
		(end -0.635 -17.145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "d6587424-16a3-493f-9c36-04d141b387fb")
	)
	(fp_line
		(start 0.635 -17.145)
		(end 0.635 -13.97)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "26734136-1ed2-49f7-a0e7-1940ae00c813")
	)
	(fp_line
		(start 0.635 -13.97)
		(end 1.905 -13.97)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "0d05a942-bde5-4e20-ae34-dbda26f6113b")
	)
	(fp_line
		(start 1.905 -17.145)
		(end 3.175 -17.145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "a3ab2aea-c583-422a-8b28-88478ef3153e")
	)
	(fp_line
		(start 1.905 -13.97)
		(end 1.905 -17.145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "65ef5dd3-c7df-4b94-9692-b3c97c1fc47c")
	)
	(fp_line
		(start 3.175 -17.145)
		(end 3.175 -13.97)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "2f5e6f65-7ee2-416b-ae93-70c13e1157cc")
	)
	(fp_line
		(start 3.175 -13.97)
		(end 4.445 -13.97)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "ac9de6d9-ce01-400c-8437-be854a147476")
	)
	(fp_line
		(start 4.445 -17.145)
		(end 5.715 -17.145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "6404f2ec-816a-443a-b428-9c28ec07eace")
	)
	(fp_line
		(start 4.445 -13.97)
		(end 4.445 -17.145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "3a4c1034-1638-4b51-821b-690de0601433")
	)
	(fp_line
		(start 5.715 -17.145)
		(end 5.715 -13.97)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "5bcbb33a-0d31-4254-b874-50af284b460b")
	)
	(fp_line
		(start 5.715 -13.97)
		(end 6.985 -13.97)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "5117aa2c-8f2b-4c08-ae14-34b76c598128")
	)
	(fp_line
		(start 6.985 -17.145)
		(end 9.525 -17.145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "5e599660-1f21-4691-836c-b20753584425")
	)
	(fp_line
		(start 6.985 -13.97)
		(end 6.985 -17.145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "3230a3ef-1a1a-4316-81fb-8a08523cb993")
	)
	(fp_rect
		(start -1.6 -18)
		(end 10.4 0)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "d6ebbbcb-8a9f-4d45-b3a1-600bc3c96b0c")
	)
	(fp_text user "${REFERENCE}"
		(at 4.445 -6.35 0)
		(layer "F.Fab")
		(uuid "0afcc648-f871-411e-89ed-b654b23f1807")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at 1.27 -0.4)
		(size 0.9 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "e6f22f37-4636-42f5-bf6a-ac327fcc79e3")
	)
	(pad "2" smd rect
		(at 0 -0.4)
		(size 0.9 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "77fb9082-7be6-4ce4-b0be-f2c67528dd28")
	)
	(pad "3" smd rect
		(at 2.54 -0.4)
		(size 0.9 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "693269f7-9d4c-41e7-af1c-5ad4ac18f670")
	)
	(pad "4" smd rect
		(at 3.81 -0.4)
		(size 0.9 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "a028292b-8d82-4149-9597-2deafbb27bf8")
	)
	(pad "5" smd rect
		(at 5.08 -0.4)
		(size 0.9 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "20c43249-bf3e-4309-8342-10c3389b5764")
	)
	(pad "6" smd rect
		(at 6.35 -0.4)
		(size 0.9 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "ab4a0c60-d66e-4d8f-9b96-f91a6662b3b0")
	)
	(pad "7" smd rect
		(at 7.62 -0.4)
		(size 0.9 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "265cd175-0f5d-4f26-9a7c-7bc4233776e8")
	)
	(pad "8" smd rect
		(at 8.89 -0.4)
		(size 0.9 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
		(uuid "f61beebc-386b-4aad-800f-7cb7fdbaae3c")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "*.Cu")
		(uuid "0d37ea73-c5bb-4ad7-adda-78fadfc227aa")
		(name "Antenna_keepout")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -1.9 -11.5) (xy -1.9 -18.3) (xy 10.7 -18.3) (xy 10.7 -11.5)
			)
		)
	)
	(model "${my_additions}/nRF24L01_SMD.stp"
		(offset
			(xyz 4.4 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
