(footprint "BH-10_PCB_edge" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at -7.4 -2.3 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6678c034-451b-4fb8-b12d-9e7a8f78f8d8)
  )
  (fp_text value "BH-10_PCB_edge" (at -0.1 1.3) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7052b3aa-9c43-4b25-b762-970073c129a2)
  )
  (fp_text user "PCB Edge" (at 8 0 unlocked) (layer "Cmts.User")
      (effects (font (size 0.5 0.5) (thickness 0.1)) (justify left))
    (tstamp bcec9e5f-ab3b-4aed-8e7c-d8f2f9298703)
  )
  (fp_text user "${REFERENCE}" (at -0.1 2.8) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 166bff57-3db3-41f2-a968-1f35cab1cd8c)
  )
  (fp_line (start -6.1 -0.2) (end -6.1 -4.5)
    (stroke (width 0.15) (type default)) (layer "B.SilkS") (tstamp 362b74d9-087c-4f3d-86a6-8ab571ea53c0))
  (fp_line (start 6.1 -0.2) (end 6.1 -4.5)
    (stroke (width 0.15) (type default)) (layer "B.SilkS") (tstamp b75ff83d-b7b7-4856-8b57-1f2e9b316c67))
  (fp_line (start -6.1 -0.2) (end -6.1 -4.5)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 5d0cac70-bff0-4482-ad06-e0243e9d2db1))
  (fp_line (start 6.1 -4.5) (end 5.6 -4.5)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp b7abe3ab-24b5-4f61-a90c-ed554f8214a3))
  (fp_line (start 6.1 -0.2) (end 6.1 -4.5)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 5e3783a1-2906-4c67-ad2c-6b1a08bf56cc))
  (fp_poly
    (pts
      (xy 6.3 -0.8)
      (xy 6.9 -0.4)
      (xy 6.9 -1.2)
    )

    (stroke (width 0.1) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 322b4f80-c3f4-42b8-9527-c927397522c7))
  (fp_line (start 8 0) (end -8 0)
    (stroke (width 0.1) (type default)) (layer "Cmts.User") (tstamp f3d38e1f-5ad5-48ea-bc51-94521f131d2a))
  (fp_rect (start -10.15 0.1) (end 10.15 9.1)
    (stroke (width 0.05) (type default)) (fill none) (layer "B.CrtYd") (tstamp 56b73cc6-ace5-44ba-8f42-51ae9428cc93))
  (fp_rect (start -10.15 0.1) (end 10.15 9.1)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp e3cfa804-632c-43d6-8d2a-ee30da28748d))
  (fp_rect (start -10 0.1) (end 10 9)
    (stroke (width 0.1) (type default)) (fill none) (layer "B.Fab") (tstamp 1d5c98b3-6e64-48d5-9b7e-07bb6df87f5d))
  (fp_rect (start -5.4 -2.9) (end -4.8 0.1)
    (stroke (width 0.1) (type solid)) (fill solid) (layer "B.Fab") (tstamp e36c0686-78e2-47eb-8371-0bd870956666))
  (fp_rect (start -2.9 -2.9) (end -2.3 0.1)
    (stroke (width 0.1) (type solid)) (fill solid) (layer "B.Fab") (tstamp 2c04ce84-1900-4977-9b0c-d438a50fe7c0))
  (fp_rect (start -0.3 -2.9) (end 0.3 0.1)
    (stroke (width 0.1) (type solid)) (fill solid) (layer "B.Fab") (tstamp ea773064-0a11-4644-b952-a4b021947814))
  (fp_rect (start 2.2 -2.9) (end 2.8 0.1)
    (stroke (width 0.1) (type solid)) (fill solid) (layer "B.Fab") (tstamp 06e60699-855d-4fe4-a21b-cb16a0e31e96))
  (fp_rect (start 4.8 -2.9) (end 5.4 0.1)
    (stroke (width 0.1) (type solid)) (fill solid) (layer "B.Fab") (tstamp 39e8f14e-b669-457a-80c2-89c4d2a819f8))
  (fp_line (start -1.3 0.1) (end -1.3 9)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp b7998752-b511-4ca4-bb0f-403bbf00806c))
  (fp_line (start 1.3 0.1) (end 1.3 9)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp d3893853-4e31-4259-8b1b-147ba4b7fc14))
  (fp_rect (start -10 0.1) (end 10 9)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 89f53474-e6a6-4b5e-a668-73b623e8133c))
  (fp_rect (start -5.4 -2.9) (end -4.8 0.1)
    (stroke (width 0.1) (type solid)) (fill solid) (layer "F.Fab") (tstamp 4360d604-2a94-4253-bb1a-61b9ef7c56c6))
  (fp_rect (start -2.9 -2.9) (end -2.3 0.1)
    (stroke (width 0.1) (type solid)) (fill solid) (layer "F.Fab") (tstamp 7ce3db90-9c54-45eb-9184-bcbe53c10ea3))
  (fp_rect (start -0.3 -2.9) (end 0.3 0.1)
    (stroke (width 0.1) (type solid)) (fill solid) (layer "F.Fab") (tstamp 8f26b550-fbc0-44f1-b046-3ffcf6e7783e))
  (fp_rect (start 2.2 -2.9) (end 2.8 0.1)
    (stroke (width 0.1) (type solid)) (fill solid) (layer "F.Fab") (tstamp 160bed38-5a4b-47d4-b35a-35fc650e646f))
  (fp_rect (start 4.8 -2.9) (end 5.4 0.1)
    (stroke (width 0.1) (type solid)) (fill solid) (layer "F.Fab") (tstamp 4de3acef-7ca6-4d55-a563-a9da8b6c85e7))
  (pad "1" smd rect (at 5.08 -2.2) (size 1 4) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 8cbe8714-3e10-4473-bad6-635c5b9aa24c))
  (pad "2" smd rect (at 5.08 -2.2) (size 1 4) (layers "B.Cu" "B.Paste" "B.Mask") (tstamp 1ab3fd4e-f9c3-464c-ae24-821463d9d464))
  (pad "3" smd rect (at 2.54 -2.2) (size 1 4) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp b64b5c3d-df53-4e58-ad79-37da8e08a55e))
  (pad "4" smd rect (at 2.54 -2.2) (size 1 4) (layers "B.Cu" "B.Paste" "B.Mask") (tstamp 35311681-c978-458d-a86f-72222c884a82))
  (pad "5" smd rect (at 0 -2.2) (size 1 4) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 8e0c7a3f-7a02-4f84-95fc-8e9208efac22))
  (pad "6" smd rect (at 0 -2.2) (size 1 4) (layers "B.Cu" "B.Paste" "B.Mask") (tstamp 8222bf90-e7de-422f-8532-5f5c6e777600))
  (pad "7" smd rect (at -2.54 -2.2) (size 1 4) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp da3f493c-b912-4d0b-94fc-3847bc722850))
  (pad "8" smd rect (at -2.54 -2.2) (size 1 4) (layers "B.Cu" "B.Paste" "B.Mask") (tstamp 4e758f16-b0dd-4e56-885c-c16cb0d137b8))
  (pad "9" smd rect (at -5.08 -2.2) (size 1 4) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp fad8b438-3def-40f6-8c7a-5e99feaf9707))
  (pad "10" smd rect (at -5.08 -2.2) (size 1 4) (layers "B.Cu" "B.Paste" "B.Mask") (tstamp cc00d0e2-bb57-4884-aed5-a640954ad59a))
  (model "${KICAD7_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x05_P2.54mm_Vertical.step"
    (offset (xyz 5.08 0 0.46))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 -90 90))
  )
)
