(footprint "Cherry_MX__no_pins" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Cherry MX mechanical switch")
  (tags "cherry MX mechanical switch")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -7.8) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 0839d5ba-9bca-45a5-8d67-30596555217a)
  )
  (fp_text value "Cherry_MX__no_pins" (at 0 5.8) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2be6c60c-3ba7-46f2-ac47-20d9d48be69d)
  )
  (fp_text user "${REFERENCE}" (at -0.1 4.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 36665e41-9bcb-4b61-a20b-b76ccfed3353)
  )
  (fp_rect (start -7.1 -7.1) (end 7.1 7.1)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp aa8af213-21ab-4ec2-b70a-a143ea8d7cb8))
  (fp_rect (start -7 -7) (end 7 7)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.CrtYd") (tstamp 2c7e5ed8-2a3a-4678-b9ab-9f88df9e9e40))
  (fp_rect (start -7.1 -7.1) (end 7.1 7.1)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp fddde8ca-8467-498a-aa09-5074d5e36b73))
  (fp_circle (center 0 0) (end 2.2 0)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 2c87b15d-ad28-45da-8122-d486912f2dfe))
  (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers "F&B.Cu" "*.Mask") (tstamp 7818c84c-c76e-475b-8fdc-a5a133581fc9))
  (pad "1" thru_hole circle (at -3.81 -2.54) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask") (tstamp 7a5f26d6-0316-4cb9-998a-2e9eb042ce1b))
  (pad "2" thru_hole circle (at 2.54 -5.08) (size 2.5 2.5) (drill 1.5) (layers "*.Cu" "*.Mask") (tstamp 2de927a0-0ffe-4308-a07b-8c8db7e47c91))
  (model "${my_additions}/cherry_mx_blue_PLATE.step"
    (offset (xyz 0.3 0.3 5.5))
    (scale (xyz 1 1 1))
    (rotate (xyz 180 0 90))
  )
)
