(footprint "L_06030" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "SMD Inductor MHCC, MHCI series")
  (tags "MHCC, MHCI, 06030, inductor")
  (attr smd)
  (fp_text reference "REF**" (at -3.6 -4.1 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp c0559723-9555-4b9d-a8d2-c70b846cceb1)
  )
  (fp_text value "L_06030" (at 0 4.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9c2df3ed-6ee0-4c63-bae8-dc47f158c257)
  )
  (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 33e7d3ef-bc39-44d0-8ec0-a3d5a0d5bae3)
  )
  (fp_line (start -3.4 -3.4) (end 3.4 -3.4)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 2277db75-11c1-4f93-ba35-3b1eef471ddc))
  (fp_line (start -3.4 -1.9) (end -3.4 -3.4)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 2047b62d-622c-4039-a7f5-69aeb18c1291))
  (fp_line (start -3.4 3.4) (end -3.4 1.9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp eccb3f3c-8591-4dc6-8312-0b5064651959))
  (fp_line (start 3.4 -3.4) (end 3.4 -1.9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 9ecf9cc0-f5ec-4557-a34b-231a46378fa6))
  (fp_line (start 3.4 1.9) (end 3.4 3.4)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 16fafd3e-de93-450b-bb4d-a8c0c1aed308))
  (fp_line (start 3.4 3.4) (end -3.4 3.4)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 8bf55bd7-0619-4229-9c6a-299b4cf67c5a))
  (fp_rect (start -3.65 -3.4) (end 3.65 3.4)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.CrtYd") (tstamp e3308254-13ce-4ad7-b4ef-907eee241aed))
  (fp_rect (start -3.3 -3.3) (end 3.3 3.3)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 4c791bf4-87a3-4575-8916-977e7f088611))
  (pad "1" smd roundrect (at -3.175 0) (size 2.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp aa6f421b-e071-4fab-8009-263670a732c1))
  (pad "2" smd roundrect (at 3.175 0) (size 2.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (thermal_bridge_angle 45) (tstamp 976f077d-fdcb-4455-af10-d43bc761dc04))
  (model "${my_additions}/Inductor_SMD_AMPLF_0630.STEP"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 90))
  )
)
