(footprint "Tactile_switch_3x4x2mm-2Pad" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Small SMD tactile 3x4mm button")
  (tags "SMD tactile button switch")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.3) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ea6afd9d-fa23-4bcf-ad60-5d1004f7b106)
  )
  (fp_text value "Tactile_switch_3x4x2mm-2Pad" (at 0 2.5 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5d2ee62d-0c4f-4b67-8f42-681a4f1abb2b)
  )
  (fp_text user "${REFERENCE}" (at 0 4) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e1521779-4618-4863-9f8d-1c3f1b943b90)
  )
  (fp_line (start -2.1 -1.6) (end -2.1 -0.9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 583aadcb-f79c-45b1-88d1-b99a79adb212))
  (fp_line (start -2.1 0.9) (end -2.1 1.6)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 43b41bdb-a30e-4b96-a499-e8e9b34d843c))
  (fp_line (start -2.1 1.6) (end 2.1 1.6)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 075de177-491f-4264-884f-7ece8e6648fa))
  (fp_line (start 2.1 -1.6) (end -2.1 -1.6)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 08fdfb98-f207-4fe4-a77e-6f5054ded8fd))
  (fp_line (start 2.1 -0.9) (end 2.1 -1.6)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 890ccdfb-148d-41a4-999e-5fef427c60e7))
  (fp_line (start 2.1 1.6) (end 2.1 0.9)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp e874c21b-0c6e-46b8-a60b-973c3cf26343))
  (fp_circle (center 0 0) (end 0.9 0)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp 594982d3-5e0b-4281-a225-42d009017ba4))
  (fp_rect (start -2 -1.5) (end 2 1.5)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.CrtYd") (tstamp fdbf1f44-d652-41be-b47e-51ca2ba35c90))
  (fp_rect (start -2.1 -1.6) (end 2.1 1.6)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp cbac564b-e804-4631-88da-91830e02710e))
  (fp_circle (center 0 0) (end 0.9 0)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 9787c24a-ddd8-4137-918d-32e1f2dd4bc3))
  (pad "1" smd rect (at -2.2 0) (size 1.35 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp bb5bbe49-5992-4a91-97a9-b764ed20d545))
  (pad "2" smd rect (at 2.2 0) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 6acf641d-e35d-4c78-a17d-e30876e45fb7))
  (model "${my_additions}/3x4x2mm-2Pad.stp"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
