(footprint "HF32FV-16" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Hongfa HF32FV-16/xx SUBMINIATURE HIGH POWER RELAY")
  (tags "relay, power relay, hongfa")
  (attr through_hole)
  (fp_text reference "REF**" (at -9.7 -6.3) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 8590b739-661a-498a-8af0-204f742606da)
  )
  (fp_text value "HF32FV-16" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 439598d8-86dd-4571-9313-4c624334ee2d)
  )
  (fp_text user "${REFERENCE}" (at 0 -2.54) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 53ca09c6-d425-48bd-b650-82e8fca9c78e)
  )
  (fp_rect (start -9.5 -5.4) (end 9.5 5.4)
    (stroke (width 0.15) (type default)) (fill none) (layer "F.SilkS") (tstamp 52e58547-9ab1-4946-b612-7513d386bf7f))
  (fp_rect (start -9.2 -5.1) (end 9.2 5.1)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp a56d7187-ac10-4957-a463-b56cbda3ec96))
  (fp_rect (start -9.2 -5.1) (end 9.2 5.1)
    (stroke (width 0.15) (type default)) (fill none) (layer "F.Fab") (tstamp b6d05e4d-7350-4fe4-aeaf-36c0ff6968ae))
  (pad "1" thru_hole circle (at -7.62 3.8) (size 2.3 2.3) (drill 1.3) (layers "*.Cu" "*.Mask") (tstamp b73ee053-f7d7-492f-98b7-1426a7a47d1a))
  (pad "2" thru_hole oval (at 5.08 3.45) (size 2.2 3.6) (drill oval 0.8 2) (layers "*.Cu" "*.Mask") (tstamp ba463adf-0cd8-4da7-9495-ec50a27145b2))
  (pad "3" thru_hole oval (at 7.62 -3.45) (size 2.2 3.6) (drill oval 0.8 2) (layers "*.Cu" "*.Mask") (tstamp 14334450-d34f-46cd-ac41-45e53d1ad29b))
  (pad "4" thru_hole circle (at -7.62 -3.8) (size 2.3 2.3) (drill 1.3) (layers "*.Cu" "*.Mask") (tstamp 2dfa5666-f6ec-4cd9-b006-2d2e8fcc2d0a))
  (model "${MY_ADDITIONS}/32FV-16.stp"
    (offset (xyz -32 -6.2 1.7))
    (scale (xyz 1 1 1))
    (rotate (xyz 180 0 0))
  )
)
