(footprint "SS-12D10Lx_slider_switch" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "XKB SS-12D10Lx SPDT Slider switch")
  (tags "sp2t, spdt, slider, switch")
  (attr through_hole)
  (fp_text reference "REF**" (at -6.9 -4.3) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 06883f12-e420-49fa-8e12-062b53d87d50)
  )
  (fp_text value "SS-12D10Lx" (at 0 4.3) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c7d10a78-9410-4642-8c16-ebf3dadc11b8)
  )
  (fp_text user "${REFERENCE}" (at 0 -4.3) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp da55f86b-425e-4a2b-bc00-a147748c768c)
  )
  (fp_rect (start -6.6 -3.5) (end 6.6 3.5)
    (stroke (width 0.15) (type default)) (fill none) (layer "F.SilkS") (tstamp d6d6816b-e45e-4654-a13e-50e189bb7e83))
  (fp_rect (start -6.5 -3.4) (end 6.5 3.4)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 22ad0724-38e6-4c25-9e52-7f4faf12c14a))
  (fp_rect (start -6.4 -3.3) (end 6.4 3.3)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 4f30929a-dde7-4f2a-8d4e-bb9dae64790a))
  (pad "1" thru_hole oval (at -4.7 0) (size 2.9 4.5) (drill oval 0.9 2.5) (layers "*.Cu" "*.Mask") (tstamp 4a7b43c4-f7a3-42cf-8256-a78ad582b01f))
  (pad "2" thru_hole oval (at 0 0) (size 2.9 4.5) (drill oval 0.9 2.5) (layers "*.Cu" "*.Mask") (tstamp 91b216c6-0cec-419f-b817-e81bad319e29))
  (pad "3" thru_hole oval (at 4.7 0) (size 2.9 4.5) (drill oval 0.9 2.5) (layers "*.Cu" "*.Mask") (tstamp b01d86d1-086f-49db-b46f-acbf9458114d))
  (model "${my_additions}/ss-12d10l5.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
