(footprint "USB_Micro-B_4_legs" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "USB-B micro connector with 4 legs")
  (tags "usb, micro")
  (attr smd)
  (fp_text reference "REF**" (at -5.1 -3.7 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9a15aa35-32a0-4587-a302-4e0779d85071)
  )
  (fp_text value "USB_Micro-B_4_legs" (at 0.3 2.7) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fbc680d0-deb9-4753-b150-1773e09f840c)
  )
  (fp_text user "PCB Edge" (at 0 0 unlocked) (layer "Cmts.User")
      (effects (font (size 0.5 0.5) (thickness 0.1) bold))
    (tstamp ebe65df2-7e3c-4e91-9200-c61efb4f4f33)
  )
  (fp_text user "${REFERENCE}" (at 0.3 4.2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bd4d790b-bf5c-4d20-9fab-dfd7b9758f0b)
  )
  (fp_line (start -3.7 -3.2) (end -3.7 -4.6)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp baf12bb0-1db1-4949-b9ef-f6841b8c39f3))
  (fp_line (start -3.7 -0.2) (end -3.7 -1.1)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp a0e8c365-c5cd-4548-a468-d0eecfc7ad75))
  (fp_line (start 3.7 -3.2) (end 3.7 -4.6)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp da3ade9b-9038-44d0-80b0-c99df3fa2cb3))
  (fp_line (start 3.7 -0.2) (end 3.7 -1.1)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 6a731891-be58-4c22-b18b-f3b008ef81f9))
  (fp_poly
    (pts
      (xy -1.3 -6.5)
      (xy -1.1 -6.8)
      (xy -1.5 -6.8)
    )

    (stroke (width 0.1) (type solid)) (fill solid) (layer "F.SilkS") (tstamp efc60539-3bad-4e79-8301-4296920f643f))
  (fp_line (start -4 0) (end 4 0)
    (stroke (width 0.1) (type default)) (layer "Cmts.User") (tstamp 331399cd-b2bc-4549-9ee5-c2ae5007a9d0))
  (fp_rect (start -3.6 -6.9) (end 3.6 1.7)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp c50c5fb9-689f-435b-8720-6c23a2a1c652))
  (fp_line (start -3.6 -6.9) (end -2.6 -6.9)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 626049ee-38ea-4bf5-8cc7-723cef059e6a))
  (fp_line (start -3.6 1.7) (end -3.6 -6.9)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 7d9d534e-fcf7-412a-9734-62c126b09504))
  (fp_line (start -3.6 1.7) (end 3.6 1.7)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp d364ee15-3faf-4ce9-97cd-18ae255c429c))
  (fp_line (start -2.6 -6.9) (end -2.6 -4.9)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 2adf05a7-abc1-4d6c-bbce-9b84ce3fe976))
  (fp_line (start -2.6 -4.9) (end 2.6 -4.9)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp d9d2bda6-22f7-4a85-ba74-3b1710a4d5ab))
  (fp_line (start 2.6 -6.9) (end 2.6 -4.9)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp b3667509-c3a6-46c6-839a-d18a85e05558))
  (fp_line (start 3.6 -6.9) (end 2.6 -6.9)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp ab4fae80-f8a6-4a48-b4ad-610d7101a7d7))
  (fp_line (start 3.6 1.7) (end 3.6 -6.9)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp beceb573-702c-4a66-85d1-d238dff76291))
  (pad "" np_thru_hole circle (at -2 -4.3) (size 0.55 0.55) (drill 0.55) (layers "F&B.Cu" "*.Mask") (tstamp 7e36a1ef-ce28-462c-9223-68a48cd166d1))
  (pad "" np_thru_hole circle (at 2 -4.3) (size 0.55 0.55) (drill 0.55) (layers "F&B.Cu" "*.Mask") (tstamp 745e01ea-f7ef-4a80-bf4b-5e7888a4fbdf))
  (pad "1" smd rect (at -1.3 -5.2) (size 0.4 2.15) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp a63adf9b-d90d-45d4-9693-e1fa8c6ddacf))
  (pad "2" smd rect (at -0.65 -5.2) (size 0.4 2.15) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp d6415638-c587-4ff8-84be-c78c110016c5))
  (pad "3" smd rect (at 0 -5.2) (size 0.4 2.15) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp e2753b1b-4f40-4c90-bd21-3965ed35e8bb))
  (pad "4" smd rect (at 0.65 -5.2) (size 0.4 2.15) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 03685b69-c56b-4189-8a3b-429b49bea9fc))
  (pad "5" smd rect (at 1.3 -5.2) (size 0.4 2.15) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp b3b2b6c4-5dea-443f-9403-481aef5a7ab9))
  (pad "6" thru_hole oval (at -3.6 -5.62) (size 1.1 1.8) (drill oval 0.5 1.2) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp d867b528-1f7e-4dfd-a13e-c5b143767586))
  (pad "6" thru_hole oval (at -3.6 -2.15) (size 1.1 1.8) (drill oval 0.5 1.2) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 8ee0c742-fb56-4fe6-801d-68fa6c06613a))
  (pad "6" smd rect (at -1.5 -1) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 79e5ebf0-648b-4a12-82c4-827d7f3f3a14))
  (pad "6" smd rect (at 1.5 -1) (size 1.1 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp bc253c23-d1f2-43dc-9c8d-177bba1fd778))
  (pad "6" thru_hole oval (at 3.6 -5.62) (size 1.1 1.8) (drill oval 0.5 1.2) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp ee97e94d-f0b3-4347-810d-ecce2af62d14))
  (pad "6" thru_hole oval (at 3.6 -2.15) (size 1.1 1.8) (drill oval 0.5 1.2) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp f6edf306-46c4-4de2-b82b-6e163bf53cc4))
  (model "${my_additions}/USB_B_Micro_U254-051N-4BH806.step"
    (offset (xyz -3.71 -0.57 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
