(footprint "SS12D06-angled" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "SS12D06 slide switch")
  (tags "SS12D06, switch")
  (attr through_hole)
  (fp_text reference "REF**" (at -1.1 11.6 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify right))
    (tstamp 029b5aac-97d9-43aa-8b60-f3d075c83487)
  )
  (fp_text value "SS12D06-angled" (at 0 6.4 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6177f6bf-9e37-44a3-8c57-fe93e5fb0a0d)
  )
  (fp_text user "${REFERENCE}" (at 0 7.9 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b7ba574e-ee22-433a-8ecc-8f807d842161)
  )
  (fp_rect (start -6.5 4) (end 6.5 10.7)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp 1b1d74bc-a88f-46ea-8cdd-b9f08b9bd1fb))
  (fp_rect (start -5 1.6) (end -4.6 4)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 5129161c-6212-4f15-8d2c-c8e39b733cf3))
  (fp_rect (start -0.8 10.7) (end 3.1 14.4)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp dd8956fe-0518-4e58-b40c-bee6af74b4d8))
  (fp_rect (start -0.2 1.6) (end 0.2 4)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 9e44b14b-2508-4f94-9f7c-dde4d4b6ff3a))
  (fp_rect (start 4.6 1.6) (end 5 4)
    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp b16e7f77-f292-4dc0-aafd-890c5461a4f9))
  (fp_rect (start 6.4 14.5) (end -6.4 -1.4)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.CrtYd") (tstamp fe3e08ed-f1d1-4441-8bc4-b6c90840e0c5))
  (fp_line (start -4.8 1.6) (end -4.8 4.1)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 8237efa5-7b6b-46bd-9651-6b33b8cf74f0))
  (fp_line (start -0.85 14.45) (end -0.85 10.6)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 0c8b3af4-f74c-4422-ac07-4907fe7839b5))
  (fp_line (start 0 4.15) (end 0 1.6)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp f1ba4607-d5e7-45bc-a7bd-2129d506fc79))
  (fp_line (start 3.05 10.6) (end 3.05 14.45)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 6ba47fe4-3310-4a75-9dea-db568ceb0221))
  (fp_line (start 3.05 14.45) (end -0.85 14.45)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 493e3605-91bd-453d-b8c5-bc78abfd5dd0))
  (fp_line (start 4.8 4.1) (end 4.8 1.6)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 0a35a573-b477-46a6-a942-a7723e08008c))
  (fp_rect (start -6.35 4.15) (end 6.35 10.55)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp 5a0425ee-18cb-43cd-b7ec-f6576d4e5089))
  (pad "1" thru_hole oval (at -4.8 0) (size 2.2 2.8) (drill oval 1.2 1.8) (layers "*.Cu" "*.Mask") (tstamp 73fa4242-df59-4719-ae5e-bdf9f1c717d1))
  (pad "2" thru_hole oval (at 0 0) (size 2.2 2.8) (drill oval 1.2 1.8) (layers "*.Cu" "*.Mask") (tstamp 65126f89-a644-4b7e-a14a-6e8c0aabc841))
  (pad "3" thru_hole oval (at 4.8 0) (size 2.2 2.8) (drill oval 1.2 1.8) (layers "*.Cu" "*.Mask") (tstamp 25a6620e-9d91-4ef0-824e-fd524f3f9283))
  (model "${my_additions}/SS12D06.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
