(footprint "Crystal_generator_7050" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Crystal 7x5mm SMD")
  (tags "crystal, generator, 7050, 7x5")
  (attr smd)
  (fp_text reference "REF**" (at -4.4 3.5 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 7d125767-2285-40b7-a665-dcf3b0bd0b03)
  )
  (fp_text value "Xtal_7050" (at 0 3.3) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 205311bb-28f9-468d-85b2-dccf181c7d6a)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4e2261a6-56de-48fb-b334-0426026886f3)
  )
  (fp_line (start -3.6 3.3) (end -3.6 -2.6)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 4fca7ad7-1735-462a-84ac-a2bd2db71e30))
  (fp_line (start -1.4 -2.6) (end 1.4 -2.6)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 23c09d2f-795a-43ba-b096-b070b0ea3977))
  (fp_line (start 1.4 2.6) (end -1.4 2.6)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp c5a69c65-020b-4170-94c4-d3f0b78812bf))
  (fp_line (start 3.6 -2.6) (end 3.6 2.6)
    (stroke (width 0.15) (type default)) (layer "F.SilkS") (tstamp 61a86f82-c046-4f5d-9cc7-3229f22ea616))
  (fp_circle (center -3.1 3.7) (end -2.9 3.7)
    (stroke (width 0.15) (type solid)) (fill solid) (layer "F.SilkS") (tstamp a13b1d73-6ffe-47e6-89ff-ab3fc98d8acd))
  (fp_rect (start -3.5 -2.5) (end 3.5 2.5)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 8adbf762-d8cf-49a1-bb29-a106c1ca5783))
  (fp_rect (start -3.4 -2.4) (end 3.4 2.4)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp bc80d9af-92a7-4cfa-a210-c1a4fcd87cf2))
  (fp_circle (center -2.6 1.7) (end -2.2 1.7)
    (stroke (width 0.1) (type solid)) (fill solid) (layer "F.Fab") (tstamp d276eee3-b02a-4d57-99b0-83952f40c7f7))
  (pad "1" smd rect (at -2.54 2.2) (size 1.8 2) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp c94a05d9-4398-4ffa-b030-9df66722fbd7))
  (pad "2" smd rect (at 2.54 2.2) (size 1.8 2) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 894b7322-2228-43c3-9fae-e4f35711c87d))
  (pad "3" smd rect (at 2.54 -2.2) (size 1.8 2) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 026aa20a-1929-4978-afbe-95ee9757d718))
  (pad "4" smd rect (at -2.54 -2.2) (size 1.8 2) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 74f5b811-6a7e-4052-bb70-1c684957abb6))
  (model "${my_additions}/crystal_7050.stp"
    (offset (xyz -3.5 -2.5 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
