(footprint "Fuse_1812_HandSolder_plus_THT" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Fuse SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
  (tags "fuse handsolder plus trhough-hole pads")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 08e3cc40-a961-4547-8b96-57a6010139e2)
  )
  (fp_text value "Fuse_1812_HandSolder_plus_THT" (at 0 2.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 8a71d230-fd0c-44f1-bc06-9a46f771681a)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 31a043f3-95df-4daf-aeab-2f9597299aa5)
  )
  (fp_line (start -1.386252 -1.71) (end 1.386252 -1.71)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a0c9ffab-3db3-4171-ab74-2e36537ccba1))
  (fp_line (start -1.386252 1.71) (end 1.386252 1.71)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3d9794af-c6ad-42a9-a0e6-6f38ac8fc454))
  (fp_line (start -3.12 -1.95) (end 3.12 -1.95)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ca61d57d-1c61-45f2-8838-37f60da9368e))
  (fp_line (start -3.12 1.95) (end -3.12 -1.95)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 297d40c6-5c20-42b3-88aa-914505b94f58))
  (fp_line (start 3.12 -1.95) (end 3.12 1.95)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c9a56dd4-514e-4a99-b86b-b64fe1eb5ac3))
  (fp_line (start 3.12 1.95) (end -3.12 1.95)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 95e99304-6285-483a-9d75-019528fa0978))
  (fp_line (start -2.25 -1.6) (end 2.25 -1.6)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f725f17c-d744-4538-8bf8-ddb75e124a1e))
  (fp_line (start -2.25 1.6) (end -2.25 -1.6)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dab29ee6-2cb5-4d81-b74a-11beb3bd3a09))
  (fp_line (start 2.25 -1.6) (end 2.25 1.6)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 90870a81-1bd0-4eb5-b3d8-0884615f8eca))
  (fp_line (start 2.25 1.6) (end -2.25 1.6)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e94e39de-c0da-4d30-b7eb-c8e1aeef5dfe))
  (pad "1" thru_hole circle (at -2.5 -0.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 9d31eeae-50da-4067-898c-81219ed43aca))
  (pad "1" smd roundrect (at -2.225 0) (size 1.3 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308) (tstamp 83a0d48f-ba11-4401-8828-0e7504307ded))
  (pad "2" smd roundrect (at 2.225 0) (size 1.3 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308) (tstamp 387f3196-a575-4511-83e7-110ec20cfe69))
  (pad "2" thru_hole circle (at 2.5 0.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 418b421b-af68-4956-952b-064855fc54a1))
  (model "${my_additions}/MF-R110.STEP"
    (offset (xyz 0 0.7 10.1))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 -7))
  )
  (model "${my_additions}/fuse_smd1812.stp"
    (offset (xyz 0 0 1.05))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
