(footprint "USB_Micro-B_Vertical" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "USB Micro-B receptacle, through-hole, vertical,")
  (tags "usb micro receptacle vertical")
  (attr through_hole)
  (fp_text reference "REF**" (at 1.3 -2.48) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c6aff463-1363-48b4-b491-2a56b962fcb6)
  )
  (fp_text value "USB_Micro-B_Vertical" (at 1.3 2.92) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 248be61f-2fb7-4ca1-95e0-6330332e00b2)
  )
  (fp_text user "${REFERENCE}" (at 1.3 0.22) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 26318f28-2115-4360-a983-bf4cf7c644da)
  )
  (fp_line (start -2.85 -1.38) (end 5.45 -1.38)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp ad65b1c5-de24-4776-b316-9c1683005c96))
  (fp_line (start -2.85 -0.905) (end -2.85 -1.38)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 9b4c5cd3-40df-4df2-9d94-2cecde43f3c3))
  (fp_line (start -2.85 1.345) (end -2.85 1.82)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp a32196ef-2ccc-4b7d-b113-0f3497b11066))
  (fp_line (start -2.85 1.82) (end 5.45 1.82)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp e3bfe556-1451-4579-8605-2a9375eb913e))
  (fp_line (start -1 -1.68) (end 1 -1.68)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 317f3c24-19a5-4197-8d8d-ae6577a41849))
  (fp_line (start 5.45 -1.38) (end 5.45 -0.905)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 1750c308-b8b8-416f-9c4c-778e590d3db4))
  (fp_line (start 5.45 1.82) (end 5.45 1.345)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp af086fd3-2b7c-49f5-bbe7-f7af734245f8))
  (fp_line (start -3.2 -1.73) (end -3.2 2.17)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ae3ae96a-2368-4626-9355-aa7fbd95821d))
  (fp_line (start -3.2 2.17) (end 5.8 2.17)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cf653026-43dd-4e81-8325-9def1d71b262))
  (fp_line (start 5.8 -1.73) (end -3.2 -1.73)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a9f3369c-bc0f-4c9c-ae40-8c6331f33180))
  (fp_line (start 5.8 2.17) (end 5.8 -1.73)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f24ca52a-a124-4eee-b518-f9bbf35b4b55))
  (fp_line (start -2.7 -1.23) (end -1 -1.23)
    (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp ff00f0f2-28f2-4c94-8f8a-969dfad604f7))
  (fp_line (start -2.7 1.67) (end -2.7 -1.23)
    (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 41b6563c-7a6c-4821-93ea-ad07b2c850d8))
  (fp_line (start -1 -1.23) (end 0 -0.23)
    (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp abba648a-57bf-4331-8895-87417039bb5a))
  (fp_line (start 0 -0.23) (end 1 -1.23)
    (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 48cc58f9-b051-411b-aa71-169d76701ad3))
  (fp_line (start 1 -1.23) (end 5.3 -1.23)
    (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 54602339-d83a-4fdc-8059-75d5000ad76e))
  (fp_line (start 5.3 -1.23) (end 5.3 1.67)
    (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 148d5cc4-b156-433f-9f4e-753b4a7297d4))
  (fp_line (start 5.3 1.67) (end -2.7 1.67)
    (stroke (width 0.15) (type solid)) (layer "F.Fab") (tstamp 246198e1-6c06-44a7-b391-60f16bc7dbaf))
  (pad "1" thru_hole rect (at 0 0) (size 0.84 0.84) (drill 0.44) (layers "*.Cu" "*.Mask") (tstamp 5da9cb99-16b4-47e4-bf0f-c34b302dae9c))
  (pad "2" thru_hole circle (at 0.65 1) (size 0.84 0.84) (drill 0.44) (layers "*.Cu" "*.Mask") (tstamp ef3bee2d-391b-42b2-9695-d2cbc6a51b8c))
  (pad "3" thru_hole circle (at 1.3 0) (size 0.84 0.84) (drill 0.44) (layers "*.Cu" "*.Mask") (tstamp bb97af1d-6c99-4ea5-b93e-30901724bec1))
  (pad "4" thru_hole circle (at 1.95 1) (size 0.84 0.84) (drill 0.44) (layers "*.Cu" "*.Mask") (tstamp 9b9b7fab-fa4e-4192-bba5-5e24651edf32))
  (pad "5" thru_hole circle (at 2.6 0) (size 0.84 0.84) (drill 0.44) (layers "*.Cu" "*.Mask") (tstamp 6e78b9c0-5911-4aa0-8d80-66dfc35f36ce))
  (pad "6" thru_hole oval (at -2.275 0.22) (size 0.85 1.85) (drill oval 0.35 1.35) (layers "*.Cu" "*.Mask") (tstamp 34030271-8d72-4896-876c-0c8a93c170e2))
  (pad "6" thru_hole oval (at 4.875 0.22) (size 0.85 1.85) (drill oval 0.35 1.35) (layers "*.Cu" "*.Mask") (tstamp 83ba3d31-a300-4e0c-af39-a79ed7723551))
  (model "${my_additions}/micro_usb_vetical.STEP"
    (offset (xyz 1.3 -1.75 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
