(footprint "Converter_ACDC_HiLink_HLK-5Mxx" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -12.4 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp cc54046a-e276-49ce-9c0d-6281ee5f5ed2)
  )
  (fp_text value "Converter_ACDC_HiLink_HLK-5Mxx" (at 0.2 12.9 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp adfa2677-2f8c-49c4-bb7e-bbadf42aa403)
  )
  (fp_text user "AC" (at -14.3 -3 unlocked) (layer "B.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    (tstamp 0ee5f4d2-1113-4d52-a6f3-488a915be517)
  )
  (fp_text user "+Vo" (at 13.9 9 unlocked) (layer "B.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    (tstamp 5f29b4bc-23b3-46c5-9b24-a3649b362458)
  )
  (fp_text user "-Vo" (at 13.9 -9.1 unlocked) (layer "B.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    (tstamp d30c793a-8a6a-4343-9864-23bfbde48789)
  )
  (fp_text user "AC" (at -14.2 3 unlocked) (layer "B.SilkS")
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    (tstamp d8477791-f838-48b5-839e-9a01b91d4312)
  )
  (fp_text user "-Vo" (at 13.8 -9.1 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 338b3114-b5c1-45a1-a5ac-a1653fcd6f6b)
  )
  (fp_text user "AC" (at -14.3 -3 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 81389511-e8b6-427d-b320-3062329654cf)
  )
  (fp_text user "+Vo" (at 13.7 9 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 86292e1f-c996-46a1-b2df-828102123376)
  )
  (fp_text user "AC" (at -14.2 3 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bc711eb5-3a82-4845-b887-0631c848377e)
  )
  (fp_rect (start -19 -11.5) (end 19 11.5) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 5db7906c-1cf8-4452-858c-edc3ace0ade3))
  (fp_rect (start -19.5 -12) (end 19.5 12) (layer "F.CrtYd") (width 0.12) (fill none) (tstamp abf30c98-8038-48e9-b2d6-e6ffc3e0e47c))
  (pad "1" thru_hole circle (at -16.8 -3) (size 2.3 2.3) (drill 1) (layers *.Cu *.Mask) (tstamp 3515e32e-05e9-4076-9aaf-a0e68065df2f))
  (pad "2" thru_hole circle (at -16.8 3) (size 2.3 2.3) (drill 1) (layers *.Cu *.Mask) (tstamp 160d70d6-c707-43a5-9375-79cd06f69cd6))
  (pad "3" thru_hole circle (at 16.8 -9) (size 2.3 2.3) (drill 1) (layers *.Cu *.Mask) (tstamp 9345fb43-2016-4cbf-bda1-444c5a79b1d1))
  (pad "4" thru_hole circle (at 16.8 9) (size 2.3 2.3) (drill 1) (layers *.Cu *.Mask) (tstamp 0ad47eee-7b5f-44de-b4a4-637a3be4d9bc))
  (model "${my_additions}/Hi-Link_HLK_5W.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
