(footprint "Crystal_Seiko_MC-146_4P-L6.7-W1.5-P0.85-BL" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (tags "crystal, oscillator")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -1.5) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9e3c05c0-d1c5-41fd-b88b-6d8d9e6b4acb)
  )
  (fp_text value "Crystal_Seiko_MC-146_4P-L6.7-W1.5-P0.85-BL" (at 0 2.4) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6d066847-ce2f-4727-95af-1df41b493a90)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4d8abf43-1894-4c66-aeec-94601248b072)
  )
  (fp_line (start -2.45 -0.75) (end 2.45 -0.75)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e66782e1-515c-440d-852e-405a8a3c9b3b))
  (fp_line (start -2.45 0.75) (end 2.45 0.75)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e994d502-3b16-4070-b8cd-b93f2d798be8))
  (fp_poly
    (pts
      (xy -2.4 1.5)
      (xy -3 1.5)
      (xy -2.7 1.1)
    )

    (stroke (width 0.1) (type solid)) (fill solid) (layer "F.SilkS") (tstamp f9e36e40-c0a8-490d-bccb-47b9c586f652))
  (fp_rect (start -3.4 -0.8) (end 3.4 0.8)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp d1907d76-d7ca-427c-b771-242883ceca68))
  (fp_rect (start -2.5 -0.7) (end 2.5 0.7)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp df6e844b-7433-4572-b2e5-00d1e78cac4a))
  (pad "1" smd rect (at -3.4 0.45) (size 1.7 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 0078d957-4a45-4974-b31b-fae2206d348a))
  (pad "2" smd rect (at 3.4 0.45) (size 1.7 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 968d6375-3442-473b-9641-c79ca0705a95))
  (pad "3" smd rect (at 3.4 -0.45) (size 1.7 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp eba99aad-7b0c-4d4f-b893-5ecf807ed678))
  (pad "4" smd rect (at -3.4 -0.45) (size 1.7 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp da03ad79-d7f3-4b8d-9c6e-4b14f14b8291))
  (model "$(my_additions)/Crystal_Seiko_MC-146_4P-L6.7-W1.5-P0.85-BL.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
