(footprint "Buzzer_5020" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (descr "Buzzer 5x5x2mm 2-4v")
  (tags "buzzer 5020")
  (attr smd)
  (fp_text reference "REF**" (at -0.1 -3.5 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a264eadd-10cf-4ff0-8658-27d2364ef3ec)
  )
  (fp_text value "Buzzer_5020" (at 0 3.7 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1e5852f6-08e4-43b0-83c0-67f11c9e1c71)
  )
  (fp_line (start 2.6 -1.6) (end 2.6 0.9) (layer "F.SilkS") (width 0.12) (tstamp 2fcd4eef-5c1a-4ec5-b854-d6b8e3a15ab6))
  (fp_line (start -2.6 -2.6) (end 1.6 -2.6) (layer "F.SilkS") (width 0.12) (tstamp 39a13777-4699-46ab-a3ad-3c1947f2d605))
  (fp_line (start -2.6 0.9) (end -2.6 -0.9) (layer "F.SilkS") (width 0.12) (tstamp 70d3c1dc-12cb-42e1-af57-d552eb2d1c88))
  (fp_line (start -2.6 2.6) (end 2.6 2.6) (layer "F.SilkS") (width 0.12) (tstamp 8378d8d5-2e37-4fcd-8854-49d23a24ddd2))
  (fp_line (start 1.6 -2.6) (end 2.6 -1.6) (layer "F.SilkS") (width 0.12) (tstamp b12e9fd9-c568-4d72-b0ab-aeaca64fd758))
  (fp_circle (center 0 -1.15) (end 0.4 -1.15) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 453fb9b1-c76f-4075-80b9-c943970c51d0))
  (fp_rect (start -2.8 -2.8) (end 2.8 2.8) (layer "F.CrtYd") (width 0.12) (fill none) (tstamp 88524f99-ea7c-4275-94c3-0aa0e559ecb1))
  (pad "" smd rect (at -2.25 -1.75) (size 2.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 56009e6e-6109-476d-8d4a-25f09ba71bf5))
  (pad "1" smd rect (at -2.25 1.75) (size 2.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp 8da527fe-a8dd-46f1-ae83-f28e51920d2d))
  (pad "2" smd rect (at 2.25 1.75) (size 2.5 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (tstamp ca67c3ac-5c9e-4dcb-8d5d-cf43f80506a2))
  (model "${my_additions}/Buzzer_5020.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
