(footprint "Fuse_1808_0451_Holder_HandSolder"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Fuse SMD 1808 https://aliexpress.ru/item/10000001106516.html?sku_id=12000024121607749&spm=a2g2w.productlist.search_results.17.7f124aa6lKLWXf")
	(tags "fuse handsolder")
	(property "Reference" "REF**"
		(at 0.2 -3.5 0)
		(layer "F.SilkS")
		(uuid "08e3cc40-a961-4547-8b96-57a6010139e2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Fuse_1808_0451_Holder_HandSolder"
		(at 0.1 3.6 0)
		(layer "F.Fab")
		(uuid "8a71d230-fd0c-44f1-bc06-9a46f771681a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "68deee24-c476-4fcf-9e53-f97ccb8af18e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "f9afb0f7-2e1d-44cf-b67e-8b73432ea62c")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -5 -2.5)
		(end -5 -2.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "92ed25c5-f60e-41c4-bab9-154553222289")
	)
	(fp_line
		(start -5 -2.5)
		(end 5 -2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a0c9ffab-3db3-4171-ab74-2e36537ccba1")
	)
	(fp_line
		(start -5 2.5)
		(end -5 2.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3674c9a8-6aee-4969-870b-4ca385424e32")
	)
	(fp_line
		(start -5 2.5)
		(end 5 2.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3d9794af-c6ad-42a9-a0e6-6f38ac8fc454")
	)
	(fp_line
		(start 5 -2.5)
		(end 5 -2.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "95477d2e-dc30-4f92-9020-ae21e7752032")
	)
	(fp_line
		(start 5 2.5)
		(end 5 2.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "73d356fe-5aa3-42d9-9072-3c84da46af07")
	)
	(fp_rect
		(start -5.2 -2.6)
		(end 5.2 2.6)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "2ea4ac5b-264a-4a57-aea6-a1f01b36cacc")
	)
	(fp_line
		(start -2.25 1.6)
		(end -2.25 -1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "dab29ee6-2cb5-4d81-b74a-11beb3bd3a09")
	)
	(fp_line
		(start 2.25 -1.6)
		(end 2.25 1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "90870a81-1bd0-4eb5-b3d8-0884615f8eca")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "31a043f3-95df-4daf-aeab-2f9597299aa5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -3.61 0)
		(size 5.08 3.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.08)
		(uuid "83a0d48f-ba11-4401-8828-0e7504307ded")
	)
	(pad "2" smd roundrect
		(at 3.61 0)
		(size 5.08 3.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.08)
		(uuid "387f3196-a575-4511-83e7-110ec20cfe69")
	)
	(embedded_fonts no)
	(model "${MY_ADDITIONS}/SMD-fuse-holder-for-1808-fuse_with_fuse.step"
		(offset
			(xyz 0 0 0.2)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
