(footprint "nRF24L01+_GT-24_mini_Breakout"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -8.4 0.2 90)
		(layer "F.SilkS")
		(uuid "295750fe-1677-4a9b-8148-d4848e8fcd97")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify left)
		)
	)
	(property "Value" "NRF24L01+_GT-24_mini_Breakout"
		(at 0 5.7 180)
		(layer "F.Fab")
		(uuid "7d9cf9eb-962e-4154-9a59-5ec509d7ecbd")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0bd88a86-b15e-4707-8f6a-5de01528a3a3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "66979720-854b-4db7-af69-844ab04e9561")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -7.5 -10.9)
		(end -7.5 0.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3ad37e76-5e2d-4b7e-839b-1923eda221ca")
	)
	(fp_line
		(start -7.5 0.2)
		(end -5.2 0.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "1afc24aa-74a3-4181-83f1-6f34842c98de")
	)
	(fp_line
		(start 0 -7.3)
		(end 0 -2.3)
		(stroke
			(width 0.3)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c03a5060-a0cc-48db-8b02-13ff6c3fee54")
	)
	(fp_line
		(start 5.2 0.2)
		(end 7.5 0.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "6909c533-0b79-4057-a0e0-de6adabc0b28")
	)
	(fp_line
		(start 7.5 0.2)
		(end 7.5 -8.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "5e2754b0-60d9-494e-9450-1c1531a8e2e0")
	)
	(fp_arc
		(start -1.1 -10.1)
		(mid 2.08177 -9.471689)
		(end 2.843986 -6.319315)
		(stroke
			(width 0.3)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "77a439f5-28ac-4a67-a9fa-fc43abaf7c72")
	)
	(fp_arc
		(start -0.5 -9.6)
		(mid 1.650406 -8.978142)
		(end 2.308012 -6.838398)
		(stroke
			(width 0.3)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "758ef867-74db-4bc0-a4b5-aa2afb415a8f")
	)
	(fp_arc
		(start 0 -9)
		(mid 1.202082 -8.502082)
		(end 1.7 -7.3)
		(stroke
			(width 0.3)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "7e9d8961-d690-4a4e-9412-365eac521120")
	)
	(fp_circle
		(center 0 -7.3)
		(end 1 -7.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "ccaeb7f2-04fd-4ec6-aad6-438a3ae97bbf")
	)
	(fp_poly
		(pts
			(xy -5.1 -0.4) (xy -5.6 -0.7) (xy -5.6 -0.1)
		)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "12ac1760-aa3f-4c4b-af05-1685c88a882e")
	)
	(fp_rect
		(start -7.25 -18.3)
		(end 7.25 0)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "26683dea-c235-440e-aea0-3737388a85e6")
	)
	(fp_text user "ANT"
		(at 5.7 -14.6 90)
		(unlocked yes)
		(layer "Cmts.User")
		(uuid "710a3991-1bd3-4cc1-96b5-e68f31ae24d3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify left bottom)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0.1 3.7 180)
		(layer "F.Fab")
		(uuid "d9bea502-d8f9-4792-a1f8-42f8630a3983")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at -7.4 -12.4)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1)
		(uuid "224e4376-a6cd-41e3-aeb7-1d9a4393be03")
	)
	(pad "1" smd rect
		(at 4.445 0)
		(size 0.8 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.1)
		(thermal_bridge_angle 45)
		(uuid "f3c794c2-886e-4392-9b46-9c61dbaf0950")
	)
	(pad "1" thru_hole circle
		(at 7.4 -10.15)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1)
		(uuid "dd34bad1-7d85-42e7-b60d-d30b0b905eca")
	)
	(pad "2" smd rect
		(at -4.445 0)
		(size 0.8 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.1)
		(thermal_bridge_angle 45)
		(uuid "442c2930-a8c5-4b93-8f62-8bb270132480")
	)
	(pad "3" smd rect
		(at -3.175 0)
		(size 0.8 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.1)
		(thermal_bridge_angle 45)
		(uuid "73e0d87a-ce8d-413f-8180-b145bbd70bc5")
	)
	(pad "4" smd rect
		(at -1.905 0)
		(size 0.8 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.1)
		(thermal_bridge_angle 45)
		(uuid "9a0193b6-6989-49e1-a85e-3d7eef764f4d")
	)
	(pad "5" smd rect
		(at -0.635 0)
		(size 0.8 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.1)
		(thermal_bridge_angle 45)
		(uuid "d3b3231c-11fc-40a4-aa6b-19e716a119de")
	)
	(pad "6" smd rect
		(at 0.635 0)
		(size 0.8 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.1)
		(thermal_bridge_angle 45)
		(uuid "b1949f51-e398-482f-9cac-427eddbf8c00")
	)
	(pad "7" smd rect
		(at 1.905 0)
		(size 0.8 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.1)
		(thermal_bridge_angle 45)
		(uuid "8d9ef88e-d147-4188-ac2a-3e2ee3ace03d")
	)
	(pad "8" smd rect
		(at 3.175 0)
		(size 0.8 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.1)
		(thermal_bridge_angle 45)
		(uuid "e10257df-85a1-498d-b37f-153e63011240")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(uuid "4cb551ee-56fd-4824-b7c8-d78d0ff40b49")
		(name "No ground")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 3.5 -17.9) (xy 3.5 -13.8) (xy 6.6 -13.8) (xy 6.6 -17.9)
			)
		)
	)
	(embedded_fonts no)
	(model "${MY_ADDITIONS}/NRF24L01+_GT-24-mini.step"
		(offset
			(xyz 0 0 1.2)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
