(footprint "RQM0029A-MFG"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "VQFN-HR 29-pin")
	(tags "BQ25672RQMR, VQFN-HR, 29-VQFN")
	(property "Reference" "REF**"
		(at 0 -3.2 0)
		(layer "F.SilkS")
		(uuid "e16d066a-b15a-43eb-9e73-e4f514506ba8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "BQ25672RQMR "
		(at 0 2.9 0)
		(layer "F.Fab")
		(uuid "fd8861fa-6432-4f38-be82-9b6855ccdd23")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "49724e87-b137-41b7-b9fa-77d1de5a3d8a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "21dd7272-40b8-4920-80c0-83a861a558db")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.3 -2.3)
		(end -2.049998 -2.3)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "029d846b-88c6-4ea1-a663-722bd1ed3b2d")
	)
	(fp_line
		(start -2.3 -2.049998)
		(end -2.3 -2.3)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "906bb298-de6b-402f-84fe-abc6dc2a5643")
	)
	(fp_line
		(start -2.3 2.3)
		(end -2.3 2.049998)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2ea2e796-7dbd-4b96-ae46-fd6ed962d24a")
	)
	(fp_line
		(start -2.3 2.3)
		(end -2.049998 2.3)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "16b519c3-afbb-495d-a479-7c316a16b368")
	)
	(fp_line
		(start 2.049998 -2.3)
		(end 2.3 -2.3)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "45e30de9-71fb-42cf-bbd6-43a562484202")
	)
	(fp_line
		(start 2.049998 2.3)
		(end 2.3 2.3)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7d77eeaf-7256-499f-85cf-608e7c6be6f9")
	)
	(fp_line
		(start 2.3 -2.049998)
		(end 2.3 -2.3)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "66d59a48-75c2-45dc-9299-94c668f293b3")
	)
	(fp_line
		(start 2.3 2.3)
		(end 2.3 2.049998)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ad21d4d0-f6ce-4369-b474-112310b529c8")
	)
	(fp_circle
		(center -2.75 -1.599999)
		(end -2.624999 -1.599999)
		(stroke
			(width 0.25)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "c5ccab00-41b2-466e-ba2d-68fe3f250bcd")
	)
	(fp_rect
		(start -2.4 -2.4)
		(end 2.4 2.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "36b031c2-adf7-4120-b716-ac61a2b72a1c")
	)
	(fp_line
		(start -2.049998 -2.049998)
		(end 2.049998 -2.049998)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3dd27924-c95d-443b-b305-b1b3e932fba5")
	)
	(fp_line
		(start -2.049998 2.050001)
		(end -2.049998 -2.049998)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "011d1816-2b82-4644-b0b5-fd70171e0283")
	)
	(fp_line
		(start -2.049998 2.050001)
		(end 2.049998 2.050001)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "10caa625-3c01-4d96-9cda-038a36c968b3")
	)
	(fp_line
		(start 2.049998 2.050001)
		(end 2.049998 -2.049998)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "14217598-6bb0-4d19-af80-09db6aca6903")
	)
	(fp_circle
		(center -1.6 -1.625001)
		(end -1.474999 -1.625001)
		(stroke
			(width 0.25)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "2f260f58-7a26-43b1-9d21-81cc03e4e372")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -2.8 0)
		(layer "F.Fab")
		(uuid "7b98e7e3-9dc7-4d6d-a8e2-ad2bfbef7f6c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -1.725 -1.6)
		(size 0.95 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "87083074-b1df-4ce2-8398-7f31f0f6af91")
	)
	(pad "1" smd roundrect
		(at -1.35 -1.85)
		(size 0.2 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "7e18e75a-8a3a-45c3-b65a-b0ec9e3256c2")
	)
	(pad "2" smd roundrect
		(at -1.9 -1.2)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "ca017dc1-69d2-4026-af76-9269150991ef")
	)
	(pad "3" smd roundrect
		(at -1.9 -0.8)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "2a5bbbe6-58d3-4677-abcc-e80bd6cbc7ff")
	)
	(pad "4" smd roundrect
		(at -1.9 -0.4)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "89af3f25-1981-4588-bdff-a777a60321c8")
	)
	(pad "5" smd roundrect
		(at -1.9 0)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "f2f56a26-8492-4a63-8b59-07e1a0688bfe")
	)
	(pad "6" smd roundrect
		(at -1.9 0.4)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "e3d6c73b-494b-4f8b-bc30-454d8b308429")
	)
	(pad "7" smd roundrect
		(at -1.9 0.8)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "b158804a-d0c2-4ffc-9193-f4d25c76023d")
	)
	(pad "8" smd roundrect
		(at -1.9 1.2)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "9533482d-b957-45da-9f93-a5f7b669055d")
	)
	(pad "9" smd roundrect
		(at -1.75 1.6)
		(size 0.9 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "b65823f4-b039-42b9-a8ed-fd92aec90fce")
	)
	(pad "9" smd roundrect
		(at -1.4 1.85)
		(size 0.2 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "4c7f75e4-6fb5-4e89-a820-f1a2261e4f65")
	)
	(pad "10" smd roundrect
		(at -1 1.9 90)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "0b7af1d7-d07e-4db5-a8bb-98855d1a5286")
	)
	(pad "11" smd roundrect
		(at -0.6 1.9 90)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "e7de82a1-8592-426c-a4f9-822f3cd73e3b")
	)
	(pad "12" smd roundrect
		(at -0.2 1.9 90)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "1b5dc4c1-1118-4b44-86af-05d744f46d26")
	)
	(pad "13" smd roundrect
		(at 0.2 1.9 90)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "9147e659-8440-4198-b69f-90ab22389fb5")
	)
	(pad "14" smd roundrect
		(at 0.6 1.9 90)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "1eabb2e4-7b0b-4485-8e29-1f384d32b9ad")
	)
	(pad "15" smd roundrect
		(at 1 1.9 90)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "42c3bf3c-8864-49c8-b8c0-28e8ab018398")
	)
	(pad "16" smd roundrect
		(at 1.4 1.85)
		(size 0.2 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "fa9b07c7-9522-49b7-8bae-bd3c594a30a2")
	)
	(pad "16" smd roundrect
		(at 1.75 1.6)
		(size 0.9 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "009396aa-6553-4d11-9e5e-3da4a133b809")
	)
	(pad "17" smd roundrect
		(at 1.85 1.2)
		(size 0.7 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "9036f7e6-7148-4562-b4e6-37123329e34c")
	)
	(pad "18" smd roundrect
		(at 1.875 0.8)
		(size 0.65 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "bdd23a4f-aa38-4957-87f7-dba4616af85d")
	)
	(pad "19" smd roundrect
		(at 1.8625 0.4)
		(size 0.68 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "f43b341f-0a03-4a88-88a7-94fde2c7b760")
	)
	(pad "20" smd roundrect
		(at 1.9 0)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "c2414840-72f7-41ca-ae4d-44701a390256")
	)
	(pad "21" smd roundrect
		(at 1.9 -0.4)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "8ce059a4-c2fb-48d5-8bd4-c21e967510f9")
	)
	(pad "22" smd roundrect
		(at 1.9 -0.8)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "2a85971a-b93e-4739-9681-fc66e5b8387a")
	)
	(pad "23" smd roundrect
		(at 1.9 -1.2)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "ce0616b9-2319-42bf-a49b-1e5d3c31afbe")
	)
	(pad "24" smd roundrect
		(at 1.35 -1.85)
		(size 0.2 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "4e6dd002-5f06-4518-8ac2-e04abd3e9ee4")
	)
	(pad "24" smd roundrect
		(at 1.725 -1.6)
		(size 0.95 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "48319372-ad0d-49b5-a99c-8a3f90c370c1")
	)
	(pad "25" smd roundrect
		(at 0.9 -1.7)
		(size 0.2 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "fed93ada-3307-47af-bd23-692497968d7c")
	)
	(pad "26" smd roundrect
		(at 0.45 -1.7)
		(size 0.2 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "9800631f-41ff-47d9-94f6-6e1c20004104")
	)
	(pad "27" smd roundrect
		(at 0 -1.7)
		(size 0.2 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "ec220193-65db-4cdb-a48e-90f168f66a46")
	)
	(pad "28" smd roundrect
		(at -0.45 -1.7)
		(size 0.2 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "68b6edf8-45be-47ec-9d74-789e903ede4d")
	)
	(pad "29" smd roundrect
		(at -0.9 -1.725)
		(size 0.2 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
		(uuid "36e3684f-62b7-4604-afc5-5e2401924fce")
	)
	(embedded_fonts no)
	(model "${MY_ADDITIONS}/RQM0029A.stp"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
