(footprint "ESP-01_proper"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Wi-Fi Module, https://docs.ai-thinker.com/_media/esp8266/esp8266_series_modules_user_manual_en.pdf")
	(tags "Wi-Fi Module")
	(property "Reference" "REF**"
		(at 3.8 -10.2 0)
		(layer "F.SilkS")
		(uuid "d8effc85-5684-4466-8535-a99f82591335")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "ESP-01_proper"
		(at 3.7 -19 0)
		(layer "F.Fab")
		(uuid "6ffd1dab-5bab-4aa1-96a9-4ab576ada2b3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "757c17aa-3ded-4ed5-876f-63f43c1be221")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "1c658b4b-0150-4ed8-8493-ad84e7cfc671")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_rect
		(start -3.61 -20.77)
		(end 11.01 4.15)
		(stroke
			(width 0.12)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "a0af32bf-69e2-41bf-9381-c72df5627f57")
	)
	(fp_rect
		(start -1.3 -1.3)
		(end 9.02 3.84)
		(stroke
			(width 0.12)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "623187d2-2f8c-4776-abac-c60cd51a932c")
	)
	(fp_poly
		(pts
			(xy -0.480921 -2.449755) (xy 0.519079 -2.449755) (xy 0.019079 -1.449755)
		)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "aebc66f5-f481-466d-a00d-f3acd30f2fe2")
	)
	(fp_rect
		(start -3.75 -20.91)
		(end 11.15 4.29)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "327597de-7052-49e0-8c10-8573a6444a80")
	)
	(fp_line
		(start -3.5 -0.96)
		(end -3.5 0.87)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "5d4fe3d7-3be4-4b37-94b3-d71cd05d55fe")
	)
	(fp_line
		(start -1.56 0.03)
		(end -3.5 -0.96)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "3a343de0-3a81-4549-b63d-00a0550be98f")
	)
	(fp_line
		(start -1.56 0.03)
		(end -3.5 0.87)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "b46dae9f-3633-4c93-b23e-62d2fbf93b7a")
	)
	(fp_rect
		(start -3.5 -20.66)
		(end 10.9 4.04)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "cb5e3626-80eb-4434-9838-786c086abb42")
	)
	(fp_text user "${REFERENCE}"
		(at 3.7 -11.8 0)
		(layer "F.Fab")
		(uuid "a2c9e3fb-eee8-454a-a997-836484989193")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1470588235)
		(uuid "5852532e-84b3-44b9-bc38-11e16151ee3f")
	)
	(pad "2" thru_hole circle
		(at 0 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "909402fa-089b-4f6b-8cbc-915b46d40474")
	)
	(pad "3" thru_hole circle
		(at 2.54 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f8ba2933-fe7f-48fb-8bc1-4f6fd6f8eb1d")
	)
	(pad "4" thru_hole circle
		(at 2.54 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5cb99055-8d4a-4873-beb3-42ba3680623c")
	)
	(pad "5" thru_hole circle
		(at 5.08 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "fdfff63f-7cd4-4078-afd6-2f667fef81f1")
	)
	(pad "6" thru_hole circle
		(at 5.08 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e76ed5b2-0159-44ba-8701-e97082e5805d")
	)
	(pad "7" thru_hole circle
		(at 7.62 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "bf6c95f2-5042-4005-bf68-9098e207f1ed")
	)
	(pad "8" thru_hole circle
		(at 7.62 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1e9cae4a-3d4d-48c7-bdaa-7fd14a701858")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(uuid "9e0b8615-afdf-416b-90a8-5814408a416e")
		(name "No Copper")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -3.475 -20.625) (xy 10.85 -20.6) (xy 10.825 -13.975) (xy -3.5 -14)
			)
		)
	)
	(embedded_fonts no)
	(model "${MY_ADDITIONS}/ESP-01S_PBD-8.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
