(footprint "FPC_Connector_1.0K-GL-18PBF" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 7.8 -2) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)) (justify left))
    (tstamp 94301549-96c0-4953-874f-e924b7bb031f)
  )
  (fp_text value "1.0K-GL-18PBF" (at 0 2) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 5bd7eed4-5629-4464-9a20-412e3f8de3f9)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a355961f-05ce-412f-997b-e9436e0bedac)
  )
  (fp_line (start -12.5 -1.2) (end -12.5 1.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 2ce92740-7761-49b8-8dfb-cf596e4a98d6))
  (fp_line (start -12.5 1.2) (end -8 1.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp e8718297-b91b-47b0-8c77-9f45e9642a9e))
  (fp_line (start -9 -1.2) (end -12.5 -1.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp be9addb2-3258-4cb4-8683-1aed22bbf97c))
  (fp_line (start -5 -1.2) (end -6 -1.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp d296f0f9-11fb-4dd7-acf2-135e1d31fec7))
  (fp_line (start -4 1.2) (end -5 1.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 5335e3e2-7c76-4f4a-9c95-3fad3e6fcac7))
  (fp_line (start -3 -1.2) (end -4 -1.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp b195730b-86f2-44ce-bbcc-7e49fc144945))
  (fp_line (start -2 1.2) (end -3 1.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp c9be2ba9-e913-4791-8c55-3cab7c33aef2))
  (fp_line (start -1 -1.2) (end -2 -1.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 03dc3498-af0d-473f-88df-492c97644838))
  (fp_line (start 0 1.2) (end -1 1.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 18ad2ed4-6036-4ca5-bedc-53ef1df48d88))
  (fp_line (start 1 -1.2) (end 0 -1.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp d559695f-958d-4982-8a46-2c9ee02a4f55))
  (fp_line (start 2 1.2) (end 1 1.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 46dc7382-01bd-4ebb-97b2-c250aa7fafb8))
  (fp_line (start 3 -1.2) (end 2 -1.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 93622fb1-b269-4a9d-bf2b-10860488099f))
  (fp_line (start 4 1.2) (end 3 1.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 026745a2-d418-4556-b8b9-f1191c45b9e4))
  (fp_line (start 5 -1.2) (end 4 -1.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp b271bffa-8095-439c-96dd-cbcc87aa11af))
  (fp_line (start 6 1.2) (end 5 1.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 62159c31-c306-4944-b1a4-4c9d1b923a3c))
  (fp_line (start 9 1.2) (end 12.5 1.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp eacdf569-7e1f-43b8-be8e-04023bf0c300))
  (fp_line (start 12.5 -1.2) (end 8 -1.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 0bc03b1c-acc0-4437-b220-7b582fcdce3f))
  (fp_line (start 12.5 1.2) (end 12.5 -1.2)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 11f7226e-426b-4db9-98c1-18ebb95b3716))
  (fp_poly
    (pts
      (xy -8.5 -2.6)
      (xy -8.7 -2.9)
      (xy -8.3 -2.9)
    )

    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 5ece8139-0abe-46d4-85da-a7f248789841))
  (fp_rect (start -12.55 -1.25) (end 12.55 1.25)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.CrtYd") (tstamp 3409e40f-dd02-4f34-b009-f09b647ea471))
  (fp_rect (start -12.4 -1.1) (end 12.4 1.1)
    (stroke (width 0.1) (type default)) (fill none) (layer "F.Fab") (tstamp fc31a47e-764d-467d-9808-fa42e4a1eefe))
  (pad "1" smd rect (at -8.5 -1.65) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 6db15002-274a-4051-a682-e288baecba32))
  (pad "2" smd rect (at -7.5 1.65) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 212036a9-22b7-40d1-bca1-3c7bc095716f))
  (pad "3" smd rect (at -6.5 -1.65) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 9bffe55a-23ed-4958-9466-c72c83d8242d))
  (pad "4" smd rect (at -5.5 1.65) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 567b8386-c4c6-4035-9381-f462de2c1329))
  (pad "5" smd rect (at -4.5 -1.651) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 2063d699-50b9-4831-9d99-96ddea69cc2f))
  (pad "6" smd rect (at -3.5 1.65) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp af0395e1-df12-44d1-99db-2fccb8065dd8))
  (pad "7" smd rect (at -2.5 -1.65) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 3fb7035f-df62-4b12-bb4c-4a6c174219f8))
  (pad "8" smd rect (at -1.5 1.65) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 08bb4d37-05f6-4329-9ee6-e31eaab7244b))
  (pad "9" smd rect (at -0.5 -1.65) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 2d14ec7d-51be-484a-8052-88fdb4a52b90))
  (pad "10" smd rect (at 0.5 1.65) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 5c730916-539a-484b-ab6c-7f7c0bc99a62))
  (pad "11" smd rect (at 1.5 -1.65) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 0297cd77-5b0e-4d77-abbf-ee51f9e1885b))
  (pad "12" smd rect (at 2.5 1.65) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp a3fcab23-7c3f-48c1-bd24-23fdf7abb156))
  (pad "13" smd rect (at 3.5 -1.65) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 14fa147f-9a4e-4904-9436-688c9d416ee7))
  (pad "14" smd rect (at 4.5 1.65) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 975ea3c6-7d69-4f50-93f3-0a8caa4805e5))
  (pad "15" smd rect (at 5.5 -1.65) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 11257312-e8f6-4d57-a98f-271a0eaea928))
  (pad "16" smd rect (at 6.5 1.65) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp fc23d61f-811a-4f49-8116-2aa43aa95a84))
  (pad "17" smd rect (at 7.5 -1.65) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp e90ae1a0-f1d6-4cb7-9954-21c8e25cfdc7))
  (pad "18" smd rect (at 8.5 1.65) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp c5e9ed57-ef88-47ca-b6c2-fb408303a87e))
  (pad "MP" smd rect (at -10.9 0) (size 2 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 58630dcc-7943-4de8-bc1c-969424be373d))
  (pad "MP" smd rect (at 10.9 0) (size 2 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp fd45901f-a0f0-4c13-ba47-24d19b1cfb6a))
)
