(footprint "NRF24L01_SMD_Breakout"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -3.175 -1.905 90)
		(layer "F.SilkS")
		(uuid "a7785c7d-17e6-4bd8-8b22-3a4f028535d4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "NRF24L01_SMD_Breakout"
		(at 4.445 -19.05 0)
		(layer "F.Fab")
		(uuid "de0ba54f-2cdf-4fb0-a32e-edee07fba029")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at -18.415 32.425 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4c6ba108-b1cd-4ac2-8723-040166c8de3d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at -18.415 32.425 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "cb47fd5a-7f6e-4461-b489-625b96544a00")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.905 0)
		(end -1.905 -10.795)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "742356ca-c2f0-428f-b810-fc12fdba68e3")
	)
	(fp_line
		(start -0.835 0)
		(end -1.905 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3478fc46-cfe7-4f9a-9be5-03f7fbda2ca9")
	)
	(fp_line
		(start 9.725 0)
		(end 10.795 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "88ea4b79-5fc4-4181-a28d-dab0b9271df9")
	)
	(fp_line
		(start 10.795 0)
		(end 10.795 -10.795)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "943bf883-21ad-47de-baac-c26df2e04b9e")
	)
	(fp_rect
		(start -1.6 -18)
		(end 10.4 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "2d545c18-a573-4636-9c27-11f712afb152")
	)
	(fp_line
		(start -1.6 -11.5)
		(end 10.4 -11.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "66103c1e-be0f-4690-a562-0bb76b54bfc9")
	)
	(fp_line
		(start -0.635 -17.145)
		(end 0.635 -17.145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "aa1073cb-11bf-40ce-84b5-f8624e966208")
	)
	(fp_line
		(start -0.635 -12.065)
		(end -0.635 -17.145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "d6587424-16a3-493f-9c36-04d141b387fb")
	)
	(fp_line
		(start 0.635 -17.145)
		(end 0.635 -13.97)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "26734136-1ed2-49f7-a0e7-1940ae00c813")
	)
	(fp_line
		(start 0.635 -13.97)
		(end 1.905 -13.97)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "0d05a942-bde5-4e20-ae34-dbda26f6113b")
	)
	(fp_line
		(start 1.905 -17.145)
		(end 3.175 -17.145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "a3ab2aea-c583-422a-8b28-88478ef3153e")
	)
	(fp_line
		(start 1.905 -13.97)
		(end 1.905 -17.145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "65ef5dd3-c7df-4b94-9692-b3c97c1fc47c")
	)
	(fp_line
		(start 3.175 -17.145)
		(end 3.175 -13.97)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "2f5e6f65-7ee2-416b-ae93-70c13e1157cc")
	)
	(fp_line
		(start 3.175 -13.97)
		(end 4.445 -13.97)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "ac9de6d9-ce01-400c-8437-be854a147476")
	)
	(fp_line
		(start 4.445 -17.145)
		(end 5.715 -17.145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "6404f2ec-816a-443a-b428-9c28ec07eace")
	)
	(fp_line
		(start 4.445 -13.97)
		(end 4.445 -17.145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "3a4c1034-1638-4b51-821b-690de0601433")
	)
	(fp_line
		(start 5.715 -17.145)
		(end 5.715 -13.97)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "5bcbb33a-0d31-4254-b874-50af284b460b")
	)
	(fp_line
		(start 5.715 -13.97)
		(end 6.985 -13.97)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "5117aa2c-8f2b-4c08-ae14-34b76c598128")
	)
	(fp_line
		(start 6.985 -17.145)
		(end 9.525 -17.145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "5e599660-1f21-4691-836c-b20753584425")
	)
	(fp_line
		(start 6.985 -13.97)
		(end 6.985 -17.145)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "3230a3ef-1a1a-4316-81fb-8a08523cb993")
	)
	(fp_rect
		(start -1.6 -18)
		(end 10.4 0)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "d6ebbbcb-8a9f-4d45-b3a1-600bc3c96b0c")
	)
	(fp_text user "${REFERENCE}"
		(at 4.445 -6.35 0)
		(layer "F.Fab")
		(uuid "0afcc648-f871-411e-89ed-b654b23f1807")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at 1.27 -0.4)
		(size 0.9 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "e6f22f37-4636-42f5-bf6a-ac327fcc79e3")
	)
	(pad "2" smd rect
		(at 0 -0.4)
		(size 0.9 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "77fb9082-7be6-4ce4-b0be-f2c67528dd28")
	)
	(pad "3" smd rect
		(at 2.54 -0.4)
		(size 0.9 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "693269f7-9d4c-41e7-af1c-5ad4ac18f670")
	)
	(pad "4" smd rect
		(at 3.81 -0.4)
		(size 0.9 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "a028292b-8d82-4149-9597-2deafbb27bf8")
	)
	(pad "5" smd rect
		(at 5.08 -0.4)
		(size 0.9 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "20c43249-bf3e-4309-8342-10c3389b5764")
	)
	(pad "6" smd rect
		(at 6.35 -0.4)
		(size 0.9 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "ab4a0c60-d66e-4d8f-9b96-f91a6662b3b0")
	)
	(pad "7" smd rect
		(at 7.62 -0.4)
		(size 0.9 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "265cd175-0f5d-4f26-9a7c-7bc4233776e8")
	)
	(pad "8" smd rect
		(at 8.89 -0.4)
		(size 0.9 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "f61beebc-386b-4aad-800f-7cb7fdbaae3c")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(uuid "0d37ea73-c5bb-4ad7-adda-78fadfc227aa")
		(name "Antenna_keepout")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -1.9 -11.5) (xy -1.9 -18.3) (xy 10.7 -18.3) (xy 10.7 -11.5)
			)
		)
	)
	(embedded_fonts no)
	(model "${MY_ADDITIONS}/nRF24L01_SMD.stp"
		(offset
			(xyz 4.4 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
