(footprint "Magnetic_pogo_4pin_2..54mm_male"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "4-pin magnetic Male Pogo connector")
	(tags "pogo, connector, 4pin")
	(property "Reference" "REF**"
		(at 0 -2.8 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "dfba582d-3a61-45e7-86af-f7f4ae3cea36")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Magnetic_pogo_4pin_2..54mm_male"
		(at 0 3 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "81f27e0c-95b8-4e43-a828-fbebef40600e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://aliexpress.ru/item/1005006125313623.html?sku_id=12000035866966080"
		(at 0 1.9 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "98c6129d-ce44-4aea-8e3d-801173a8c0d9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "4-pin magnetic Male Pogo connector"
		(at 0 1.9 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8526fe8b-e2bc-427d-af4a-0391c3caccee")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -9.63 -2)
		(end 9.63 -2)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "15d614e5-6d98-4e86-84da-df61e9957bc5")
	)
	(fp_line
		(start 9.63 2)
		(end -9.63 2)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "b1aa3681-3ea2-4127-9471-82c5c47281c1")
	)
	(fp_arc
		(start -9.63 2)
		(mid -11.63 0)
		(end -9.63 -2)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "cfd6b630-137a-41b8-ae00-086cef0a7f77")
	)
	(fp_arc
		(start -6.77 2)
		(mid -8.77 0)
		(end -6.77 -2)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "95fd7609-217c-4b6d-91f7-ff480aec40bb")
	)
	(fp_arc
		(start 6.77 -2)
		(mid 8.77 0)
		(end 6.77 2)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e9cc978e-7fd3-455b-8c3f-a93d8d5e3195")
	)
	(fp_arc
		(start 9.63 -2)
		(mid 11.63 0)
		(end 9.63 2)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a3bd1c75-bd41-4b03-806c-b57d58042ab2")
	)
	(fp_circle
		(center -10.22 0)
		(end -9.47 0)
		(stroke
			(width 0.15)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "37f69e32-5e87-410a-a02b-bb14f51ea7eb")
	)
	(fp_circle
		(center 10.22 0)
		(end 10.97 0)
		(stroke
			(width 0.15)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "be9a1dff-45e7-4cf3-ac61-46ba70f34a4e")
	)
	(fp_line
		(start -9.62 -2)
		(end 9.62 -2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "65552f79-13d3-4530-8fcc-e0ce67405f04")
	)
	(fp_line
		(start -9.62 2)
		(end 9.62 2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "682d665a-e6ff-4889-b7f5-1fd107a58ba4")
	)
	(fp_arc
		(start -9.62 2)
		(mid -11.62 0)
		(end -9.62 -2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "6c5012c0-5dd8-4097-9529-0fb2dd13a943")
	)
	(fp_arc
		(start 9.62 -2)
		(mid 11.62 0)
		(end 9.62 2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4121f8f7-191d-469b-9e44-81bb8b74bdbc")
	)
	(fp_line
		(start -9.63 -2)
		(end 9.63 -2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "20e72b8f-8cfc-4266-896f-a0f82a037e74")
	)
	(fp_line
		(start 9.63 2)
		(end -9.63 2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "0b28af1d-d563-451b-8401-acb14df8cad7")
	)
	(fp_arc
		(start -9.63 2)
		(mid -11.63 0)
		(end -9.63 -2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "5ab7ed75-ef4f-4104-ad4d-834f15ba4485")
	)
	(fp_arc
		(start -6.77 2)
		(mid -8.77 0)
		(end -6.77 -2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "eb08a9ce-3dd8-438a-acf6-c03d85dc5234")
	)
	(fp_arc
		(start 6.77 -2)
		(mid 8.77 0)
		(end 6.77 2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "52e8025f-47e4-44ea-9f82-813e211aff8b")
	)
	(fp_arc
		(start 9.63 -2)
		(mid 11.63 0)
		(end 9.63 2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "69d5c6dc-05ab-4cb6-bcd1-0921de2670bf")
	)
	(fp_circle
		(center -10.22 0)
		(end -9.47 0)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "631cecb7-b0b8-43c8-b2fd-0788fb6db62b")
	)
	(fp_circle
		(center 10.22 0)
		(end 10.97 0)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "3195e6c9-6e53-45fd-853a-730d06439d5c")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -2.8 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "410d61d7-50b5-4d38-8d79-d6e5a1f0509f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole roundrect
		(at -3.81 0)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1388888889)
		(uuid "189ace4b-de28-4fe5-9e3b-5e091a3582dc")
	)
	(pad "2" thru_hole circle
		(at -1.27 0)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "347e514e-d7da-402a-bf20-2a3daa9075ce")
	)
	(pad "3" thru_hole circle
		(at 1.27 0)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e10e4ac6-13b2-42ab-9403-37666cd356ce")
	)
	(pad "4" thru_hole circle
		(at 3.81 0)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2c16323e-8660-4e73-98f6-275e59b0dc7f")
	)
	(embedded_fonts no)
	(model "${MY_ADDITIONS}/MagneticPogoMale-4pin.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
