(footprint "SW_DPDT_x2_slider_MSS22D18"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "slider DPDT switch")
	(tags "slider switch dpdt")
	(property "Reference" "REF**"
		(at 0 -5.6 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "27502ab1-9b6e-416b-855f-8152592d8ea9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "MSS22D18"
		(at 0 5.6 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "e5b6b488-ecb9-46f6-a303-a3c046e92500")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2eb208ea-8ae3-4921-91ed-401146561e4c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "90a66bf5-c60a-47e3-b837-6216b28bdfba")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -1.9 -4.7)
		(end 1.9 4.7)
		(stroke
			(width 0.12)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "9fe6b252-3619-491f-ab60-c4291cd09223")
	)
	(fp_poly
		(pts
			(xy -3.1 -3.3) (xy -2.7 -3.7) (xy -3.5 -3.7)
		)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "55556ee2-64b6-4a3b-b42f-a8112ad2036f")
	)
	(fp_rect
		(start -3 -4.7)
		(end 3 4.7)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "480742f3-ab99-4179-957f-d9ec82471c71")
	)
	(fp_rect
		(start -1.75 -4.55)
		(end 1.75 4.55)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "3beb48c3-289c-4fdb-9d98-f4ce0ce487a9")
	)
	(fp_rect
		(start -0.9 -1.9)
		(end 0.9 -0.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill yes)
		(layer "F.Fab")
		(uuid "c73aeb8c-a669-4f9c-adf1-d0389b309172")
	)
	(fp_rect
		(start -0.9 -1.9)
		(end 0.9 1.9)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "14d99314-8289-448a-8cc8-ef2e2908c0f0")
	)
	(fp_text user "${REFERENCE}"
		(at 0 7.1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "acb56299-6e30-404b-891a-38c13be61f1b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -3.1 -2.5)
		(size 1.7 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
		(uuid "e3945b45-7f09-4f1b-bcbf-02fd5695e775")
	)
	(pad "2" smd roundrect
		(at -3.1 0)
		(size 1.7 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
		(uuid "f684d915-5419-4b80-91b8-8b38c1c5f4f5")
	)
	(pad "3" smd roundrect
		(at -3.1 2.5)
		(size 1.7 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
		(uuid "7e96d7b3-1b01-4b25-9a72-142da5604988")
	)
	(pad "4" smd roundrect
		(at 3.1 2.5)
		(size 1.7 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
		(uuid "248ac1b8-d9e8-42d2-94bc-265c806bac47")
	)
	(pad "5" smd roundrect
		(at 3.1 0)
		(size 1.7 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
		(uuid "9f7d36b6-5d9b-4862-acac-a23b6a153dca")
	)
	(pad "6" smd roundrect
		(at 3.1 -2.5)
		(size 1.7 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(thermal_bridge_angle 45)
		(uuid "c5e775bb-f5e9-45f5-9c57-3fe7b3db7723")
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "SW_Slide_MSS22D18.step")
			(type model)
			(data |KLUv/aAnCgkArGECCu3veCjw1BSWA6hst/vQFPhU6GS/TwpL/4HBlKSUSaZk4mk+GZCB54OTSAkB
[encoded data, 87966 characters]
				wvxm3rH8DOG3HGU=|
			)
			(checksum "7CB567A37B662C151C848DB8723EA529")
		)
	)
	(model "kicad-embed://SW_Slide_MSS22D18.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
