(footprint "Tactile_switch_3x4x2mm-2Pad"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Small SMD tactile 3x4mm button")
	(tags "SMD tactile button switch")
	(property "Reference" "REF**"
		(at 0 -2.3 0)
		(layer "F.SilkS")
		(uuid "ea6afd9d-fa23-4bcf-ad60-5d1004f7b106")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Tactile_switch_3x4x2mm-2Pad"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "5d2ee62d-0c4f-4b67-8f42-681a4f1abb2b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "3aac38a2-352d-4226-849a-f2972fe996db")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "8d672443-e70c-4793-8b45-bdb714ea75df")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.1 -1.6)
		(end -2.1 -0.9)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "583aadcb-f79c-45b1-88d1-b99a79adb212")
	)
	(fp_line
		(start -2.1 0.9)
		(end -2.1 1.6)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "43b41bdb-a30e-4b96-a499-e8e9b34d843c")
	)
	(fp_line
		(start -2.1 1.6)
		(end 2.1 1.6)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "075de177-491f-4264-884f-7ece8e6648fa")
	)
	(fp_line
		(start 2.1 -1.6)
		(end -2.1 -1.6)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "08fdfb98-f207-4fe4-a77e-6f5054ded8fd")
	)
	(fp_line
		(start 2.1 -0.9)
		(end 2.1 -1.6)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "890ccdfb-148d-41a4-999e-5fef427c60e7")
	)
	(fp_line
		(start 2.1 1.6)
		(end 2.1 0.9)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e874c21b-0c6e-46b8-a60b-973c3cf26343")
	)
	(fp_circle
		(center 0 0)
		(end 0.9 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "594982d3-5e0b-4281-a225-42d009017ba4")
	)
	(fp_rect
		(start -2 -1.5)
		(end 2 1.5)
		(stroke
			(width 0.12)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "fdbf1f44-d652-41be-b47e-51ca2ba35c90")
	)
	(fp_rect
		(start -2.1 -1.6)
		(end 2.1 1.6)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "cbac564b-e804-4631-88da-91830e02710e")
	)
	(fp_circle
		(center 0 0)
		(end 0.9 0)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "9787c24a-ddd8-4137-918d-32e1f2dd4bc3")
	)
	(fp_text user "${REFERENCE}"
		(at 0 4 0)
		(layer "F.Fab")
		(uuid "e1521779-4618-4863-9f8d-1c3f1b943b90")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -2.2 0)
		(size 1.35 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "bb5bbe49-5992-4a91-97a9-b764ed20d545")
	)
	(pad "2" smd rect
		(at 2.2 0)
		(size 1.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "6acf641d-e35d-4c78-a17d-e30876e45fb7")
	)
	(embedded_fonts no)
	(model "${MY_ADDITIONS}/3x4x2mm-2Pad.stp"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
