(footprint "TestPoint_Pad_D0.8mm_no_circle" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "SMD pad as test Point, diameter 0.8mm")
  (tags "test point SMD pad")
  (attr exclude_from_pos_files exclude_from_bom)
  (fp_text reference "REF**" (at 0 -1.448) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ed08342a-eaee-43e9-b96e-1dd00b47763e)
  )
  (fp_text value "TestPoint_Pad_D0.8mm_no_circle" (at 0 1.55) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a41410ba-6764-40d3-8271-3889cd1f68dc)
  )
  (fp_circle (center 0 0) (end 0.381 0)
    (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp f02f025d-d308-4e0d-bc6c-e230724bf915))
  (pad "1" smd circle (at 0 0) (size 0.8 0.8) (layers "F.Cu" "F.Mask") (tstamp bab732e9-e79a-410d-8a2b-e7d9e8d299bb))
)
